FreeSWITCH Verto™ Video Transcoding Demo
FreeSWITCH Verto™ Looking For Devices
FreeSWITCH Verto™ Testing Network Connection

# Testing Network Connection

Verto™ IN CALL
User Controls

Additional Canvas: |  |

FreeSWITCH Verto™ Video Transcoding Demo (*checking*)

Login
Password
Hostname
Websocket URL
Camera:
Share Device:
Microphone:
Speaker:
Use Video Stereo Audio Use STUN
Video Quality: QVGA 320x240 VGA 640x480 QVGA WIDE 320x180 VGA WIDE 640x360 HD 1280x720 HHD 1920x1080
Max Outgoing Bandwidth: 250kb 500kb 1mb 1.5mb 2mb 5mb No Limit Server Default
Max Incoming Bandwidth: 250kb 500kb 1mb 1.5mb 2mb 5mb No Limit Server Default
Use Dedicated Remote Encoder Scale Remote Video To Match Camera

## Video Streaming (USE STEREO HEADPHONES IF POSSIBLE)

## Codec Test and Conference

Name
CID Number
Email
Avatar
Extension

FreeSWITCH VERTO™ WebRTC Demo Directory
Dial | Desc
3d1 | 3D sound demo #1
3d2 | 3D sound demo #2
stereo1 | Stereo sound demo #1
stereo2 | Stereo sound demo #2
stereo3 | Stereo sound demo #3
3500 | Local 48k Stereo Conference
cluecon | ClueCon Hotline
<number> | Call a US/Canda Number
vuc | VoIP Users Conference
888 | FreeSWITCH Community Conference
3300 | Local 48k Conference
5000 | Try the Demo IVR
9664 | Listen to Hold Music
9386 | Funny Prompts
9198 | Tetris (tone generator)

## Logged Out

You have been logged out or disconnected from the server.

## Login Error

Error logging in

## Call On hold

The call is on hold

## Incoming Call

Incoming Call