# SAM3S SMC

## Static Memory Controller (SMC) User Interface

### Registers

Register Mapping
Address | Register | Name | Access | Reset
--- | --- | --- | --- | ---
0x400E0000 | SMC Setup Register (CS_number = 0) | SMC_SETUP0 | read-write | 0x01010101
0x400E0004 | SMC Pulse Register (CS_number = 0) | SMC_PULSE0 | read-write | 0x01010101
0x400E0008 | SMC Cycle Register (CS_number = 0) | SMC_CYCLE0 | read-write | 0x00030003
0x400E000C | SMC Mode Register (CS_number = 0) | SMC_MODE0 | read-write | 0x10000003
0x400E0010 | SMC Setup Register (CS_number = 1) | SMC_SETUP1 | read-write | 0x01010101
0x400E0014 | SMC Pulse Register (CS_number = 1) | SMC_PULSE1 | read-write | 0x01010101
0x400E0018 | SMC Cycle Register (CS_number = 1) | SMC_CYCLE1 | read-write | 0x00030003
0x400E001C | SMC Mode Register (CS_number = 1) | SMC_MODE1 | read-write | 0x10000003
0x400E0020 | SMC Setup Register (CS_number = 2) | SMC_SETUP2 | read-write | 0x01010101
0x400E0024 | SMC Pulse Register (CS_number = 2) | SMC_PULSE2 | read-write | 0x01010101
0x400E0028 | SMC Cycle Register (CS_number = 2) | SMC_CYCLE2 | read-write | 0x00030003
0x400E002C | SMC Mode Register (CS_number = 2) | SMC_MODE2 | read-write | 0x10000003
0x400E0030 | SMC Setup Register (CS_number = 3) | SMC_SETUP3 | read-write | 0x01010101
0x400E0034 | SMC Pulse Register (CS_number = 3) | SMC_PULSE3 | read-write | 0x01010101
0x400E0038 | SMC Cycle Register (CS_number = 3) | SMC_CYCLE3 | read-write | 0x00030003
0x400E003C | SMC Mode Register (CS_number = 3) | SMC_MODE3 | read-write | 0x10000003
0x400E0040 | SMC Setup Register (CS_number = 4) | SMC_SETUP4 | read-write | 0x01010101
0x400E0044 | SMC Pulse Register (CS_number = 4) | SMC_PULSE4 | read-write | 0x01010101
0x400E0048 | SMC Cycle Register (CS_number = 4) | SMC_CYCLE4 | read-write | 0x00030003
0x400E004C | SMC Mode Register (CS_number = 4) | SMC_MODE4 | read-write | 0x10000003
0x400E0080 | SMC OCMS MODE Register | SMC_OCMS | read-write | 0x00000000
0x400E0084 | SMC OCMS KEY1 Register | SMC_KEY1 | write-only | 0x00000000
0x400E0088 | SMC OCMS KEY2 Register | SMC_KEY2 | write-only | 0x00000000
0x400E00E4 | SMC Write Protect Mode Register | SMC_WPMR | read-write | 0x00000000
0x400E00E8 | SMC Write Protect Status Register | SMC_WPSR | read-only | 0x00000000

### Register Fields

#### SMC SMC Setup Register (CS_number = 0)

Name: SMC_SETUP0

Access: read-write

Address: 0x400E0000

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | NCS_RD_SETUP
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | - | NRD_SETUP
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | NCS_WR_SETUP
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | - | NWE_SETUP

- NWE_SETUP: NWE Setup Length

-

- NCS_WR_SETUP: NCS Setup Length in WRITE Access

-

- NRD_SETUP: NRD Setup Length

-

- NCS_RD_SETUP: NCS Setup Length in READ Access

-

#### SMC SMC Pulse Register (CS_number = 0)

Name: SMC_PULSE0

Access: read-write

Address: 0x400E0004

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | NCS_RD_PULSE
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | NRD_PULSE
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | NCS_WR_PULSE
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | NWE_PULSE

- NWE_PULSE: NWE Pulse Length

-

- NCS_WR_PULSE: NCS Pulse Length in WRITE Access

-

- NRD_PULSE: NRD Pulse Length

-

- NCS_RD_PULSE: NCS Pulse Length in READ Access

-

#### SMC SMC Cycle Register (CS_number = 0)

Name: SMC_CYCLE0

Access: read-write

Address: 0x400E0008

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | - | - | - | - | - | NRD_CYCLE
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
NRD_CYCLE
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | - | - | - | - | - | NWE_CYCLE
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
NWE_CYCLE

- NWE_CYCLE: Total Write Cycle Length

-

- NRD_CYCLE: Total Read Cycle Length

-

#### SMC SMC Mode Register (CS_number = 0)

Name: SMC_MODE0

Access: read-write

Address: 0x400E000C

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | PS | - | - | - | PMEN
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | - | - | TDF_MODE | TDF_CYCLES
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | DBW | - | - | - | -
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | - | EXNW_MODE | - | - | WRITE_MODE | READ_MODE

- READ_MODE

  Value | Name | Description
  --- | --- | ---
  0 | - | The read operation is controlled by the NCS signal.
  1 | - | The read operation is controlled by the NRD signal.

- WRITE_MODE

  Value | Name | Description
  --- | --- | ---
  0 | - | The write operation is controlled by the NCS signal.
  1 | - | The write operation is controlled by the NWE signal.

- EXNW_MODE: NWAIT Mode

  Value | Name | Description
  --- | --- | ---
  0x0 | DISABLED | Disabled
  0x2 | FROZEN | Frozen Mode
  0x3 | READY | Ready Mode

- DBW: Data Bus Width

  Value | Name | Description
  --- | --- | ---
  0x0 | 8_BIT | 8-bit bus
  0x1 | 16_BIT | 16-bit bus
  0x2 | 32_BIT | 32-bit bus

- TDF_CYCLES: Data Float Time

-

- TDF_MODE: TDF Optimization

  Value | Name | Description
  --- | --- | ---
  0 | - | TDF optimization is disabled.
  1 | - | TDF optimization is enabled.

- PMEN: Page Mode Enabled

  Value | Name | Description
  --- | --- | ---
  0 | - | Standard read is applied.
  1 | - | Asynchronous burst read in page mode is applied on the corresponding chip select.

- PS: Page Size

  Value | Name | Description
  --- | --- | ---
  0x0 | 4_BYTE | 4-byte page
  0x1 | 8_BYTE | 8-byte page
  0x2 | 16_BYTE | 16-byte page
  0x3 | 32_BYTE | 32-byte page

#### SMC SMC Setup Register (CS_number = 1)

Name: SMC_SETUP1

Access: read-write

Address: 0x400E0010

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | NCS_RD_SETUP
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | - | NRD_SETUP
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | NCS_WR_SETUP
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | - | NWE_SETUP

- NWE_SETUP: NWE Setup Length

-

- NCS_WR_SETUP: NCS Setup Length in WRITE Access

-

- NRD_SETUP: NRD Setup Length

-

- NCS_RD_SETUP: NCS Setup Length in READ Access

-

#### SMC SMC Pulse Register (CS_number = 1)

Name: SMC_PULSE1

Access: read-write

Address: 0x400E0014

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | NCS_RD_PULSE
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | NRD_PULSE
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | NCS_WR_PULSE
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | NWE_PULSE

- NWE_PULSE: NWE Pulse Length

-

- NCS_WR_PULSE: NCS Pulse Length in WRITE Access

-

- NRD_PULSE: NRD Pulse Length

-

- NCS_RD_PULSE: NCS Pulse Length in READ Access

-

#### SMC SMC Cycle Register (CS_number = 1)

Name: SMC_CYCLE1

Access: read-write

Address: 0x400E0018

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | - | - | - | - | - | NRD_CYCLE
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
NRD_CYCLE
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | - | - | - | - | - | NWE_CYCLE
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
NWE_CYCLE

- NWE_CYCLE: Total Write Cycle Length

-

- NRD_CYCLE: Total Read Cycle Length

-

#### SMC SMC Mode Register (CS_number = 1)

Name: SMC_MODE1

Access: read-write

Address: 0x400E001C

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | PS | - | - | - | PMEN
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | - | - | TDF_MODE | TDF_CYCLES
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | DBW | - | - | - | -
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | - | EXNW_MODE | - | - | WRITE_MODE | READ_MODE

- READ_MODE

  Value | Name | Description
  --- | --- | ---
  0 | - | The read operation is controlled by the NCS signal.
  1 | - | The read operation is controlled by the NRD signal.

- WRITE_MODE

  Value | Name | Description
  --- | --- | ---
  0 | - | The write operation is controlled by the NCS signal.
  1 | - | The write operation is controlled by the NWE signal.

- EXNW_MODE: NWAIT Mode

  Value | Name | Description
  --- | --- | ---
  0x0 | DISABLED | Disabled
  0x2 | FROZEN | Frozen Mode
  0x3 | READY | Ready Mode

- DBW: Data Bus Width

  Value | Name | Description
  --- | --- | ---
  0x0 | 8_BIT | 8-bit bus
  0x1 | 16_BIT | 16-bit bus
  0x2 | 32_BIT | 32-bit bus

- TDF_CYCLES: Data Float Time

-

- TDF_MODE: TDF Optimization

  Value | Name | Description
  --- | --- | ---
  0 | - | TDF optimization is disabled.
  1 | - | TDF optimization is enabled.

- PMEN: Page Mode Enabled

  Value | Name | Description
  --- | --- | ---
  0 | - | Standard read is applied.
  1 | - | Asynchronous burst read in page mode is applied on the corresponding chip select.

- PS: Page Size

  Value | Name | Description
  --- | --- | ---
  0x0 | 4_BYTE | 4-byte page
  0x1 | 8_BYTE | 8-byte page
  0x2 | 16_BYTE | 16-byte page
  0x3 | 32_BYTE | 32-byte page

#### SMC SMC Setup Register (CS_number = 2)

Name: SMC_SETUP2

Access: read-write

Address: 0x400E0020

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | NCS_RD_SETUP
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | - | NRD_SETUP
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | NCS_WR_SETUP
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | - | NWE_SETUP

- NWE_SETUP: NWE Setup Length

-

- NCS_WR_SETUP: NCS Setup Length in WRITE Access

-

- NRD_SETUP: NRD Setup Length

-

- NCS_RD_SETUP: NCS Setup Length in READ Access

-

#### SMC SMC Pulse Register (CS_number = 2)

Name: SMC_PULSE2

Access: read-write

Address: 0x400E0024

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | NCS_RD_PULSE
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | NRD_PULSE
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | NCS_WR_PULSE
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | NWE_PULSE

- NWE_PULSE: NWE Pulse Length

-

- NCS_WR_PULSE: NCS Pulse Length in WRITE Access

-

- NRD_PULSE: NRD Pulse Length

-

- NCS_RD_PULSE: NCS Pulse Length in READ Access

-

#### SMC SMC Cycle Register (CS_number = 2)

Name: SMC_CYCLE2

Access: read-write

Address: 0x400E0028

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | - | - | - | - | - | NRD_CYCLE
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
NRD_CYCLE
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | - | - | - | - | - | NWE_CYCLE
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
NWE_CYCLE

- NWE_CYCLE: Total Write Cycle Length

-

- NRD_CYCLE: Total Read Cycle Length

-

#### SMC SMC Mode Register (CS_number = 2)

Name: SMC_MODE2

Access: read-write

Address: 0x400E002C

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | PS | - | - | - | PMEN
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | - | - | TDF_MODE | TDF_CYCLES
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | DBW | - | - | - | -
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | - | EXNW_MODE | - | - | WRITE_MODE | READ_MODE

- READ_MODE

  Value | Name | Description
  --- | --- | ---
  0 | - | The read operation is controlled by the NCS signal.
  1 | - | The read operation is controlled by the NRD signal.

- WRITE_MODE

  Value | Name | Description
  --- | --- | ---
  0 | - | The write operation is controlled by the NCS signal.
  1 | - | The write operation is controlled by the NWE signal.

- EXNW_MODE: NWAIT Mode

  Value | Name | Description
  --- | --- | ---
  0x0 | DISABLED | Disabled
  0x2 | FROZEN | Frozen Mode
  0x3 | READY | Ready Mode

- DBW: Data Bus Width

  Value | Name | Description
  --- | --- | ---
  0x0 | 8_BIT | 8-bit bus
  0x1 | 16_BIT | 16-bit bus
  0x2 | 32_BIT | 32-bit bus

- TDF_CYCLES: Data Float Time

-

- TDF_MODE: TDF Optimization

  Value | Name | Description
  --- | --- | ---
  0 | - | TDF optimization is disabled.
  1 | - | TDF optimization is enabled.

- PMEN: Page Mode Enabled

  Value | Name | Description
  --- | --- | ---
  0 | - | Standard read is applied.
  1 | - | Asynchronous burst read in page mode is applied on the corresponding chip select.

- PS: Page Size

  Value | Name | Description
  --- | --- | ---
  0x0 | 4_BYTE | 4-byte page
  0x1 | 8_BYTE | 8-byte page
  0x2 | 16_BYTE | 16-byte page
  0x3 | 32_BYTE | 32-byte page

#### SMC SMC Setup Register (CS_number = 3)

Name: SMC_SETUP3

Access: read-write

Address: 0x400E0030

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | NCS_RD_SETUP
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | - | NRD_SETUP
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | NCS_WR_SETUP
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | - | NWE_SETUP

- NWE_SETUP: NWE Setup Length

-

- NCS_WR_SETUP: NCS Setup Length in WRITE Access

-

- NRD_SETUP: NRD Setup Length

-

- NCS_RD_SETUP: NCS Setup Length in READ Access

-

#### SMC SMC Pulse Register (CS_number = 3)

Name: SMC_PULSE3

Access: read-write

Address: 0x400E0034

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | NCS_RD_PULSE
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | NRD_PULSE
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | NCS_WR_PULSE
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | NWE_PULSE

- NWE_PULSE: NWE Pulse Length

-

- NCS_WR_PULSE: NCS Pulse Length in WRITE Access

-

- NRD_PULSE: NRD Pulse Length

-

- NCS_RD_PULSE: NCS Pulse Length in READ Access

-

#### SMC SMC Cycle Register (CS_number = 3)

Name: SMC_CYCLE3

Access: read-write

Address: 0x400E0038

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | - | - | - | - | - | NRD_CYCLE
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
NRD_CYCLE
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | - | - | - | - | - | NWE_CYCLE
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
NWE_CYCLE

- NWE_CYCLE: Total Write Cycle Length

-

- NRD_CYCLE: Total Read Cycle Length

-

#### SMC SMC Mode Register (CS_number = 3)

Name: SMC_MODE3

Access: read-write

Address: 0x400E003C

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | PS | - | - | - | PMEN
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | - | - | TDF_MODE | TDF_CYCLES
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | DBW | - | - | - | -
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | - | EXNW_MODE | - | - | WRITE_MODE | READ_MODE

- READ_MODE

  Value | Name | Description
  --- | --- | ---
  0 | - | The read operation is controlled by the NCS signal.
  1 | - | The read operation is controlled by the NRD signal.

- WRITE_MODE

  Value | Name | Description
  --- | --- | ---
  0 | - | The write operation is controlled by the NCS signal.
  1 | - | The write operation is controlled by the NWE signal.

- EXNW_MODE: NWAIT Mode

  Value | Name | Description
  --- | --- | ---
  0x0 | DISABLED | Disabled
  0x2 | FROZEN | Frozen Mode
  0x3 | READY | Ready Mode

- DBW: Data Bus Width

  Value | Name | Description
  --- | --- | ---
  0x0 | 8_BIT | 8-bit bus
  0x1 | 16_BIT | 16-bit bus
  0x2 | 32_BIT | 32-bit bus

- TDF_CYCLES: Data Float Time

-

- TDF_MODE: TDF Optimization

  Value | Name | Description
  --- | --- | ---
  0 | - | TDF optimization is disabled.
  1 | - | TDF optimization is enabled.

- PMEN: Page Mode Enabled

  Value | Name | Description
  --- | --- | ---
  0 | - | Standard read is applied.
  1 | - | Asynchronous burst read in page mode is applied on the corresponding chip select.

- PS: Page Size

  Value | Name | Description
  --- | --- | ---
  0x0 | 4_BYTE | 4-byte page
  0x1 | 8_BYTE | 8-byte page
  0x2 | 16_BYTE | 16-byte page
  0x3 | 32_BYTE | 32-byte page

#### SMC SMC Setup Register (CS_number = 4)

Name: SMC_SETUP4

Access: read-write

Address: 0x400E0040

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | NCS_RD_SETUP
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | - | NRD_SETUP
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | NCS_WR_SETUP
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | - | NWE_SETUP

- NWE_SETUP: NWE Setup Length

-

- NCS_WR_SETUP: NCS Setup Length in WRITE Access

-

- NRD_SETUP: NRD Setup Length

-

- NCS_RD_SETUP: NCS Setup Length in READ Access

-

#### SMC SMC Pulse Register (CS_number = 4)

Name: SMC_PULSE4

Access: read-write

Address: 0x400E0044

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | NCS_RD_PULSE
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | NRD_PULSE
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | NCS_WR_PULSE
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | NWE_PULSE

- NWE_PULSE: NWE Pulse Length

-

- NCS_WR_PULSE: NCS Pulse Length in WRITE Access

-

- NRD_PULSE: NRD Pulse Length

-

- NCS_RD_PULSE: NCS Pulse Length in READ Access

-

#### SMC SMC Cycle Register (CS_number = 4)

Name: SMC_CYCLE4

Access: read-write

Address: 0x400E0048

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | - | - | - | - | - | NRD_CYCLE
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
NRD_CYCLE
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | - | - | - | - | - | NWE_CYCLE
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
NWE_CYCLE

- NWE_CYCLE: Total Write Cycle Length

-

- NRD_CYCLE: Total Read Cycle Length

-

#### SMC SMC Mode Register (CS_number = 4)

Name: SMC_MODE4

Access: read-write

Address: 0x400E004C

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | PS | - | - | - | PMEN
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | - | - | TDF_MODE | TDF_CYCLES
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | DBW | - | - | - | -
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | - | EXNW_MODE | - | - | WRITE_MODE | READ_MODE

- READ_MODE

  Value | Name | Description
  --- | --- | ---
  0 | - | The read operation is controlled by the NCS signal.
  1 | - | The read operation is controlled by the NRD signal.

- WRITE_MODE

  Value | Name | Description
  --- | --- | ---
  0 | - | The write operation is controlled by the NCS signal.
  1 | - | The write operation is controlled by the NWE signal.

- EXNW_MODE: NWAIT Mode

  Value | Name | Description
  --- | --- | ---
  0x0 | DISABLED | Disabled
  0x2 | FROZEN | Frozen Mode
  0x3 | READY | Ready Mode

- DBW: Data Bus Width

  Value | Name | Description
  --- | --- | ---
  0x0 | 8_BIT | 8-bit bus
  0x1 | 16_BIT | 16-bit bus
  0x2 | 32_BIT | 32-bit bus

- TDF_CYCLES: Data Float Time

-

- TDF_MODE: TDF Optimization

  Value | Name | Description
  --- | --- | ---
  0 | - | TDF optimization is disabled.
  1 | - | TDF optimization is enabled.

- PMEN: Page Mode Enabled

  Value | Name | Description
  --- | --- | ---
  0 | - | Standard read is applied.
  1 | - | Asynchronous burst read in page mode is applied on the corresponding chip select.

- PS: Page Size

  Value | Name | Description
  --- | --- | ---
  0x0 | 4_BYTE | 4-byte page
  0x1 | 8_BYTE | 8-byte page
  0x2 | 16_BYTE | 16-byte page
  0x3 | 32_BYTE | 32-byte page

#### SMC SMC OCMS MODE Register

Name: SMC_OCMS

Access: read-write

Address: 0x400E0080

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | - | - | - | - | - | -
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
- | - | - | - | CS3SE | CS2SE | CS1SE | CS0SE
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
- | - | - | - | - | - | - | -
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | - | - | - | - | - | - | SMSE

- SMSE: Static Memory Controller Scrambling Enable

  Value | Name | Description
  --- | --- | ---
  0 | - | Disable Scrambling for SMC access.
  1 | - | Enable Scrambling for SMC access.

- CS0SE: Chip Select (x = 0 to 3) Scrambling Enable

  Value | Name | Description
  --- | --- | ---
  0 | - | Disable Scrambling for CSx.
  1 | - | Enable Scrambling for CSx.

- CS1SE: Chip Select (x = 0 to 3) Scrambling Enable

  Value | Name | Description
  --- | --- | ---
  0 | - | Disable Scrambling for CSx.
  1 | - | Enable Scrambling for CSx.

- CS2SE: Chip Select (x = 0 to 3) Scrambling Enable

  Value | Name | Description
  --- | --- | ---
  0 | - | Disable Scrambling for CSx.
  1 | - | Enable Scrambling for CSx.

- CS3SE: Chip Select (x = 0 to 3) Scrambling Enable

  Value | Name | Description
  --- | --- | ---
  0 | - | Disable Scrambling for CSx.
  1 | - | Enable Scrambling for CSx.

#### SMC SMC OCMS KEY1 Register

Name: SMC_KEY1

Access: write-only

Address: 0x400E0084

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
KEY1
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
KEY1
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
KEY1
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
KEY1

- KEY1: Off Chip Memory Scrambling (OCMS) Key Part 1

-

#### SMC SMC OCMS KEY2 Register

Name: SMC_KEY2

Access: write-only

Address: 0x400E0088

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
KEY2
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
KEY2
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
KEY2
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
KEY2

- KEY2: Off Chip Memory Scrambling (OCMS) Key Part 2

-

#### SMC SMC Write Protect Mode Register

Name: SMC_WPMR

Access: read-write

Address: 0x400E00E4

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
WPKEY
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
WPKEY
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
WPKEY
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | - | - | - | - | - | - | WPEN

- WPEN: Write Protect Enable

  Value | Name | Description
  --- | --- | ---
  0 | - | Disables the Write Protect if WPKEY corresponds to 0x534D43 ("SMC" in ASCII).
  1 | - | Enables the Write Protect if WPKEY corresponds to 0x534D43 ("SMC" in ASCII).

- WPKEY: Write Protect KEY

-

#### SMC SMC Write Protect Status Register

Name: SMC_WPSR

Access: read-only

Address: 0x400E00E8

31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
- | - | - | - | - | - | - | -
23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
WPVSRC
15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
WPVSRC
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
- | - | - | - | - | - | - | WPVS

- WPVS: Write Protect Enable

  Value | Name | Description
  --- | --- | ---
  0 | - | No Write Protect Violation has occurred since the last read of the SMC_WPSR register.
  1 | - | A Write Protect Violation occurred since the last read of the SMC_WPSR register. If this violation is an unauthorized attempt to write a protected register, the associated violation is reported into field WPVSRC.

- WPVSRC: Write Protect Violation Source

-