## Broadcast <a name="Broadcast"></a> {#openvino_docs_ops_movement_Broadcast_3}

**Versioned name**: *Broadcast-3*

**Category**: Data movement

**Short description**: *Broadcast* replicates data on the first input to fit a given shape on the second input.

**Detailed description**:

*Broadcast* takes the first tensor `data` and, following broadcasting rules that are specified by `mode` attribute and the 3rd input `axes_mapping`, builds a new tensor with shape matching the 2nd input tensor `target_shape`. `target_shape` input is a 1D integer tensor that represents required shape of the output.

Attribute `mode` and the 3rd input `axes_mapping` are relevant for cases when rank of the input `data` tensor doesn't match the size of the `target_shape` input. They both define how axes from `data` shape are mapped to the output axes. If `mode` is set to `numpy`, it means that the standard one-directional numpy broadcasting rules are applied. They are similar to rules that applied in all binary element-wise operations in case when `auto_broadcasting` attribute is set to `numpy`, and are similar to rules described at [here](https://docs.scipy.org/doc/numpy/user/basics.broadcasting.html#general-broadcasting-rules), when only one-directional broadcasting is applied: input tensor `data` is broadcasted to `target_shape` but not vice-versa.

In case if `mode` is set to `bidirectional`, then the broadcast rule is similar to `numpy.array(input) * numpy.ones(target_shape)`. Dimensions are right alignment. Two corresponding dimension must have the same value, or one of them is equal to 1. If this attribute value is used, then the 3rd input for the operation shouldn't be provided. The behaviour of such kind of broadcasting is equivalent to ONNX operation [Expand](https://github.com/onnx/onnx/blob/rel-1.7.0/docs/Operators.md#Expand). 

In case if `mode` is set to `explicit`, then 3rd input `axes_mapping` comes to play. It contains a list of axis indices, each index maps an axis from the 1st input tensor `data` to axis in the output. The size of `axis_mapping` should match the rank of input `data` tensor, so all axes from `data` tensor should be mapped to axes of the output.

For example, `axes_mapping = [1]` enables broadcasting of a tensor with shape `[C]` to shape `[N,C,H,W]` by replication of initial tensor along dimensions 0, 2 and 3. Another example is broadcasting of tensor with shape `[H,W]` to shape `[N,H,W,C]` with `axes_mapping = [1, 2]`. Both examples requires `mode` set to `explicit` and providing mentioned `axes_mapping` input, because such operations cannot be expressed with `axes_mapping` set to `numpy`.


**Attributes**:

* *mode*

  * **Description**: specifies rules used for mapping of `input` tensor axes to output shape axes.
  * **Range of values**:
    * *numpy* - numpy broadcasting rules, aligned with ONNX Broadcasting. Description is available in <a href="https://github.com/onnx/onnx/blob/master/docs/Broadcasting.md">ONNX docs</a>.; only one-directional broadcasting is applied from `data` to `target_shape`. If this attribute value is used, then the 3rd input for the operation shouldn't be provided.
    * *explicit* - mapping of the input `data` shape axes to output shape is provided as an explicit 3rd input.
    * *bidirectional* - the broadcast rule is similar to `numpy.array(input) * numpy.ones(target_shape)`. Dimensions are right alignment. Two corresponding dimension must have the same value, or one of them is equal to 1. If this attribute value is used, then the 3rd input for the operation shouldn't be provided.
  * **Type**: string
  * **Default value**: "numpy"
  * **Required**: *no*


**Inputs**:

*   **1**: `data` - source tensor of type *T* and shape that is being broadcasted. Required.

*   **2**: `target_shape` - 1D tensor of type *T_SHAPE* describing output shape. Required.

*   **3**: `axes_mapping` - 1D tensor of type *T_SHAPE* describing a list of axis indices, each index maps an axis from the 1st input tensor `data` to axis in the output. The index values in this tensor should be sorted, that disables on-the-fly transpositions of input `data` tensor while the broadcasting. `axes_mapping` input is needed for `mode` equal to *explicit* only.

**Outputs**:

*   **1**: Output tensor of `data` tensor type with replicated content from the 1st tensor `data` and with shape matched `target_shape`.

**Types**

* *T*: any numeric type.

* *T_SHAPE*: any integer type.

**Example**

```xml
<layer ... type="Broadcast" ...>
    <data mode="numpy"/>
    <input>
        <port id="0">
            <dim>16</dim>
            <dim>1</dim>
            <dim>1</dim>
       </port>
        <port id="1">
            <dim>4</dim>   <!--The tensor contains 4 elements: [1, 16, 50, 50] -->
        </port>
        <!-- the 3rd input shouldn't be provided with mode="numpy" -->
    </input>
    <output>
        <port id="2">
            <dim>1</dim>
            <dim>16</dim>
            <dim>50</dim>
            <dim>50</dim>
        </port>
    </output>
</layer>

<layer ... type="Broadcast" ...>
    <data mode="explicit"/>
    <input>
        <port id="0">
            <dim>16</dim>
       </port>
        <port id="1">
            <dim>4</dim>   <!--The tensor contains 4 elements: [1, 16, 50, 50] -->
        </port>
        <port id="1">
            <dim>1</dim>   <!--The tensor contains 1 elements: [1] -->
        </port>
    </input>
    <output>
        <port id="2">
            <dim>1</dim>
            <dim>16</dim>
            <dim>50</dim>
            <dim>50</dim>
        </port>
    </output>
</layer>

<layer ... type="Broadcast" ...>
    <data mode="explicit"/>
    <input>
        <port id="0">
            <dim>50</dim>
            <dim>50</dim>
       </port>
        <port id="1">
            <dim>4</dim>   <!--The tensor contains 4 elements: [1, 50, 50, 16] -->
        </port>
        <port id="1">
            <dim>2</dim>   <!--The tensor contains 2 elements: [1, 2] -->
        </port>
    </input>
    <output>
        <port id="2">
            <dim>1</dim>
            <dim>50</dim>
            <dim>50</dim>
            <dim>16</dim>
        </port>
    </output>
</layer>

<layer ... type="Broadcast" ...>
    <data mode="bidirectional"/>
    <input>
        <port id="0">
            <dim>16</dim>
            <dim>1</dim>
            <dim>1</dim>
       </port>
        <port id="1">
            <dim>4</dim>   <!--The tensor contains 4 elements: [1, 1, 50, 50] -->
        </port>
        <!-- the 3rd input shouldn't be provided with mode="bidirectional" -->
    </input>
    <output>
        <port id="2">
            <dim>1</dim>
            <dim>16</dim>
            <dim>50</dim>
            <dim>50</dim>
        </port>
    </output>
</layer>
```
