# Firmware settings

## Memory Settings

| Option | Setting |
|:------|:-------|
| Node Interleaving | Disable |

## Processor Settings

| Option | Setting |
|:------|:-------|
| Virtualization | Enable |
| VT-D | Enable |
| SR-IOV | Enable |
| x2APIC | Enable |
| Turbo | Enable |
| Hyper-Threading | Enable |
| Direct Cache Access | Enable |
| Prefetchers (DCU IP, DCU Streamers, MLC Spatial, MLC Streamer) | Enable |
| LLC Prefetch | Disable |

## Power

| Option | Setting |
|:------|:-------|
| Power Profile | Maximum Performance |
| Power Control | Maximum Performance |
| Capping | Disable |
| P-States (Turbo Only) on Intel Grantley/Broadwell | Disable |
| P-States on Intel Skylake/Purley | Enable |
| C-States | Disable |
| C1 Enhanced | Disable |
| Power Recovery | Always On, Random |

## UPI Settings

| Option | Setting |
|:------|:-------|
| XPT Prefetch | Disable |
| Stale AtoS | Disable |
| KTI Prefetch | Enable |
| LLC Dead Line Alloc | Enable |

## TPM

| Option | Setting |
|:------|:-------|
| TPM 2.0 State | Enable |

## Boot

| Option | Setting |
|:------|:-------|
| Boot Mode | UEFI |
| Boot Sequence Retry | Enable |
| Secure Boot State | Enable |
| Secure Boot Policy | Default |

## BMC

| Option | Setting |
|:------|:-------|
| Network | Dedicated |
| IPMI | Administrative access only |
| Users | Administrator account |

## Storage Controller (for Spaces Direct)

| Option | Setting |
|:------|:-------|
| Mode | HBA Mode |

## Misc

| Option | Setting |
|:------|:-------|
| NMI Button (optional) | Enabled |
| Intel TXT | Disabled |