(footprint "SW_TS-1187A-B-A-B" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Part" "1825910-6")
  (property "Sheetfile" "main_board.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Push button switch, generic, two pins")
  (property "ki_keywords" "switch normally-open pushbutton push-button")
  (attr smd)
  (fp_text reference "SW1" (at -4.41 -0.025 -90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d2f71644-d893-4c30-afab-230f7981417b)
  )
  (fp_text value "Reset" (at 6.795 3.565) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3f748ac1-7238-431c-8f5a-ed5508308e02)
  )
  (fp_line (start -2.55 -1.18) (end -2.55 1.18)
    (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp f794cda3-0bb9-42f9-9193-8037f7ec4c6e))
  (fp_line (start 2.25 -2.55) (end -2.25 -2.55)
    (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp ecfba8e8-af71-431f-9802-65f725581ae9))
  (fp_line (start 2.25 2.55) (end -2.25 2.55)
    (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 0b100d11-e983-4ffd-bd4f-510096af312c))
  (fp_line (start 2.55 1.18) (end 2.55 -1.18)
    (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp c53e2f37-2dbb-479c-ad86-c46fe2177629))
  (fp_line (start -3.75 -2.5) (end -3.75 -1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 88aab4b0-664c-4b24-9c6a-f086c1522a71))
  (fp_line (start -3.75 -2.5) (end -2.8 -2.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 06dbf0e3-a495-4576-8d5a-3ddef6722791))
  (fp_line (start -3.75 -1.25) (end -2.8 -1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 05dec6b7-e742-40a8-8289-718cc85ed410))
  (fp_line (start -3.75 1.25) (end -2.8 1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1c8d2df6-cb99-44fe-b45e-c79ab2275c82))
  (fp_line (start -3.75 2.5) (end -3.75 1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7771e6ff-a145-40c5-abcb-39fe1512ea89))
  (fp_line (start -3.75 2.5) (end -2.8 2.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 50ddb0e0-8ba6-4d60-87b3-b372c387010f))
  (fp_line (start -2.8 -2.8) (end -2.8 -2.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7ce8cc73-729f-48ba-8dba-354c811bcada))
  (fp_line (start -2.8 -1.25) (end -2.8 1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 53337a99-62e8-4964-b6ea-4f13ff996e1a))
  (fp_line (start -2.8 2.8) (end -2.8 2.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7eb86b92-d342-4858-8861-6dfefc699ffc))
  (fp_line (start -2.8 2.8) (end 2.8 2.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7b1a649e-86e5-45e4-9076-1f6ce834ba2f))
  (fp_line (start 2.8 -2.8) (end -2.8 -2.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d0ea88dc-14c0-41f4-8a38-9d8326a3954e))
  (fp_line (start 2.8 -2.8) (end 2.8 -2.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6c136a1a-517a-41dc-b695-e1cf319dcae3))
  (fp_line (start 2.8 -1.25) (end 2.8 1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 659f073f-a3af-48d8-b29e-db9c5823b71c))
  (fp_line (start 2.8 2.8) (end 2.8 2.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7e4527ae-5962-4ec9-a448-b39b861b6b1c))
  (fp_line (start 3.75 -2.5) (end 2.8 -2.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0dd99e7a-d526-431e-9e70-c237fa584049))
  (fp_line (start 3.75 -2.5) (end 3.75 -1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c775c3ea-d814-451e-9e1a-dd0dc622679d))
  (fp_line (start 3.75 -1.25) (end 2.8 -1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8cd89b6f-34f9-41d7-847b-826097ec14ad))
  (fp_line (start 3.75 1.25) (end 2.8 1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e9f1ff61-f7b1-4817-94b4-8241c86c7331))
  (fp_line (start 3.75 2.5) (end 2.8 2.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dd1c7ac6-c536-43b9-b513-5142a39f66c9))
  (fp_line (start 3.75 2.5) (end 3.75 1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c30257b1-e4cd-4c97-869d-3c466023c514))
  (fp_line (start -2.55 -2.55) (end -2.55 2.55)
    (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp 792a5af1-569a-4f6a-9d15-b0543d5c16f4))
  (fp_line (start -2.55 2.55) (end 2.55 2.55)
    (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp 0fa098a9-a2fc-4ca5-ab72-f4ff4f06a220))
  (fp_line (start 2.55 -2.55) (end -2.55 -2.55)
    (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp b8e94a51-e235-4770-8c3f-6ce9f4d3b026))
  (fp_line (start 2.55 2.55) (end 2.55 -2.55)
    (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp bc66b2d8-a5d8-4a8d-8ed4-d13108044259))
  (pad "1" smd rect (at -3 -1.875) (size 1 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.102) (tstamp cbbded6e-fd7e-4b60-bb57-4e5732d52539))
  (pad "1" smd rect (at 3 -1.875) (size 1 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.102) (tstamp 43108a30-e6d6-4973-ab48-93a1f2727aa6))
  (pad "2" smd rect (at -3 1.875) (size 1 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.102) (tstamp 8780fedb-75af-4e56-9d37-6a2014f9c69a))
  (pad "2" smd rect (at 3 1.875) (size 1 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.102) (tstamp 4a040c76-b7aa-416a-9a6d-49aa4e8e6885))
)
