(footprint "OSC_X322516MLB4SI" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "JLCPCB P/N" "C9002")
  (property "Sheetfile" "main_board.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Four pin crystal, GND on pins 2 and 4")
  (property "ki_keywords" "quartz ceramic resonator oscillator")
  (attr smd)
  (fp_text reference "Y1" (at -2.302061 -0.04 270) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 066886bd-e6e8-4615-8efd-5e6d0061342d)
  )
  (fp_text value "Crystal_GND24" (at 4.9088 2.6564) (layer "F.Fab")
      (effects (font (size 0.64 0.64) (thickness 0.15)))
    (tstamp d3f5a9be-7ee7-4eee-82bc-a5fbd4c581ac)
  )
  (fp_circle (center -2.05 -1.1) (end -1.95 -1.1)
    (stroke (width 0.2) (type solid)) (fill none) (layer "F.SilkS") (tstamp f7f56400-d56c-45d1-9eca-a1668584563d))
  (fp_line (start -1.7 -2.05) (end 1.7 -2.05)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp baae0646-142d-4210-99d0-c36b32b00e4e))
  (fp_line (start -1.7 2.05) (end -1.7 -2.05)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f6a40d8a-bff6-440f-a872-8f32405f5e65))
  (fp_line (start 1.7 -2.05) (end 1.7 2.05)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 47d4194f-7c7c-4228-9055-a9532dfabb9b))
  (fp_line (start 1.7 2.05) (end -1.7 2.05)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 191b8257-1c23-4d84-937a-51ca5adc63ba))
  (fp_line (start -1.25 -1.6) (end 1.25 -1.6)
    (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp bae2bed9-a523-4a4b-bd4a-6a3d93d1a63f))
  (fp_line (start -1.25 1.6) (end -1.25 -1.6)
    (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp d9437fda-3c3e-4806-b17c-074de8406f38))
  (fp_line (start 1.25 -1.6) (end 1.25 1.6)
    (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp ffed4f4d-7952-40bc-b0a1-51ee41a2769c))
  (fp_line (start 1.25 1.6) (end -1.25 1.6)
    (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp 98eb60cc-ea7f-4dc6-8e9c-253886148825))
  (fp_circle (center -2.05 -1.1) (end -1.95 -1.1)
    (stroke (width 0.2) (type solid)) (fill none) (layer "F.Fab") (tstamp 7dfd8dce-4fc2-45ff-a4f8-28567a171e9f))
  (pad "1" smd rect (at -0.85 -1.1) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 82f725e3-dbb7-462d-ace7-d76b790fd2f5))
  (pad "2" smd rect (at -0.85 1.1) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f97e1702-0a5e-45e8-a353-1bc033638f99))
  (pad "3" smd rect (at 0.85 1.1) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 2bc06300-93f1-4138-873f-2d12d74ba0b2))
  (pad "4" smd rect (at 0.85 -1.1) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8b7bae04-f966-4191-be76-d786bd6ff4ec))
)
