(footprint "GT-TC029B-H025-L1N" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Part" "1825910-6")
  (property "Sheetfile" "main_board.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Push button switch, generic, two pins")
  (property "ki_keywords" "switch normally-open pushbutton push-button")
  (attr smd)
  (fp_text reference "SW2" (at 0.02 0.16 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2d448c87-4a97-49cd-b076-2f189a90b057)
  )
  (fp_text value "Boot" (at 12.4 -0.18) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bf1f2e07-1ad9-4c95-adfe-fda9a9fba05c)
  )
  (fp_line (start -1.05 -3) (end 1.05 -3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b3d6f3f1-e8a6-4c37-9624-cbabf9281043))
  (fp_line (start -1.05 3) (end -1.05 -3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9f01eea4-9f4e-449f-bb1b-a597bd5431a9))
  (fp_line (start 1.05 -3) (end 1.05 3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d0c40f57-5e6f-44cc-906b-7877aab502d7))
  (fp_line (start 1.05 3) (end -1.05 3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5b22b697-c679-4c86-b1db-bf47632742b3))
  (pad "1" smd rect (at 0 2.225) (size 1.6 1.05) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 207e17ea-2df4-42ce-8cd9-4179a48ac000))
  (pad "2" smd rect (at 0 -2.225) (size 1.6 1.05) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp a858cbff-0f64-45c2-a3ae-6f1e54aca076))
  (model "${KIPRJMOD}/Snap EDA/GT-TC029B-H025-L1N v1.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
