(module JST_ZH_S7B-ZR_1x07_P1.50mm_Horizontal (layer F.Cu) (tedit 6050757A)
  (descr "JST ZH series connector, S7B-ZR (http://www.jst-mfg.com/product/pdf/eng/eZH.pdf)")
  (tags "connector JST ZH horizontal")
  (fp_text reference REF** (at 4.5 -3.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value JST_ZH_S7B-ZR_1x07_P1.50mm_Horizontal (at 4.5 6) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 9.8 -1.4) (end 10.5 -1.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.5 -1.4) (end -0.8 -1.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.92 -1.28) (end -0.92 1.52) (layer F.Fab) (width 0.12))
  (fp_line (start -1.38 -1.28) (end -0.92 -1.28) (layer F.Fab) (width 0.12))
  (fp_line (start -1.38 4.48) (end -1.38 -1.28) (layer F.Fab) (width 0.12))
  (fp_line (start 10.38 4.48) (end -1.38 4.48) (layer F.Fab) (width 0.12))
  (fp_line (start 10.38 -1.28) (end 10.38 4.48) (layer F.Fab) (width 0.12))
  (fp_line (start 9.92 -1.28) (end 9.92 1.52) (layer F.Fab) (width 0.12))
  (fp_line (start -0.92 1.52) (end 9.92 1.52) (layer F.Fab) (width 0.12))
  (fp_line (start 9.92 -1.28) (end 10.38 -1.28) (layer F.Fab) (width 0.12))
  (fp_line (start 8.85 4.2) (end 8.85 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.15 2) (end 8.85 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.85 4.2) (end 9.15 4.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.15 4.2) (end 9.15 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.65 4.2) (end 7.65 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.65 2) (end 7.35 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.35 4.2) (end 7.65 4.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.35 4.2) (end 7.35 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.15 2) (end 5.85 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.85 4.2) (end 5.85 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.85 4.2) (end 6.15 4.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.15 4.2) (end 6.15 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.35 4.2) (end 4.65 4.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.35 4.2) (end 4.35 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.65 4.2) (end 4.65 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.65 2) (end 4.35 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.85 4.2) (end 2.85 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.15 4.2) (end 3.15 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.15 2) (end 2.85 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.85 4.2) (end 3.15 4.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.35 4.2) (end 1.65 4.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.65 2) (end 1.35 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.65 4.2) (end 1.65 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.35 4.2) (end 1.35 2) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.15 4.2) (end 0.15 4.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.15 4.2) (end 0.15 2) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.15 4.2) (end -0.15 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.15 2) (end -0.15 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.8 -1.4) (end 9.8 1.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.8 1.4) (end -0.8 -1.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.8 1.4) (end 9.8 1.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.5 4.6) (end 10.5 4.6) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 -1.4) (end 10.5 4.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.5 4.6) (end -1.5 -1.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -2 -2.5) (end -2 5.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11 -2.5) (end -2 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11 5.1) (end 11 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2 5.1) (end 11 5.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.25 1.52) (end 0 1.12) (layer F.Fab) (width 0.12))
  (fp_line (start 0 1.12) (end 0.25 1.52) (layer F.Fab) (width 0.12))
  (fp_text user %R (at 4.5 2.4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 2 thru_hole oval (at 1.5 -0.02) (size 1.17 1.87) (drill 0.75) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 3 -0.02) (size 1.17 1.87) (drill 0.75) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 6 -0.02) (size 1.17 1.87) (drill 0.75) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 4.5 -0.02) (size 1.17 1.87) (drill 0.75) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 7.5 -0.02) (size 1.17 1.87) (drill 0.75) (layers *.Cu *.Mask))
  (pad 1 thru_hole roundrect (at 0 -0.02) (size 1.17 1.87) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.214))
  (pad 7 thru_hole oval (at 9 -0.02) (size 1.17 1.87) (drill 0.75) (layers *.Cu *.Mask))
)
