## smartctl -j -V
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-j",
      "-V"
    ],
    "exit_status": 0
  }
}

## smartctl --scan -j
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "--scan",
      "-j"
    ],
    "exit_status": 0
  },
  "devices": [
    {
      "name": "/dev/sda",
      "info_name": "/dev/sda",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdb",
      "info_name": "/dev/sdb",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdc",
      "info_name": "/dev/sdc",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdd",
      "info_name": "/dev/sdd",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sde",
      "info_name": "/dev/sde",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdf",
      "info_name": "/dev/sdf",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdg",
      "info_name": "/dev/sdg",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdh",
      "info_name": "/dev/sdh",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdi",
      "info_name": "/dev/sdi",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdj",
      "info_name": "/dev/sdj",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdk",
      "info_name": "/dev/sdk",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdl",
      "info_name": "/dev/sdl",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdm",
      "info_name": "/dev/sdm",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_10]",
      "type": "megaraid,10",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_11]",
      "type": "megaraid,11",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_12]",
      "type": "megaraid,12",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_13]",
      "type": "megaraid,13",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_14]",
      "type": "megaraid,14",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_15]",
      "type": "megaraid,15",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_16]",
      "type": "megaraid,16",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_17]",
      "type": "megaraid,17",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_18]",
      "type": "megaraid,18",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_19]",
      "type": "megaraid,19",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/nvme0",
      "info_name": "/dev/nvme0",
      "type": "nvme",
      "protocol": "NVMe"
    },
    {
      "name": "/dev/nvme1",
      "info_name": "/dev/nvme1",
      "type": "nvme",
      "protocol": "NVMe"
    }
  ]
}


## smartctl --scan -d sat -j
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "--scan",
      "-d",
      "sat",
      "-j"
    ],
    "exit_status": 0
  },
  "devices": [
    {
      "name": "/dev/sda",
      "info_name": "/dev/sda",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdb",
      "info_name": "/dev/sdb",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdc",
      "info_name": "/dev/sdc",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdd",
      "info_name": "/dev/sdd",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sde",
      "info_name": "/dev/sde",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdf",
      "info_name": "/dev/sdf",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdg",
      "info_name": "/dev/sdg",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdh",
      "info_name": "/dev/sdh",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdi",
      "info_name": "/dev/sdi",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdj",
      "info_name": "/dev/sdj",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdk",
      "info_name": "/dev/sdk",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdl",
      "info_name": "/dev/sdl",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdm",
      "info_name": "/dev/sdm",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_10]",
      "type": "megaraid,10",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_11]",
      "type": "megaraid,11",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_12]",
      "type": "megaraid,12",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_13]",
      "type": "megaraid,13",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_14]",
      "type": "megaraid,14",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_15]",
      "type": "megaraid,15",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_16]",
      "type": "megaraid,16",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_17]",
      "type": "megaraid,17",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_18]",
      "type": "megaraid,18",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/bus/0",
      "info_name": "/dev/bus/0 [megaraid_disk_19]",
      "type": "megaraid,19",
      "protocol": "SCSI"
    }
  ]
}


## smartctl -a $DEVICE_NAME -j
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sda"
    ],
    "exit_status": 4
  },
  "device": {
    "name": "/dev/sda",
    "info_name": "/dev/sda",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "AVAGO",
  "product": "MR9380-8e",
  "model_name": "AVAGO MR9380-8e",
  "revision": "4.68",
  "scsi_version": "SPC-3",
  "user_capacity": {
    "blocks": 156254601216,
    "bytes": 80002355822592
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "serial_number": "00f32e146d8215e82470c6f20eb00506",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705567880,
    "asctime": "Thu Jan 18 09:51:20 2024 CET"
  },
  "temperature": {
    "current": 0,
    "drive_trip": 0
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdb"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdb",
    "info_name": "/dev/sdb",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZLW2GVJY0000C2231WWJ",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705567880,
    "asctime": "Thu Jan 18 09:51:20 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 30,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 1
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33621.587",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2742.278",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.689",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdc"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdc",
    "info_name": "/dev/sdc",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZLW2GVA10000C2231WUM",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705567881,
    "asctime": "Thu Jan 18 09:51:21 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 32,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 19
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33627.791",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2750.804",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.669",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdd"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdd",
    "info_name": "/dev/sdd",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN102FW0000C2233L0B",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705567882,
    "asctime": "Thu Jan 18 09:51:22 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 31,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 1
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33624.876",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2710.962",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.653",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sde"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sde",
    "info_name": "/dev/sde",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN102Y70000C2235UN6",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705567882,
    "asctime": "Thu Jan 18 09:51:22 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 31,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 5
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33623.456",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2710.877",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.659",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdf"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdf",
    "info_name": "/dev/sdf",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN101R60000C2179K5S",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705567883,
    "asctime": "Thu Jan 18 09:51:23 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 29,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15839,
    "minutes": 59
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33615.532",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2728.557",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.659",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdg"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdg",
    "info_name": "/dev/sdg",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN0X61Y0000C2180BAM",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705567884,
    "asctime": "Thu Jan 18 09:51:24 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 27,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15839,
    "minutes": 50
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33621.646",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2708.366",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.686",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdh"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdh",
    "info_name": "/dev/sdh",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN102T80000C2235Z2H",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705567885,
    "asctime": "Thu Jan 18 09:51:25 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 30,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15839,
    "minutes": 59
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33624.478",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2714.312",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.635",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdi"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdi",
    "info_name": "/dev/sdi",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN102XG0000C2235WTW",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705567885,
    "asctime": "Thu Jan 18 09:51:25 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 31,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 11
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33614.203",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2705.450",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.657",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdj"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdj",
    "info_name": "/dev/sdj",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN0X6040000C2180A21",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705567886,
    "asctime": "Thu Jan 18 09:51:26 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 31,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15839,
    "minutes": 50
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33626.607",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2741.291",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.638",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdk"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdk",
    "info_name": "/dev/sdk",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN102WT0000C2235WUR",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705567887,
    "asctime": "Thu Jan 18 09:51:27 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 30,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 0
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33627.048",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2732.919",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.668",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdl"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdl",
    "info_name": "/dev/sdl",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN102GC0000C2236M68",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705567888,
    "asctime": "Thu Jan 18 09:51:28 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 29,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 2
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33617.767",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2717.217",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.673",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdm"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdm",
    "info_name": "/dev/sdm",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN102W90000C2235WML",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705567889,
    "asctime": "Thu Jan 18 09:51:29 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 27,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 4
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33619.963",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2701.985",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.672",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0"
    ],
    "messages": [
      {
        "string": "/dev/bus/0: Unable to detect device type",
        "severity": "error"
      }
    ],
    "exit_status": 1
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0"
    ],
    "messages": [
      {
        "string": "/dev/bus/0: Unable to detect device type",
        "severity": "error"
      }
    ],
    "exit_status": 1
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0"
    ],
    "messages": [
      {
        "string": "/dev/bus/0: Unable to detect device type",
        "severity": "error"
      }
    ],
    "exit_status": 1
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0"
    ],
    "messages": [
      {
        "string": "/dev/bus/0: Unable to detect device type",
        "severity": "error"
      }
    ],
    "exit_status": 1
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0"
    ],
    "messages": [
      {
        "string": "/dev/bus/0: Unable to detect device type",
        "severity": "error"
      }
    ],
    "exit_status": 1
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0"
    ],
    "messages": [
      {
        "string": "/dev/bus/0: Unable to detect device type",
        "severity": "error"
      }
    ],
    "exit_status": 1
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0"
    ],
    "messages": [
      {
        "string": "/dev/bus/0: Unable to detect device type",
        "severity": "error"
      }
    ],
    "exit_status": 1
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0"
    ],
    "messages": [
      {
        "string": "/dev/bus/0: Unable to detect device type",
        "severity": "error"
      }
    ],
    "exit_status": 1
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0"
    ],
    "messages": [
      {
        "string": "/dev/bus/0: Unable to detect device type",
        "severity": "error"
      }
    ],
    "exit_status": 1
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0"
    ],
    "messages": [
      {
        "string": "/dev/bus/0: Unable to detect device type",
        "severity": "error"
      }
    ],
    "exit_status": 1
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/nvme0"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/nvme0",
    "info_name": "/dev/nvme0",
    "type": "nvme",
    "protocol": "NVMe"
  },
  "model_name": "Micron_2200_MTFDHBA256TCK",
  "serial_number": "19292D86AB6C",
  "firmware_version": "P1MU003",
  "nvme_pci_vendor": {
    "id": 4932,
    "subsystem_id": 4932
  },
  "nvme_ieee_oui_identifier": 41077,
  "nvme_controller_id": 0,
  "nvme_version": {
    "string": "1.2.1",
    "value": 66049
  },
  "nvme_number_of_namespaces": 1,
  "nvme_namespaces": [
    {
      "id": 1,
      "size": {
        "blocks": 500118192,
        "bytes": 256060514304
      },
      "capacity": {
        "blocks": 500118192,
        "bytes": 256060514304
      },
      "utilization": {
        "blocks": 500118192,
        "bytes": 256060514304
      },
      "formatted_lba_size": 512,
      "eui64": {
        "oui": 41077,
        "ext_id": 5058767724
      }
    }
  ],
  "user_capacity": {
    "blocks": 500118192,
    "bytes": 256060514304
  },
  "logical_block_size": 512,
  "local_time": {
    "time_t": 1705567889,
    "asctime": "Thu Jan 18 09:51:29 2024 CET"
  },
  "smart_status": {
    "passed": true,
    "nvme": {
      "value": 0
    }
  },
  "nvme_smart_health_information_log": {
    "critical_warning": 0,
    "temperature": 35,
    "available_spare": 100,
    "available_spare_threshold": 5,
    "percentage_used": 6,
    "data_units_read": 12020390,
    "data_units_written": 13682990,
    "host_reads": 47358412,
    "host_writes": 151438288,
    "controller_busy_time": 2974,
    "power_cycles": 26,
    "power_on_hours": 2357,
    "unsafe_shutdowns": 3,
    "media_errors": 0,
    "num_err_log_entries": 0,
    "warning_temp_time": 0,
    "critical_comp_time": 0,
    "temperature_sensors": [
      35,
      37
    ]
  },
  "temperature": {
    "current": 35
  },
  "power_cycle_count": 26,
  "power_on_time": {
    "hours": 2357
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/nvme1"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/nvme1",
    "info_name": "/dev/nvme1",
    "type": "nvme",
    "protocol": "NVMe"
  },
  "model_name": "Micron_2200_MTFDHBA256TCK",
  "serial_number": "19292D86AB48",
  "firmware_version": "P1MU003",
  "nvme_pci_vendor": {
    "id": 4932,
    "subsystem_id": 4932
  },
  "nvme_ieee_oui_identifier": 41077,
  "nvme_controller_id": 0,
  "nvme_version": {
    "string": "1.2.1",
    "value": 66049
  },
  "nvme_number_of_namespaces": 1,
  "nvme_namespaces": [
    {
      "id": 1,
      "size": {
        "blocks": 500118192,
        "bytes": 256060514304
      },
      "capacity": {
        "blocks": 500118192,
        "bytes": 256060514304
      },
      "utilization": {
        "blocks": 500118192,
        "bytes": 256060514304
      },
      "formatted_lba_size": 512,
      "eui64": {
        "oui": 41077,
        "ext_id": 5058767688
      }
    }
  ],
  "user_capacity": {
    "blocks": 500118192,
    "bytes": 256060514304
  },
  "logical_block_size": 512,
  "local_time": {
    "time_t": 1705567889,
    "asctime": "Thu Jan 18 09:51:29 2024 CET"
  },
  "smart_status": {
    "passed": true,
    "nvme": {
      "value": 0
    }
  },
  "nvme_smart_health_information_log": {
    "critical_warning": 0,
    "temperature": 38,
    "available_spare": 100,
    "available_spare_threshold": 5,
    "percentage_used": 7,
    "data_units_read": 11102372,
    "data_units_written": 14172228,
    "host_reads": 43255583,
    "host_writes": 152013097,
    "controller_busy_time": 2959,
    "power_cycles": 26,
    "power_on_hours": 2356,
    "unsafe_shutdowns": 3,
    "media_errors": 0,
    "num_err_log_entries": 0,
    "warning_temp_time": 0,
    "critical_comp_time": 0,
    "temperature_sensors": [
      38,
      40
    ]
  },
  "temperature": {
    "current": 38
  },
  "power_cycle_count": 26,
  "power_on_time": {
    "hours": 2356
  }
}


## smartctl -a $DEVICE_NAME -d scsi -j
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sda",
      "-d",
      "scsi"
    ],
    "exit_status": 4
  },
  "device": {
    "name": "/dev/sda",
    "info_name": "/dev/sda",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "AVAGO",
  "product": "MR9380-8e",
  "model_name": "AVAGO MR9380-8e",
  "revision": "4.68",
  "scsi_version": "SPC-3",
  "user_capacity": {
    "blocks": 156254601216,
    "bytes": 80002355822592
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "serial_number": "00f32e146d8215e82470c6f20eb00506",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568131,
    "asctime": "Thu Jan 18 09:55:31 2024 CET"
  },
  "temperature": {
    "current": 0,
    "drive_trip": 0
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdb",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdb",
    "info_name": "/dev/sdb",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZLW2GVJY0000C2231WWJ",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568131,
    "asctime": "Thu Jan 18 09:55:31 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 30,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 5
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33621.587",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2742.278",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.689",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdc",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdc",
    "info_name": "/dev/sdc",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZLW2GVA10000C2231WUM",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568131,
    "asctime": "Thu Jan 18 09:55:31 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 32,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 23
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33627.791",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2750.804",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.669",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdd",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdd",
    "info_name": "/dev/sdd",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN102FW0000C2233L0B",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568132,
    "asctime": "Thu Jan 18 09:55:32 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 31,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 6
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33624.876",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2710.963",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.653",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sde",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sde",
    "info_name": "/dev/sde",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN102Y70000C2235UN6",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568133,
    "asctime": "Thu Jan 18 09:55:33 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 31,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 9
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33623.456",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2710.877",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.659",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdf",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdf",
    "info_name": "/dev/sdf",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN101R60000C2179K5S",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568134,
    "asctime": "Thu Jan 18 09:55:34 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 29,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 3
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33615.532",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2728.558",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.659",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdg",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdg",
    "info_name": "/dev/sdg",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN0X61Y0000C2180BAM",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568135,
    "asctime": "Thu Jan 18 09:55:35 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 27,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15839,
    "minutes": 54
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33621.646",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2708.366",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.686",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdh",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdh",
    "info_name": "/dev/sdh",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN102T80000C2235Z2H",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568136,
    "asctime": "Thu Jan 18 09:55:36 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 30,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 3
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33624.478",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2714.312",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.635",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdi",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdi",
    "info_name": "/dev/sdi",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN102XG0000C2235WTW",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568136,
    "asctime": "Thu Jan 18 09:55:36 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 31,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 15
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33614.203",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2705.450",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.657",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdj",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdj",
    "info_name": "/dev/sdj",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN0X6040000C2180A21",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568137,
    "asctime": "Thu Jan 18 09:55:37 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 31,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15839,
    "minutes": 54
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33626.607",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2741.292",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.638",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdk",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdk",
    "info_name": "/dev/sdk",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN102WT0000C2235WUR",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568138,
    "asctime": "Thu Jan 18 09:55:38 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 30,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 4
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33627.048",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2732.920",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.668",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdl",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdl",
    "info_name": "/dev/sdl",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN102GC0000C2236M68",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568139,
    "asctime": "Thu Jan 18 09:55:39 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 29,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 6
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33617.767",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2717.217",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.673",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdm",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/sdm",
    "info_name": "/dev/sdm",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST12000NM002G",
  "model_name": "SEAGATE ST12000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 23437770752,
    "bytes": 12000138625024
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN102W90000C2235WML",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568140,
    "asctime": "Thu Jan 18 09:55:40 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 27,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 15840,
    "minutes": 8
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "33619.963",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "2701.985",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.672",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "scsi"
    ],
    "messages": [
      {
        "string": "Smartctl open device: /dev/bus/0 failed: No such device",
        "severity": "error"
      }
    ],
    "exit_status": 2
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "scsi"
    ],
    "messages": [
      {
        "string": "Smartctl open device: /dev/bus/0 failed: No such device",
        "severity": "error"
      }
    ],
    "exit_status": 2
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "scsi"
    ],
    "messages": [
      {
        "string": "Smartctl open device: /dev/bus/0 failed: No such device",
        "severity": "error"
      }
    ],
    "exit_status": 2
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "scsi"
    ],
    "messages": [
      {
        "string": "Smartctl open device: /dev/bus/0 failed: No such device",
        "severity": "error"
      }
    ],
    "exit_status": 2
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "scsi"
    ],
    "messages": [
      {
        "string": "Smartctl open device: /dev/bus/0 failed: No such device",
        "severity": "error"
      }
    ],
    "exit_status": 2
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "scsi"
    ],
    "messages": [
      {
        "string": "Smartctl open device: /dev/bus/0 failed: No such device",
        "severity": "error"
      }
    ],
    "exit_status": 2
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "scsi"
    ],
    "messages": [
      {
        "string": "Smartctl open device: /dev/bus/0 failed: No such device",
        "severity": "error"
      }
    ],
    "exit_status": 2
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "scsi"
    ],
    "messages": [
      {
        "string": "Smartctl open device: /dev/bus/0 failed: No such device",
        "severity": "error"
      }
    ],
    "exit_status": 2
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "scsi"
    ],
    "messages": [
      {
        "string": "Smartctl open device: /dev/bus/0 failed: No such device",
        "severity": "error"
      }
    ],
    "exit_status": 2
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "scsi"
    ],
    "messages": [
      {
        "string": "Smartctl open device: /dev/bus/0 failed: No such device",
        "severity": "error"
      }
    ],
    "exit_status": 2
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/nvme0",
      "-d",
      "scsi"
    ],
    "exit_status": 2
  },
  "device": {
    "name": "/dev/nvme0",
    "info_name": "/dev/nvme0",
    "type": "scsi",
    "protocol": "SCSI"
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/nvme1",
      "-d",
      "scsi"
    ],
    "exit_status": 2
  },
  "device": {
    "name": "/dev/nvme1",
    "info_name": "/dev/nvme1",
    "type": "scsi",
    "protocol": "SCSI"
  }
}


## smartctl -a $DEVICE_NAME -d scsi -j
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "megaraid,10"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/bus/0",
    "info_name": "/dev/bus/0 [megaraid_disk_10]",
    "type": "megaraid,10",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST10000NM0096",
  "model_name": "SEAGATE ST10000NM0096",
  "revision": "E005",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 19532873728,
    "bytes": 10000831348736
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZA2AG78L0000C921NXN4",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568286,
    "asctime": "Thu Jan 18 09:58:06 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 25,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 38877,
    "minutes": 12
  },
  "scsi_grown_defect_list": 3,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 1283198485,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 1283198485,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "902572.220",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "88370.406",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 116017892,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 116017892,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "880908.542",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "megaraid,11"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/bus/0",
    "info_name": "/dev/bus/0 [megaraid_disk_11]",
    "type": "megaraid,11",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST10000NM0096",
  "model_name": "SEAGATE ST10000NM0096",
  "revision": "E005",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 19532873728,
    "bytes": 10000831348736
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZA2AMGFF0000C921NUGM",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568303,
    "asctime": "Thu Jan 18 09:58:23 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 26,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 38877,
    "minutes": 4
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 1198956605,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 1198956605,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "902199.364",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 1,
      "total_errors_corrected": 1,
      "correction_algorithm_invocations": 1,
      "gigabytes_processed": "88534.851",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 112322121,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 112322121,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "880142.825",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "megaraid,12"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/bus/0",
    "info_name": "/dev/bus/0 [megaraid_disk_12]",
    "type": "megaraid,12",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST10000NM0096",
  "model_name": "SEAGATE ST10000NM0096",
  "revision": "E005",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 19532873728,
    "bytes": 10000831348736
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZA2AMGTB0000C9247XMZ",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568307,
    "asctime": "Thu Jan 18 09:58:27 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 26,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 38877,
    "minutes": 10
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 880144598,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 880144598,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "901433.905",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "88543.630",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 4288742820,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 4288742820,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "880141.556",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "megaraid,13"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/bus/0",
    "info_name": "/dev/bus/0 [megaraid_disk_13]",
    "type": "megaraid,13",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST10000NM0096",
  "model_name": "SEAGATE ST10000NM0096",
  "revision": "E005",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 19532873728,
    "bytes": 10000831348736
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZA2AM77G0000C927BC4C",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568312,
    "asctime": "Thu Jan 18 09:58:32 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 25,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 38877,
    "minutes": 20
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 1010793754,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 1010793754,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "901403.221",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "148460.147",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 125055476,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 125055476,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "880142.334",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "megaraid,14"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/bus/0",
    "info_name": "/dev/bus/0 [megaraid_disk_14]",
    "type": "megaraid,14",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST10000NM0096",
  "model_name": "SEAGATE ST10000NM0096",
  "revision": "E005",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 19532873728,
    "bytes": 10000831348736
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZA2AMG4W0000C928BHGZ",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568317,
    "asctime": "Thu Jan 18 09:58:37 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 26,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 38876,
    "minutes": 50
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 1247384389,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 1247384389,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "902571.689",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "88523.496",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 82726066,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 82726066,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "880144.128",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "megaraid,15"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/bus/0",
    "info_name": "/dev/bus/0 [megaraid_disk_15]",
    "type": "megaraid,15",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST10000NM0096",
  "model_name": "SEAGATE ST10000NM0096",
  "revision": "E005",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 19532873728,
    "bytes": 10000831348736
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZA2AMGDC0000C9273U49",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568322,
    "asctime": "Thu Jan 18 09:58:42 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 26,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 38877,
    "minutes": 26
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 872867626,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 872867626,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "901390.470",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "88517.852",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 4289653649,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 4289653649,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "880144.233",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "megaraid,16"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/bus/0",
    "info_name": "/dev/bus/0 [megaraid_disk_16]",
    "type": "megaraid,16",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST10000NM0096",
  "model_name": "SEAGATE ST10000NM0096",
  "revision": "E005",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 19532873728,
    "bytes": 10000831348736
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZA2AMGB10000C922T3F4",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568327,
    "asctime": "Thu Jan 18 09:58:47 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 25,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 38877,
    "minutes": 13
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 1014489580,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 1014489580,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "901982.173",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "148525.210",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 4289105028,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 4289105028,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "880142.936",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "megaraid,17"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/bus/0",
    "info_name": "/dev/bus/0 [megaraid_disk_17]",
    "type": "megaraid,17",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST10000NM0096",
  "model_name": "SEAGATE ST10000NM0096",
  "revision": "E005",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 19532873728,
    "bytes": 10000831348736
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZA2AMGN90000C910M9XG",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568332,
    "asctime": "Thu Jan 18 09:58:52 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 26,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 38877,
    "minutes": 7
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 936969963,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 936969963,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "901544.777",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "88381.926",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 19944726,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 19944726,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "880141.730",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "megaraid,18"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/bus/0",
    "info_name": "/dev/bus/0 [megaraid_disk_18]",
    "type": "megaraid,18",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST10000NM002G",
  "model_name": "SEAGATE ST10000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 19532873728,
    "bytes": 10000831348736
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZS51D1030000C2309XX0",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568338,
    "asctime": "Thu Jan 18 09:58:58 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 25,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 2184,
    "minutes": 17
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "119107.050",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "16631.791",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "110032.086",
      "total_uncorrected_errors": 0
    }
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      2
    ],
    "svn_revision": "5155",
    "platform_info": "x86_64-linux-5.10.0-27-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/bus/0",
      "-d",
      "megaraid,19"
    ],
    "exit_status": 0
  },
  "device": {
    "name": "/dev/bus/0",
    "info_name": "/dev/bus/0 [megaraid_disk_19]",
    "type": "megaraid,19",
    "protocol": "SCSI"
  },
  "vendor": "SEAGATE",
  "product": "ST10000NM002G",
  "model_name": "SEAGATE ST10000NM002G",
  "revision": "E003",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 19532873728,
    "bytes": 10000831348736
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "serial_number": "ZTN11VNZ0000C232CP2D",
  "device_type": {
    "scsi_value": 0,
    "name": "disk"
  },
  "local_time": {
    "time_t": 1705568344,
    "asctime": "Thu Jan 18 09:59:04 2024 CET"
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 26,
    "drive_trip": 60
  },
  "power_on_time": {
    "hours": 2184,
    "minutes": 19
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "119225.025",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "16698.240",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "110032.463",
      "total_uncorrected_errors": 0
    }
  }
}
