## smartctl -j -V
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-j",
      "-V"
    ],
    "exit_status": 0
  }
}


## smartctl -j --scan
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "--scan",
      "-j"
    ],
    "exit_status": 0
  },
  "devices": [
    {
      "name": "/dev/sda",
      "info_name": "/dev/sda",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdb",
      "info_name": "/dev/sdb",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdc",
      "info_name": "/dev/sdc",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdd",
      "info_name": "/dev/sdd",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sde",
      "info_name": "/dev/sde",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdf",
      "info_name": "/dev/sdf",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdg",
      "info_name": "/dev/sdg",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdh",
      "info_name": "/dev/sdh",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdi",
      "info_name": "/dev/sdi",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdj",
      "info_name": "/dev/sdj",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdk",
      "info_name": "/dev/sdk",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdl",
      "info_name": "/dev/sdl",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdm",
      "info_name": "/dev/sdm",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdn",
      "info_name": "/dev/sdn",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdo",
      "info_name": "/dev/sdo",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdp",
      "info_name": "/dev/sdp",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdq",
      "info_name": "/dev/sdq",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdr",
      "info_name": "/dev/sdr",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sds",
      "info_name": "/dev/sds",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdt",
      "info_name": "/dev/sdt",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdu",
      "info_name": "/dev/sdu",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdv",
      "info_name": "/dev/sdv",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdw",
      "info_name": "/dev/sdw",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdx",
      "info_name": "/dev/sdx",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdy",
      "info_name": "/dev/sdy",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdz",
      "info_name": "/dev/sdz",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdaa",
      "info_name": "/dev/sdaa",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdab",
      "info_name": "/dev/sdab",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdac",
      "info_name": "/dev/sdac",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdad",
      "info_name": "/dev/sdad",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdae",
      "info_name": "/dev/sdae",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdaf",
      "info_name": "/dev/sdaf",
      "type": "scsi",
      "protocol": "SCSI"
    }
  ]
}


## smartctl --scan -d sat -j
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "--scan",
      "-j",
      "-d",
      "sat"
    ],
    "exit_status": 0
  },
  "devices": [
    {
      "name": "/dev/sda",
      "info_name": "/dev/sda",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdb",
      "info_name": "/dev/sdb",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdc",
      "info_name": "/dev/sdc",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdd",
      "info_name": "/dev/sdd",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sde",
      "info_name": "/dev/sde",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdf",
      "info_name": "/dev/sdf",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdg",
      "info_name": "/dev/sdg",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdh",
      "info_name": "/dev/sdh",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdi",
      "info_name": "/dev/sdi",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdj",
      "info_name": "/dev/sdj",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdk",
      "info_name": "/dev/sdk",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdl",
      "info_name": "/dev/sdl",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdm",
      "info_name": "/dev/sdm",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdn",
      "info_name": "/dev/sdn",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdo",
      "info_name": "/dev/sdo",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdp",
      "info_name": "/dev/sdp",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdq",
      "info_name": "/dev/sdq",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdr",
      "info_name": "/dev/sdr",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sds",
      "info_name": "/dev/sds",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdt",
      "info_name": "/dev/sdt",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdu",
      "info_name": "/dev/sdu",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdv",
      "info_name": "/dev/sdv",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdw",
      "info_name": "/dev/sdw",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdx",
      "info_name": "/dev/sdx",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdy",
      "info_name": "/dev/sdy",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdz",
      "info_name": "/dev/sdz",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdaa",
      "info_name": "/dev/sdaa",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdab",
      "info_name": "/dev/sdab",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdac",
      "info_name": "/dev/sdac",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdad",
      "info_name": "/dev/sdad",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdae",
      "info_name": "/dev/sdae",
      "type": "scsi",
      "protocol": "SCSI"
    },
    {
      "name": "/dev/sdaf",
      "info_name": "/dev/sdaf",
      "type": "scsi",
      "protocol": "SCSI"
    }
  ]
}


## smartctl -a $DEVICE_NAME -j
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sda"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569565,
    "asctime": "Thu Jan 18 10:19:25 2024 CET"
  },
  "device": {
    "name": "/dev/sda",
    "info_name": "/dev/sda",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "SAMSUNG",
  "scsi_product": "MZILT960HBHQ/007",
  "scsi_model_name": "SAMSUNG MZILT960HBHQ/007",
  "scsi_revision": "GXA0",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 1875385008,
    "bytes": 960197124096
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "resource provisioned",
    "value": 1,
    "management_enabled": {
      "name": "LBPME",
      "value": 1
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 1
    }
  },
  "rotation_rate": 0,
  "form_factor": {
    "scsi_value": 3,
    "name": "2.5 inches"
  },
  "logical_unit_id": "0x5002538b731302a0",
  "serial_number": "S5G1NC0W102239",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "scsi_percentage_used_endurance_indicator": 0,
  "temperature": {
    "current": 35,
    "drive_trip": 74
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 29
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2023",
    "week_of_manufacture": "01",
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 0,
    "accumulated_load_unload_cycles": 0
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "12.699",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "6082.745",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_pending_defects": {
    "count": 0
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 3600
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdb"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569565,
    "asctime": "Thu Jan 18 10:19:25 2024 CET"
  },
  "device": {
    "name": "/dev/sdb",
    "info_name": "/dev/sdb",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3a03798",
  "serial_number": "VR2V3JBK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 39,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3865,
    "minutes": 55
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "47",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 101
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 653809,
      "gigabytes_processed": "6315.655",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 832109,
      "gigabytes_processed": "2105.744",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 7389,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 8,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 54399
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdc"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569565,
    "asctime": "Thu Jan 18 10:19:25 2024 CET"
  },
  "device": {
    "name": "/dev/sdc",
    "info_name": "/dev/sdc",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3bcf96c",
  "serial_number": "VR3AXTZK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 38,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3865,
    "minutes": 54
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "46",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 102
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 662615,
      "gigabytes_processed": "6414.491",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 871779,
      "gigabytes_processed": "2139.273",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 1623,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 8,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 48979
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdd"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569566,
    "asctime": "Thu Jan 18 10:19:26 2024 CET"
  },
  "device": {
    "name": "/dev/sdd",
    "info_name": "/dev/sdd",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3bb74a4",
  "serial_number": "VR3A2XAK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 40,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3865,
    "minutes": 57
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "46",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 101
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 674066,
      "gigabytes_processed": "6432.210",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 759936,
      "gigabytes_processed": "2147.660",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 3675,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 8,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 46994
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sde"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569566,
    "asctime": "Thu Jan 18 10:19:26 2024 CET"
  },
  "device": {
    "name": "/dev/sde",
    "info_name": "/dev/sde",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c39fda5c",
  "serial_number": "VR2UX9WK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 39,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3865,
    "minutes": 56
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "47",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 101
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 667797,
      "gigabytes_processed": "6424.631",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 850824,
      "gigabytes_processed": "2136.953",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 4827,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 8,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 49082
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdf"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569566,
    "asctime": "Thu Jan 18 10:19:26 2024 CET"
  },
  "device": {
    "name": "/dev/sdf",
    "info_name": "/dev/sdf",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c39a3dc0",
  "serial_number": "VR2RUMZK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 35,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 56
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "47",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 102
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 661906,
      "gigabytes_processed": "6445.246",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 840050,
      "gigabytes_processed": "2122.981",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 975,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 47699
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdg"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569566,
    "asctime": "Thu Jan 18 10:19:26 2024 CET"
  },
  "device": {
    "name": "/dev/sdg",
    "info_name": "/dev/sdg",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c390eee4",
  "serial_number": "VR2KPYJP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 41,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 56
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 654023,
      "gigabytes_processed": "6416.560",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 660140,
      "gigabytes_processed": "2126.413",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 1042,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53524
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdh"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569567,
    "asctime": "Thu Jan 18 10:19:27 2024 CET"
  },
  "device": {
    "name": "/dev/sdh",
    "info_name": "/dev/sdh",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c39a857c",
  "serial_number": "VR2RZE2K",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 44,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 57
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "47",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 100
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 664877,
      "gigabytes_processed": "6420.440",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 662671,
      "gigabytes_processed": "2124.411",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 1906,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 59067
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569567,
    "asctime": "Thu Jan 18 10:19:27 2024 CET"
  },
  "device": {
    "name": "/dev/sdi",
    "info_name": "/dev/sdi",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3aa0524",
  "serial_number": "VR30HNBK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 36,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 58
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 100
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 662535,
      "gigabytes_processed": "6469.127",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 851522,
      "gigabytes_processed": "2139.620",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 2123,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53517
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdj"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569567,
    "asctime": "Thu Jan 18 10:19:27 2024 CET"
  },
  "device": {
    "name": "/dev/sdj",
    "info_name": "/dev/sdj",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3a494cc",
  "serial_number": "VR2XHXVP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 39,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 57
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 99
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 655050,
      "gigabytes_processed": "6409.723",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 884289,
      "gigabytes_processed": "2118.150",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 2095,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 57014
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdk"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569567,
    "asctime": "Thu Jan 18 10:19:27 2024 CET"
  },
  "device": {
    "name": "/dev/sdk",
    "info_name": "/dev/sdk",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c390ecb0",
  "serial_number": "VR2KPTZP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 44,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3865,
    "minutes": 54
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 662565,
      "gigabytes_processed": "6385.632",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 853752,
      "gigabytes_processed": "2121.836",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 1059,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 8,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53590
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdl"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569567,
    "asctime": "Thu Jan 18 10:19:27 2024 CET"
  },
  "device": {
    "name": "/dev/sdl",
    "info_name": "/dev/sdl",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3a04118",
  "serial_number": "VR2V44ZK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 45,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 58
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "47",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 101
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 649571,
      "gigabytes_processed": "6391.646",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 667183,
      "gigabytes_processed": "2116.498",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 3608,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 2,
      "string": "Background long"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 2370,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_self_test_1": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53580
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdm"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569568,
    "asctime": "Thu Jan 18 10:19:28 2024 CET"
  },
  "device": {
    "name": "/dev/sdm",
    "info_name": "/dev/sdm",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3ab3658",
  "serial_number": "VR314ZGK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 43,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3865,
    "minutes": 55
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 100
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 660181,
      "gigabytes_processed": "7075.483",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 714543,
      "gigabytes_processed": "2129.915",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 4632,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 8,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53453
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdn"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569568,
    "asctime": "Thu Jan 18 10:19:28 2024 CET"
  },
  "device": {
    "name": "/dev/sdn",
    "info_name": "/dev/sdn",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3b0d654",
  "serial_number": "VR347WAP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 45,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 57
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 99
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 653914,
      "gigabytes_processed": "6423.440",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 816916,
      "gigabytes_processed": "2125.523",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 7400,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 50064
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdo"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569568,
    "asctime": "Thu Jan 18 10:19:28 2024 CET"
  },
  "device": {
    "name": "/dev/sdo",
    "info_name": "/dev/sdo",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3aa9e8c",
  "serial_number": "VR30UW2K",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 38,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3863,
    "minutes": 24
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 665967,
      "gigabytes_processed": "6458.457",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 856264,
      "gigabytes_processed": "2139.268",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 2305,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 6,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 52814
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdp"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569568,
    "asctime": "Thu Jan 18 10:19:28 2024 CET"
  },
  "device": {
    "name": "/dev/sdp",
    "info_name": "/dev/sdp",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "SAMSUNG",
  "scsi_product": "MZILT960HBHQ/007",
  "scsi_model_name": "SAMSUNG MZILT960HBHQ/007",
  "scsi_revision": "GXA0",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 1875385008,
    "bytes": 960197124096
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "resource provisioned",
    "value": 1,
    "management_enabled": {
      "name": "LBPME",
      "value": 1
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 1
    }
  },
  "rotation_rate": 0,
  "form_factor": {
    "scsi_value": 3,
    "name": "2.5 inches"
  },
  "logical_unit_id": "0x5002538b73130840",
  "serial_number": "S5G1NC0W102329",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "scsi_percentage_used_endurance_indicator": 0,
  "temperature": {
    "current": 36,
    "drive_trip": 74
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 55
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2023",
    "week_of_manufacture": "01",
    "accumulated_start_stop_cycles": 7,
    "specified_load_unload_count_over_device_lifetime": 0,
    "accumulated_load_unload_cycles": 0
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "12.492",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "6082.730",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_pending_defects": {
    "count": 0
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 3600
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdq"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569568,
    "asctime": "Thu Jan 18 10:19:28 2024 CET"
  },
  "device": {
    "name": "/dev/sdq",
    "info_name": "/dev/sdq",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c373187c",
  "serial_number": "VR2197XP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 39,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3863,
    "minutes": 24
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 99
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 661654,
      "gigabytes_processed": "6461.232",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 870075,
      "gigabytes_processed": "2136.954",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 5549,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 6,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 49055
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdr"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569569,
    "asctime": "Thu Jan 18 10:19:29 2024 CET"
  },
  "device": {
    "name": "/dev/sdr",
    "info_name": "/dev/sdr",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c39e0320",
  "serial_number": "VR2TWY0P",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 40,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 57
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 100
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 654513,
      "gigabytes_processed": "6434.398",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 817938,
      "gigabytes_processed": "2128.539",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 5096,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 52306
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sds"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569569,
    "asctime": "Thu Jan 18 10:19:29 2024 CET"
  },
  "device": {
    "name": "/dev/sds",
    "info_name": "/dev/sds",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3aacdf8",
  "serial_number": "VR30Y0ZK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 40,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3863,
    "minutes": 23
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 99
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 651489,
      "gigabytes_processed": "6352.592",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 828655,
      "gigabytes_processed": "2105.744",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 7214,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 6,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 57841
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdt"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569569,
    "asctime": "Thu Jan 18 10:19:29 2024 CET"
  },
  "device": {
    "name": "/dev/sdt",
    "info_name": "/dev/sdt",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3add088",
  "serial_number": "VR32LAUK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 40,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3863,
    "minutes": 24
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 673864,
      "gigabytes_processed": "6478.145",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 557413,
      "gigabytes_processed": "2147.659",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 2876,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 6,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53345
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdu"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569569,
    "asctime": "Thu Jan 18 10:19:29 2024 CET"
  },
  "device": {
    "name": "/dev/sdu",
    "info_name": "/dev/sdu",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3abd2e0",
  "serial_number": "VR31HDMK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 45,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3863,
    "minutes": 25
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 654974,
      "gigabytes_processed": "6398.929",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 881378,
      "gigabytes_processed": "2124.410",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 3769,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 6,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 51221
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdv"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569570,
    "asctime": "Thu Jan 18 10:19:30 2024 CET"
  },
  "device": {
    "name": "/dev/sdv",
    "info_name": "/dev/sdv",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3757af8",
  "serial_number": "VR22LX8P",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 36,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3863,
    "minutes": 27
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 658213,
      "gigabytes_processed": "6418.277",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 746843,
      "gigabytes_processed": "2122.979",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 8286,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 6,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 48144
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdw"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569570,
    "asctime": "Thu Jan 18 10:19:30 2024 CET"
  },
  "device": {
    "name": "/dev/sdw",
    "info_name": "/dev/sdw",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c390e258",
  "serial_number": "VR2KP3MP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 47,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 24
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 97
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 650517,
      "gigabytes_processed": "6353.739",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 876381,
      "gigabytes_processed": "2116.499",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 1667,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 51965
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdx"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569570,
    "asctime": "Thu Jan 18 10:19:30 2024 CET"
  },
  "device": {
    "name": "/dev/sdx",
    "info_name": "/dev/sdx",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3b33610",
  "serial_number": "VR35KB0P",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 45,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 22
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 96
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 657054,
      "gigabytes_processed": "6368.722",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 727099,
      "gigabytes_processed": "2121.840",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 2371,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 52610
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdy"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569570,
    "asctime": "Thu Jan 18 10:19:30 2024 CET"
  },
  "device": {
    "name": "/dev/sdy",
    "info_name": "/dev/sdy",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c37579c8",
  "serial_number": "VR22LUUP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 36,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 24
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 97
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 660954,
      "gigabytes_processed": "6420.010",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 842997,
      "gigabytes_processed": "2139.636",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 2046,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 49390
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdz"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569571,
    "asctime": "Thu Jan 18 10:19:31 2024 CET"
  },
  "device": {
    "name": "/dev/sdz",
    "info_name": "/dev/sdz",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3aacc18",
  "serial_number": "VR30XX3K",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 40,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 24
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 649667,
      "gigabytes_processed": "6351.452",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 825007,
      "gigabytes_processed": "2118.166",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 1474,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53264
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdaa"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569571,
    "asctime": "Thu Jan 18 10:19:31 2024 CET"
  },
  "device": {
    "name": "/dev/sdaa",
    "info_name": "/dev/sdaa",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3b02e58",
  "serial_number": "VR33WPJP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 42,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 23
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 97
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 658018,
      "gigabytes_processed": "6379.470",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 847883,
      "gigabytes_processed": "2126.423",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 3433,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 58443
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdab"
    ],
    "drive_database_version": {
      "string": "7.3/5319"
    },
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569571,
    "asctime": "Thu Jan 18 10:19:31 2024 CET"
  },
  "device": {
    "name": "/dev/sdab",
    "info_name": "/dev/sdab [SAT]",
    "type": "sat",
    "protocol": "ATA"
  },
  "model_family": "Intel S4510/S4610/S4500/S4600 Series SSDs",
  "model_name": "INTEL SSDSC2KB480GZ",
  "serial_number": "PHYI233307QZ480BGN",
  "wwn": {
    "naa": 5,
    "oui": 6083300,
    "id": 5737964647
  },
  "firmware_version": "7CV10120",
  "user_capacity": {
    "blocks": 937703088,
    "bytes": 480103981056
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 0,
  "form_factor": {
    "ata_value": 3,
    "name": "2.5 inches"
  },
  "trim": {
    "supported": true,
    "deterministic": true,
    "zeroed": true
  },
  "in_smartctl_database": true,
  "ata_version": {
    "string": "ACS-3 T13/2161-D revision 5",
    "major_value": 2044,
    "minor_value": 109
  },
  "sata_version": {
    "string": "SATA 3.2",
    "value": 255
  },
  "interface_speed": {
    "max": {
      "sata_value": 14,
      "string": "6.0 Gb/s",
      "units_per_second": 60,
      "bits_per_unit": 100000000
    },
    "current": {
      "sata_value": 3,
      "string": "6.0 Gb/s",
      "units_per_second": 60,
      "bits_per_unit": 100000000
    }
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "ata_smart_data": {
    "offline_data_collection": {
      "status": {
        "value": 2,
        "string": "was completed without error",
        "passed": true
      },
      "completion_seconds": 2
    },
    "self_test": {
      "status": {
        "value": 0,
        "string": "completed without error",
        "passed": true
      },
      "polling_minutes": {
        "short": 1,
        "extended": 2,
        "conveyance": 2
      }
    },
    "capabilities": {
      "values": [
        121,
        3
      ],
      "exec_offline_immediate_supported": true,
      "offline_is_aborted_upon_new_cmd": false,
      "offline_surface_scan_supported": true,
      "self_tests_supported": true,
      "conveyance_self_test_supported": true,
      "selective_self_test_supported": true,
      "attribute_autosave_enabled": true,
      "error_logging_supported": true,
      "gp_logging_supported": true
    }
  },
  "ata_sct_capabilities": {
    "value": 61,
    "error_recovery_control_supported": true,
    "feature_control_supported": true,
    "data_table_supported": true
  },
  "ata_smart_attributes": {
    "revision": 1,
    "table": [
      {
        "id": 5,
        "name": "Reallocated_Sector_Ct",
        "value": 66,
        "worst": 66,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 9,
        "name": "Power_On_Hours",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 3876,
          "string": "3876"
        }
      },
      {
        "id": 12,
        "name": "Power_Cycle_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 15,
          "string": "15"
        }
      },
      {
        "id": 170,
        "name": "Available_Reservd_Space",
        "value": 100,
        "worst": 100,
        "thresh": 10,
        "when_failed": "",
        "flags": {
          "value": 51,
          "string": "PO--CK ",
          "prefailure": true,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 171,
        "name": "Program_Fail_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 172,
        "name": "Erase_Fail_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 174,
        "name": "Unsafe_Shutdown_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 12,
          "string": "12"
        }
      },
      {
        "id": 175,
        "name": "Power_Loss_Cap_Test",
        "value": 100,
        "worst": 100,
        "thresh": 10,
        "when_failed": "",
        "flags": {
          "value": 51,
          "string": "PO--CK ",
          "prefailure": true,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 71514720474,
          "string": "2266 (16 42652)"
        }
      },
      {
        "id": 183,
        "name": "SATA_Downshift_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 184,
        "name": "End-to-End_Error_Count",
        "value": 100,
        "worst": 100,
        "thresh": 90,
        "when_failed": "",
        "flags": {
          "value": 51,
          "string": "PO--CK ",
          "prefailure": true,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 187,
        "name": "Uncorrectable_Error_Cnt",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 190,
        "name": "Drive_Temperature",
        "value": 72,
        "worst": 71,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 34,
          "string": "-O---K ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": false,
          "auto_keep": true
        },
        "raw": {
          "value": 487981084,
          "string": "28 (Min/Max 22/29)"
        }
      },
      {
        "id": 192,
        "name": "Unsafe_Shutdown_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 12,
          "string": "12"
        }
      },
      {
        "id": 194,
        "name": "Temperature_Celsius",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 34,
          "string": "-O---K ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": false,
          "auto_keep": true
        },
        "raw": {
          "value": 28,
          "string": "28"
        }
      },
      {
        "id": 197,
        "name": "Pending_Sector_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 18,
          "string": "-O--C- ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": false
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 199,
        "name": "CRC_Error_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 62,
          "string": "-OSRCK ",
          "prefailure": false,
          "updated_online": true,
          "performance": true,
          "error_rate": true,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 225,
        "name": "Host_Writes_32MiB",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 27352,
          "string": "27352"
        }
      },
      {
        "id": 226,
        "name": "Workld_Media_Wear_Indic",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 20,
          "string": "20"
        }
      },
      {
        "id": 227,
        "name": "Workld_Host_Reads_Perc",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 77,
          "string": "77"
        }
      },
      {
        "id": 228,
        "name": "Workload_Minutes",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 232537,
          "string": "232537"
        }
      },
      {
        "id": 229,
        "name": "Unknown_Attribute",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 230,
        "name": "Unknown_SSD_Attribute",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 232,
        "name": "Available_Reservd_Space",
        "value": 100,
        "worst": 100,
        "thresh": 10,
        "when_failed": "",
        "flags": {
          "value": 51,
          "string": "PO--CK ",
          "prefailure": true,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 233,
        "name": "Media_Wearout_Indicator",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 234,
        "name": "Thermal_Throttle_Status",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0/0"
        }
      },
      {
        "id": 235,
        "name": "Power_Loss_Cap_Test",
        "value": 100,
        "worst": 100,
        "thresh": 10,
        "when_failed": "",
        "flags": {
          "value": 51,
          "string": "PO--CK ",
          "prefailure": true,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 71514720474,
          "string": "2266 (16 42652)"
        }
      },
      {
        "id": 241,
        "name": "Host_Writes_32MiB",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 27352,
          "string": "27352"
        }
      },
      {
        "id": 242,
        "name": "Host_Reads_32MiB",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 93328,
          "string": "93328"
        }
      },
      {
        "id": 243,
        "name": "NAND_Writes_32MiB",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 50661,
          "string": "50661"
        }
      },
      {
        "id": 246,
        "name": "Unknown_Attribute",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      }
    ]
  },
  "power_on_time": {
    "hours": 3876
  },
  "power_cycle_count": 15,
  "temperature": {
    "current": 28
  },
  "ata_smart_error_log": {
    "summary": {
      "revision": 1,
      "count": 0
    }
  },
  "ata_smart_self_test_log": {
    "standard": {
      "revision": 1,
      "table": [
        {
          "type": {
            "value": 1,
            "string": "Short offline"
          },
          "status": {
            "value": 0,
            "string": "Completed without error",
            "passed": true
          },
          "lifetime_hours": 20
        }
      ],
      "count": 1,
      "error_count_total": 0,
      "error_count_outdated": 0
    }
  },
  "ata_smart_selective_self_test_log": {
    "revision": 1,
    "table": [
      {
        "lba_min": 0,
        "lba_max": 0,
        "status": {
          "value": 0,
          "string": "Not_testing"
        }
      },
      {
        "lba_min": 0,
        "lba_max": 0,
        "status": {
          "value": 0,
          "string": "Not_testing"
        }
      },
      {
        "lba_min": 0,
        "lba_max": 0,
        "status": {
          "value": 0,
          "string": "Not_testing"
        }
      },
      {
        "lba_min": 0,
        "lba_max": 0,
        "status": {
          "value": 0,
          "string": "Not_testing"
        }
      },
      {
        "lba_min": 0,
        "lba_max": 0,
        "status": {
          "value": 0,
          "string": "Not_testing"
        }
      }
    ],
    "flags": {
      "value": 0,
      "remainder_scan_enabled": false
    },
    "power_up_scan_resume_minutes": 0
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdac"
    ],
    "drive_database_version": {
      "string": "7.3/5319"
    },
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569571,
    "asctime": "Thu Jan 18 10:19:31 2024 CET"
  },
  "device": {
    "name": "/dev/sdac",
    "info_name": "/dev/sdac [SAT]",
    "type": "sat",
    "protocol": "ATA"
  },
  "model_family": "Intel S4510/S4610/S4500/S4600 Series SSDs",
  "model_name": "INTEL SSDSC2KB480GZ",
  "serial_number": "PHYI233307HB480BGN",
  "wwn": {
    "naa": 5,
    "oui": 6083300,
    "id": 5737964387
  },
  "firmware_version": "7CV10120",
  "user_capacity": {
    "blocks": 937703088,
    "bytes": 480103981056
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "rotation_rate": 0,
  "form_factor": {
    "ata_value": 3,
    "name": "2.5 inches"
  },
  "trim": {
    "supported": true,
    "deterministic": true,
    "zeroed": true
  },
  "in_smartctl_database": true,
  "ata_version": {
    "string": "ACS-3 T13/2161-D revision 5",
    "major_value": 2044,
    "minor_value": 109
  },
  "sata_version": {
    "string": "SATA 3.2",
    "value": 255
  },
  "interface_speed": {
    "max": {
      "sata_value": 14,
      "string": "6.0 Gb/s",
      "units_per_second": 60,
      "bits_per_unit": 100000000
    },
    "current": {
      "sata_value": 3,
      "string": "6.0 Gb/s",
      "units_per_second": 60,
      "bits_per_unit": 100000000
    }
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "ata_smart_data": {
    "offline_data_collection": {
      "status": {
        "value": 2,
        "string": "was completed without error",
        "passed": true
      },
      "completion_seconds": 2
    },
    "self_test": {
      "status": {
        "value": 0,
        "string": "completed without error",
        "passed": true
      },
      "polling_minutes": {
        "short": 1,
        "extended": 2,
        "conveyance": 2
      }
    },
    "capabilities": {
      "values": [
        121,
        3
      ],
      "exec_offline_immediate_supported": true,
      "offline_is_aborted_upon_new_cmd": false,
      "offline_surface_scan_supported": true,
      "self_tests_supported": true,
      "conveyance_self_test_supported": true,
      "selective_self_test_supported": true,
      "attribute_autosave_enabled": true,
      "error_logging_supported": true,
      "gp_logging_supported": true
    }
  },
  "ata_sct_capabilities": {
    "value": 61,
    "error_recovery_control_supported": true,
    "feature_control_supported": true,
    "data_table_supported": true
  },
  "ata_smart_attributes": {
    "revision": 1,
    "table": [
      {
        "id": 5,
        "name": "Reallocated_Sector_Ct",
        "value": 66,
        "worst": 66,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 9,
        "name": "Power_On_Hours",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 3877,
          "string": "3877"
        }
      },
      {
        "id": 12,
        "name": "Power_Cycle_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 17,
          "string": "17"
        }
      },
      {
        "id": 170,
        "name": "Available_Reservd_Space",
        "value": 100,
        "worst": 100,
        "thresh": 10,
        "when_failed": "",
        "flags": {
          "value": 51,
          "string": "PO--CK ",
          "prefailure": true,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 171,
        "name": "Program_Fail_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 172,
        "name": "Erase_Fail_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 174,
        "name": "Unsafe_Shutdown_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 14,
          "string": "14"
        }
      },
      {
        "id": 175,
        "name": "Power_Loss_Cap_Test",
        "value": 100,
        "worst": 100,
        "thresh": 10,
        "when_failed": "",
        "flags": {
          "value": 51,
          "string": "PO--CK ",
          "prefailure": true,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 80054913271,
          "string": "2295 (18 41893)"
        }
      },
      {
        "id": 183,
        "name": "SATA_Downshift_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 184,
        "name": "End-to-End_Error_Count",
        "value": 100,
        "worst": 100,
        "thresh": 90,
        "when_failed": "",
        "flags": {
          "value": 51,
          "string": "PO--CK ",
          "prefailure": true,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 187,
        "name": "Uncorrectable_Error_Cnt",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 190,
        "name": "Drive_Temperature",
        "value": 72,
        "worst": 71,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 34,
          "string": "-O---K ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": false,
          "auto_keep": true
        },
        "raw": {
          "value": 487981084,
          "string": "28 (Min/Max 22/29)"
        }
      },
      {
        "id": 192,
        "name": "Unsafe_Shutdown_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 14,
          "string": "14"
        }
      },
      {
        "id": 194,
        "name": "Temperature_Celsius",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 34,
          "string": "-O---K ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": false,
          "auto_keep": true
        },
        "raw": {
          "value": 28,
          "string": "28"
        }
      },
      {
        "id": 197,
        "name": "Pending_Sector_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 18,
          "string": "-O--C- ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": false
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 199,
        "name": "CRC_Error_Count",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 62,
          "string": "-OSRCK ",
          "prefailure": false,
          "updated_online": true,
          "performance": true,
          "error_rate": true,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 225,
        "name": "Host_Writes_32MiB",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 41185,
          "string": "41185"
        }
      },
      {
        "id": 226,
        "name": "Workld_Media_Wear_Indic",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 20,
          "string": "20"
        }
      },
      {
        "id": 227,
        "name": "Workld_Host_Reads_Perc",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 65,
          "string": "65"
        }
      },
      {
        "id": 228,
        "name": "Workload_Minutes",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 232605,
          "string": "232605"
        }
      },
      {
        "id": 229,
        "name": "Unknown_Attribute",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 230,
        "name": "Unknown_SSD_Attribute",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 232,
        "name": "Available_Reservd_Space",
        "value": 100,
        "worst": 100,
        "thresh": 10,
        "when_failed": "",
        "flags": {
          "value": 51,
          "string": "PO--CK ",
          "prefailure": true,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 233,
        "name": "Media_Wearout_Indicator",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      },
      {
        "id": 234,
        "name": "Thermal_Throttle_Status",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0/0"
        }
      },
      {
        "id": 235,
        "name": "Power_Loss_Cap_Test",
        "value": 100,
        "worst": 100,
        "thresh": 10,
        "when_failed": "",
        "flags": {
          "value": 51,
          "string": "PO--CK ",
          "prefailure": true,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 80054913271,
          "string": "2295 (18 41893)"
        }
      },
      {
        "id": 241,
        "name": "Host_Writes_32MiB",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 41185,
          "string": "41185"
        }
      },
      {
        "id": 242,
        "name": "Host_Reads_32MiB",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 79113,
          "string": "79113"
        }
      },
      {
        "id": 243,
        "name": "NAND_Writes_32MiB",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 67735,
          "string": "67735"
        }
      },
      {
        "id": 246,
        "name": "Unknown_Attribute",
        "value": 100,
        "worst": 100,
        "thresh": 0,
        "when_failed": "",
        "flags": {
          "value": 50,
          "string": "-O--CK ",
          "prefailure": false,
          "updated_online": true,
          "performance": false,
          "error_rate": false,
          "event_count": true,
          "auto_keep": true
        },
        "raw": {
          "value": 0,
          "string": "0"
        }
      }
    ]
  },
  "power_on_time": {
    "hours": 3877
  },
  "power_cycle_count": 17,
  "temperature": {
    "current": 28
  },
  "ata_smart_error_log": {
    "summary": {
      "revision": 1,
      "count": 0
    }
  },
  "ata_smart_self_test_log": {
    "standard": {
      "revision": 1,
      "table": [
        {
          "type": {
            "value": 1,
            "string": "Short offline"
          },
          "status": {
            "value": 0,
            "string": "Completed without error",
            "passed": true
          },
          "lifetime_hours": 21
        }
      ],
      "count": 1,
      "error_count_total": 0,
      "error_count_outdated": 0
    }
  },
  "ata_smart_selective_self_test_log": {
    "revision": 1,
    "table": [
      {
        "lba_min": 0,
        "lba_max": 0,
        "status": {
          "value": 0,
          "string": "Not_testing"
        }
      },
      {
        "lba_min": 0,
        "lba_max": 0,
        "status": {
          "value": 0,
          "string": "Not_testing"
        }
      },
      {
        "lba_min": 0,
        "lba_max": 0,
        "status": {
          "value": 0,
          "string": "Not_testing"
        }
      },
      {
        "lba_min": 0,
        "lba_max": 0,
        "status": {
          "value": 0,
          "string": "Not_testing"
        }
      },
      {
        "lba_min": 0,
        "lba_max": 0,
        "status": {
          "value": 0,
          "string": "Not_testing"
        }
      }
    ],
    "flags": {
      "value": 0,
      "remainder_scan_enabled": false
    },
    "power_up_scan_resume_minutes": 0
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdad"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569571,
    "asctime": "Thu Jan 18 10:19:31 2024 CET"
  },
  "device": {
    "name": "/dev/sdad",
    "info_name": "/dev/sdad",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3ab1750",
  "serial_number": "VR312XDK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 41,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 22
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 658270,
      "gigabytes_processed": "6385.926",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 892414,
      "gigabytes_processed": "2128.548",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 3686,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53456
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdae"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569571,
    "asctime": "Thu Jan 18 10:19:31 2024 CET"
  },
  "device": {
    "name": "/dev/sdae",
    "info_name": "/dev/sdae",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c39e419c",
  "serial_number": "VR2U130P",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 46,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 22
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 100
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 663606,
      "gigabytes_processed": "6396.766",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 916046,
      "gigabytes_processed": "2125.536",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 5644,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 51459
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdaf"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569571,
    "asctime": "Thu Jan 18 10:19:31 2024 CET"
  },
  "device": {
    "name": "/dev/sdaf",
    "info_name": "/dev/sdaf",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3a48ce0",
  "serial_number": "VR2XHDHP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 45,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 22
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 78
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 666325,
      "gigabytes_processed": "5796.678",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 588256,
      "gigabytes_processed": "1973.594",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 1407,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 2,
      "string": "Background long"
    },
    "result": {
      "value": 2,
      "string": "Aborted (device reset ?)"
    },
    "power_on_time": {
      "hours": 3061,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_self_test_1": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 52937
}


## smartctl -a $DEVICE_NAME -d scsi -j
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sda",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569652,
    "asctime": "Thu Jan 18 10:20:52 2024 CET"
  },
  "device": {
    "name": "/dev/sda",
    "info_name": "/dev/sda",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "SAMSUNG",
  "scsi_product": "MZILT960HBHQ/007",
  "scsi_model_name": "SAMSUNG MZILT960HBHQ/007",
  "scsi_revision": "GXA0",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 1875385008,
    "bytes": 960197124096
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "resource provisioned",
    "value": 1,
    "management_enabled": {
      "name": "LBPME",
      "value": 1
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 1
    }
  },
  "rotation_rate": 0,
  "form_factor": {
    "scsi_value": 3,
    "name": "2.5 inches"
  },
  "logical_unit_id": "0x5002538b731302a0",
  "serial_number": "S5G1NC0W102239",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "scsi_percentage_used_endurance_indicator": 0,
  "temperature": {
    "current": 35,
    "drive_trip": 74
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 30
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2023",
    "week_of_manufacture": "01",
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 0,
    "accumulated_load_unload_cycles": 0
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "12.699",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "6082.745",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_pending_defects": {
    "count": 0
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 3600
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdb",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569652,
    "asctime": "Thu Jan 18 10:20:52 2024 CET"
  },
  "device": {
    "name": "/dev/sdb",
    "info_name": "/dev/sdb",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3a03798",
  "serial_number": "VR2V3JBK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 39,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3865,
    "minutes": 57
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "47",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 101
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 653809,
      "gigabytes_processed": "6315.655",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 832171,
      "gigabytes_processed": "2105.782",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 7389,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 8,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 54399
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdc",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569653,
    "asctime": "Thu Jan 18 10:20:53 2024 CET"
  },
  "device": {
    "name": "/dev/sdc",
    "info_name": "/dev/sdc",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3bcf96c",
  "serial_number": "VR3AXTZK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 38,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3865,
    "minutes": 55
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "46",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 102
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 662615,
      "gigabytes_processed": "6414.491",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 871828,
      "gigabytes_processed": "2139.310",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 1623,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 8,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 48979
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdd",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569653,
    "asctime": "Thu Jan 18 10:20:53 2024 CET"
  },
  "device": {
    "name": "/dev/sdd",
    "info_name": "/dev/sdd",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3bb74a4",
  "serial_number": "VR3A2XAK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 40,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3865,
    "minutes": 59
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "46",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 101
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 674066,
      "gigabytes_processed": "6432.210",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 759970,
      "gigabytes_processed": "2147.694",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 3675,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 8,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 46994
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sde",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569653,
    "asctime": "Thu Jan 18 10:20:53 2024 CET"
  },
  "device": {
    "name": "/dev/sde",
    "info_name": "/dev/sde",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c39fda5c",
  "serial_number": "VR2UX9WK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 39,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3865,
    "minutes": 57
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "47",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 101
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 667797,
      "gigabytes_processed": "6424.631",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 850870,
      "gigabytes_processed": "2136.990",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 4827,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 8,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 49082
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdf",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569653,
    "asctime": "Thu Jan 18 10:20:53 2024 CET"
  },
  "device": {
    "name": "/dev/sdf",
    "info_name": "/dev/sdf",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c39a3dc0",
  "serial_number": "VR2RUMZK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 35,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 57
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "47",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 102
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 661906,
      "gigabytes_processed": "6445.246",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 840081,
      "gigabytes_processed": "2123.022",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 975,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 47699
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdg",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569654,
    "asctime": "Thu Jan 18 10:20:54 2024 CET"
  },
  "device": {
    "name": "/dev/sdg",
    "info_name": "/dev/sdg",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c390eee4",
  "serial_number": "VR2KPYJP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 41,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 57
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 654023,
      "gigabytes_processed": "6416.560",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 660196,
      "gigabytes_processed": "2126.446",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 1042,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53524
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdh",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569654,
    "asctime": "Thu Jan 18 10:20:54 2024 CET"
  },
  "device": {
    "name": "/dev/sdh",
    "info_name": "/dev/sdh",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c39a857c",
  "serial_number": "VR2RZE2K",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 44,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 58
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "47",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 100
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 664877,
      "gigabytes_processed": "6420.440",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 662704,
      "gigabytes_processed": "2124.449",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 1906,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 59067
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdi",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569654,
    "asctime": "Thu Jan 18 10:20:54 2024 CET"
  },
  "device": {
    "name": "/dev/sdi",
    "info_name": "/dev/sdi",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3aa0524",
  "serial_number": "VR30HNBK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 36,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 59
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 100
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 662535,
      "gigabytes_processed": "6469.127",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 851572,
      "gigabytes_processed": "2139.656",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 2123,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53517
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdj",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569654,
    "asctime": "Thu Jan 18 10:20:54 2024 CET"
  },
  "device": {
    "name": "/dev/sdj",
    "info_name": "/dev/sdj",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3a494cc",
  "serial_number": "VR2XHXVP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 39,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 58
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 99
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 655050,
      "gigabytes_processed": "6409.723",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 884339,
      "gigabytes_processed": "2118.181",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 2095,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 57014
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdk",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569654,
    "asctime": "Thu Jan 18 10:20:54 2024 CET"
  },
  "device": {
    "name": "/dev/sdk",
    "info_name": "/dev/sdk",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c390ecb0",
  "serial_number": "VR2KPTZP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 44,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3865,
    "minutes": 56
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 662565,
      "gigabytes_processed": "6385.632",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 853806,
      "gigabytes_processed": "2121.873",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 1059,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 8,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53590
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdl",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569655,
    "asctime": "Thu Jan 18 10:20:55 2024 CET"
  },
  "device": {
    "name": "/dev/sdl",
    "info_name": "/dev/sdl",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3a04118",
  "serial_number": "VR2V44ZK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 45,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 59
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "47",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 101
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 649571,
      "gigabytes_processed": "6391.646",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 667219,
      "gigabytes_processed": "2116.533",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 3608,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 2,
      "string": "Background long"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 2370,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_self_test_1": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53580
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdm",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569655,
    "asctime": "Thu Jan 18 10:20:55 2024 CET"
  },
  "device": {
    "name": "/dev/sdm",
    "info_name": "/dev/sdm",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3ab3658",
  "serial_number": "VR314ZGK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 43,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3865,
    "minutes": 57
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 100
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 660181,
      "gigabytes_processed": "7075.483",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 714566,
      "gigabytes_processed": "2129.945",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 4632,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 8,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53453
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdn",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569655,
    "asctime": "Thu Jan 18 10:20:55 2024 CET"
  },
  "device": {
    "name": "/dev/sdn",
    "info_name": "/dev/sdn",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3b0d654",
  "serial_number": "VR347WAP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 45,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 59
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 99
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 653914,
      "gigabytes_processed": "6423.440",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 816971,
      "gigabytes_processed": "2125.559",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 7400,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 50064
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdo",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569655,
    "asctime": "Thu Jan 18 10:20:55 2024 CET"
  },
  "device": {
    "name": "/dev/sdo",
    "info_name": "/dev/sdo",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3aa9e8c",
  "serial_number": "VR30UW2K",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 38,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3863,
    "minutes": 25
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 665967,
      "gigabytes_processed": "6458.457",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 856323,
      "gigabytes_processed": "2139.305",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 2305,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 6,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 52814
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdp",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569656,
    "asctime": "Thu Jan 18 10:20:56 2024 CET"
  },
  "device": {
    "name": "/dev/sdp",
    "info_name": "/dev/sdp",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "SAMSUNG",
  "scsi_product": "MZILT960HBHQ/007",
  "scsi_model_name": "SAMSUNG MZILT960HBHQ/007",
  "scsi_revision": "GXA0",
  "scsi_version": "SPC-5",
  "user_capacity": {
    "blocks": 1875385008,
    "bytes": 960197124096
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "resource provisioned",
    "value": 1,
    "management_enabled": {
      "name": "LBPME",
      "value": 1
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 1
    }
  },
  "rotation_rate": 0,
  "form_factor": {
    "scsi_value": 3,
    "name": "2.5 inches"
  },
  "logical_unit_id": "0x5002538b73130840",
  "serial_number": "S5G1NC0W102329",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "scsi_percentage_used_endurance_indicator": 0,
  "temperature": {
    "current": 36,
    "drive_trip": 74
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 57
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2023",
    "week_of_manufacture": "01",
    "accumulated_start_stop_cycles": 7,
    "specified_load_unload_count_over_device_lifetime": 0,
    "accumulated_load_unload_cycles": 0
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "12.492",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "6082.730",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 0,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_pending_defects": {
    "count": 0
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 3600
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdq",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569656,
    "asctime": "Thu Jan 18 10:20:56 2024 CET"
  },
  "device": {
    "name": "/dev/sdq",
    "info_name": "/dev/sdq",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c373187c",
  "serial_number": "VR2197XP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 39,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3863,
    "minutes": 25
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 99
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 661654,
      "gigabytes_processed": "6461.232",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 870123,
      "gigabytes_processed": "2136.990",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 5549,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 6,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 49055
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdr",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569656,
    "asctime": "Thu Jan 18 10:20:56 2024 CET"
  },
  "device": {
    "name": "/dev/sdr",
    "info_name": "/dev/sdr",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c39e0320",
  "serial_number": "VR2TWY0P",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 40,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3862,
    "minutes": 58
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 5,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 100
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 654513,
      "gigabytes_processed": "6434.398",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 817987,
      "gigabytes_processed": "2128.573",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 5096,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 5,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 52306
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sds",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569656,
    "asctime": "Thu Jan 18 10:20:56 2024 CET"
  },
  "device": {
    "name": "/dev/sds",
    "info_name": "/dev/sds",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3aacdf8",
  "serial_number": "VR30Y0ZK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 40,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3863,
    "minutes": 25
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 99
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 651489,
      "gigabytes_processed": "6352.592",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 828712,
      "gigabytes_processed": "2105.782",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 7214,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 6,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 57841
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdt",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569656,
    "asctime": "Thu Jan 18 10:20:56 2024 CET"
  },
  "device": {
    "name": "/dev/sdt",
    "info_name": "/dev/sdt",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3add088",
  "serial_number": "VR32LAUK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 40,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3863,
    "minutes": 25
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 673864,
      "gigabytes_processed": "6478.145",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 557435,
      "gigabytes_processed": "2147.693",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 2876,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 6,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53345
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdu",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569657,
    "asctime": "Thu Jan 18 10:20:57 2024 CET"
  },
  "device": {
    "name": "/dev/sdu",
    "info_name": "/dev/sdu",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3abd2e0",
  "serial_number": "VR31HDMK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 45,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3863,
    "minutes": 26
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 654974,
      "gigabytes_processed": "6398.929",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 881433,
      "gigabytes_processed": "2124.448",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 3769,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 6,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 51221
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdv",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569657,
    "asctime": "Thu Jan 18 10:20:57 2024 CET"
  },
  "device": {
    "name": "/dev/sdv",
    "info_name": "/dev/sdv",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3757af8",
  "serial_number": "VR22LX8P",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 36,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3863,
    "minutes": 28
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 658213,
      "gigabytes_processed": "6418.277",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 746884,
      "gigabytes_processed": "2123.020",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 8286,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 6,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 48144
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdw",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569657,
    "asctime": "Thu Jan 18 10:20:57 2024 CET"
  },
  "device": {
    "name": "/dev/sdw",
    "info_name": "/dev/sdw",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c390e258",
  "serial_number": "VR2KP3MP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 47,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 25
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 97
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 650517,
      "gigabytes_processed": "6353.739",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 876422,
      "gigabytes_processed": "2116.534",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 1667,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 51965
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdx",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569657,
    "asctime": "Thu Jan 18 10:20:57 2024 CET"
  },
  "device": {
    "name": "/dev/sdx",
    "info_name": "/dev/sdx",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3b33610",
  "serial_number": "VR35KB0P",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 45,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 24
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 96
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 657054,
      "gigabytes_processed": "6368.722",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 727145,
      "gigabytes_processed": "2121.877",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 2371,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 52610
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdy",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569657,
    "asctime": "Thu Jan 18 10:20:57 2024 CET"
  },
  "device": {
    "name": "/dev/sdy",
    "info_name": "/dev/sdy",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c37579c8",
  "serial_number": "VR22LUUP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 36,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 25
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 97
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 660954,
      "gigabytes_processed": "6420.010",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 843051,
      "gigabytes_processed": "2139.672",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 2046,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 49390
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdz",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569658,
    "asctime": "Thu Jan 18 10:20:58 2024 CET"
  },
  "device": {
    "name": "/dev/sdz",
    "info_name": "/dev/sdz",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3aacc18",
  "serial_number": "VR30XX3K",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 40,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 26
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 649667,
      "gigabytes_processed": "6351.452",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 825056,
      "gigabytes_processed": "2118.197",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 1474,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53264
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdaa",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569658,
    "asctime": "Thu Jan 18 10:20:58 2024 CET"
  },
  "device": {
    "name": "/dev/sdaa",
    "info_name": "/dev/sdaa",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3b02e58",
  "serial_number": "VR33WPJP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 42,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 25
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 97
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 658018,
      "gigabytes_processed": "6379.470",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 847928,
      "gigabytes_processed": "2126.455",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 3433,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 58443
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdab",
      "-d",
      "scsi"
    ],
    "exit_status": 4
  },
  "local_time": {
    "time_t": 1705569658,
    "asctime": "Thu Jan 18 10:20:58 2024 CET"
  },
  "device": {
    "name": "/dev/sdab",
    "info_name": "/dev/sdab",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "user_capacity": {
    "blocks": 937703088,
    "bytes": 480103981056
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "not reported",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 1
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 1
    }
  },
  "rotation_rate": 0,
  "form_factor": {
    "scsi_value": 3,
    "name": "2.5 inches"
  },
  "logical_unit_id": "0x55cd2e4156026467",
  "serial_number": "PHYI233307QZ480BGN",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "smart_support": {
    "available": false
  },
  "temperature": {
    "current": 0
  },
  "scsi_temperature": {
    "drive_trip": 0
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdac",
      "-d",
      "scsi"
    ],
    "exit_status": 4
  },
  "local_time": {
    "time_t": 1705569658,
    "asctime": "Thu Jan 18 10:20:58 2024 CET"
  },
  "device": {
    "name": "/dev/sdac",
    "info_name": "/dev/sdac",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "user_capacity": {
    "blocks": 937703088,
    "bytes": 480103981056
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "not reported",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 1
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 1
    }
  },
  "rotation_rate": 0,
  "form_factor": {
    "scsi_value": 3,
    "name": "2.5 inches"
  },
  "logical_unit_id": "0x55cd2e4156026363",
  "serial_number": "PHYI233307HB480BGN",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "smart_support": {
    "available": false
  },
  "temperature": {
    "current": 0
  },
  "scsi_temperature": {
    "drive_trip": 0
  }
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdad",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569658,
    "asctime": "Thu Jan 18 10:20:58 2024 CET"
  },
  "device": {
    "name": "/dev/sdad",
    "info_name": "/dev/sdad",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3ab1750",
  "serial_number": "VR312XDK",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 41,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 24
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 98
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 658270,
      "gigabytes_processed": "6385.926",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 892480,
      "gigabytes_processed": "2128.581",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 3686,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 53456
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdae",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569658,
    "asctime": "Thu Jan 18 10:20:58 2024 CET"
  },
  "device": {
    "name": "/dev/sdae",
    "info_name": "/dev/sdae",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c39e419c",
  "serial_number": "VR2U130P",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 46,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 24
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 100
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 663606,
      "gigabytes_processed": "6396.766",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 916096,
      "gigabytes_processed": "2125.573",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 5644,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 51459
}
{
  "json_format_version": [
    1,
    0
  ],
  "smartctl": {
    "version": [
      7,
      3
    ],
    "svn_revision": "5338",
    "platform_info": "x86_64-linux-6.1.0-13-amd64",
    "build_info": "(local build)",
    "argv": [
      "smartctl",
      "-a",
      "-j",
      "/dev/sdaf",
      "-d",
      "scsi"
    ],
    "exit_status": 0
  },
  "local_time": {
    "time_t": 1705569659,
    "asctime": "Thu Jan 18 10:20:59 2024 CET"
  },
  "device": {
    "name": "/dev/sdaf",
    "info_name": "/dev/sdaf",
    "type": "scsi",
    "protocol": "SCSI"
  },
  "scsi_vendor": "HGST",
  "scsi_product": "HUS728T8TAL5204",
  "scsi_model_name": "HGST HUS728T8TAL5204",
  "scsi_revision": "C9G0",
  "scsi_version": "SPC-4",
  "user_capacity": {
    "blocks": 15628053168,
    "bytes": 8001563222016
  },
  "logical_block_size": 512,
  "physical_block_size": 4096,
  "scsi_lb_provisioning": {
    "name": "fully provisioned",
    "value": 0,
    "management_enabled": {
      "name": "LBPME",
      "value": 0
    },
    "read_zeros": {
      "name": "LBPRZ",
      "value": 0
    }
  },
  "rotation_rate": 7200,
  "form_factor": {
    "scsi_value": 2,
    "name": "3.5 inches"
  },
  "logical_unit_id": "0x5000cca0c3a48ce0",
  "serial_number": "VR2XHDHP",
  "device_type": {
    "scsi_terminology": "Peripheral Device Type [PDT]",
    "scsi_value": 0,
    "name": "disk"
  },
  "scsi_transport_protocol": {
    "name": "SAS (SPL-4)",
    "value": 6
  },
  "smart_support": {
    "available": true,
    "enabled": true
  },
  "temperature_warning": {
    "enabled": true
  },
  "smart_status": {
    "passed": true
  },
  "temperature": {
    "current": 45,
    "drive_trip": 85
  },
  "power_on_time": {
    "hours": 3866,
    "minutes": 24
  },
  "scsi_start_stop_cycle_counter": {
    "year_of_manufacture": "2022",
    "week_of_manufacture": "48",
    "specified_cycle_count_over_device_lifetime": 50000,
    "accumulated_start_stop_cycles": 6,
    "specified_load_unload_count_over_device_lifetime": 600000,
    "accumulated_load_unload_cycles": 78
  },
  "scsi_grown_defect_list": 0,
  "scsi_error_counter_log": {
    "read": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 666325,
      "gigabytes_processed": "5796.678",
      "total_uncorrected_errors": 0
    },
    "write": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 588290,
      "gigabytes_processed": "1973.624",
      "total_uncorrected_errors": 0
    },
    "verify": {
      "errors_corrected_by_eccfast": 0,
      "errors_corrected_by_eccdelayed": 0,
      "errors_corrected_by_rereads_rewrites": 0,
      "total_errors_corrected": 0,
      "correction_algorithm_invocations": 1407,
      "gigabytes_processed": "0.001",
      "total_uncorrected_errors": 0
    }
  },
  "scsi_self_test_0": {
    "code": {
      "value": 2,
      "string": "Background long"
    },
    "result": {
      "value": 2,
      "string": "Aborted (device reset ?)"
    },
    "power_on_time": {
      "hours": 3061,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_self_test_1": {
    "code": {
      "value": 1,
      "string": "Background short"
    },
    "result": {
      "value": 0,
      "string": "Completed"
    },
    "power_on_time": {
      "hours": 9,
      "aka": "accumulated_power_on_hours"
    }
  },
  "scsi_extended_self_test_seconds": 52937
}
