
# Dell Force S-Series by SNMP

## Overview

These high performance and low latency Gigabit Ethernet switches deliver the critical functionality that advanced data center network edges demand.

## Requirements

Zabbix version: 7.2 and higher.

## Tested versions

This template has been tested on:
- Dell Force S-Series

## Configuration

> Zabbix should be configured according to the instructions in the [Templates out of the box](https://www.zabbix.com/documentation/7.2/manual/config/templates_out_of_the_box) section.

## Setup

Refer to the vendor documentation.

### Macros used

|Name|Description|Default|
|----|-----------|-------|
|{$CPU.UTIL.CRIT}||`90`|
|{$TEMP_CRIT_LOW}||`5`|
|{$TEMP_CRIT}||`65`|
|{$TEMP_WARN}||`55`|
|{$PSU_CRIT_STATUS}||`2`|
|{$FAN_CRIT_STATUS}||`2`|
|{$PSU_OK_STATUS}||`1`|
|{$FAN_OK_STATUS}||`1`|
|{$MEMORY.UTIL.MAX}||`90`|
|{$SNMP.TIMEOUT}|<p>Time interval for the SNMP availability trigger.</p>|`5m`|
|{$ICMP_LOSS_WARN}|<p>Warning threshold of ICMP packet loss in %.</p>|`20`|
|{$ICMP_RESPONSE_TIME_WARN}|<p>Warning threshold of the average ICMP response time in seconds.</p>|`0.15`|
|{$IF.ERRORS.WARN}|<p>Warning threshold of error packet rate. Can be used with interface name as context.</p>|`2`|
|{$IF.UTIL.MAX}||`90`|
|{$IFCONTROL}||`1`|
|{$NET.IF.IFNAME.MATCHES}||`^.*$`|
|{$NET.IF.IFNAME.NOT_MATCHES}|<p>Filter out loopbacks, nulls, docker veth links and docker0 bridge by default</p>|`Macro too long. Please see the template.`|
|{$NET.IF.IFOPERSTATUS.MATCHES}||`^.*$`|
|{$NET.IF.IFOPERSTATUS.NOT_MATCHES}|<p>Ignore notPresent(6)</p>|`^6$`|
|{$NET.IF.IFADMINSTATUS.MATCHES}||`^.*`|
|{$NET.IF.IFADMINSTATUS.NOT_MATCHES}|<p>Ignore down(2) administrative status</p>|`^2$`|
|{$NET.IF.IFDESCR.MATCHES}||`.*`|
|{$NET.IF.IFDESCR.NOT_MATCHES}||`CHANGE_IF_NEEDED`|
|{$NET.IF.IFALIAS.MATCHES}||`.*`|
|{$NET.IF.IFALIAS.NOT_MATCHES}||`CHANGE_IF_NEEDED`|
|{$NET.IF.IFTYPE.MATCHES}||`.*`|
|{$NET.IF.IFTYPE.NOT_MATCHES}||`CHANGE_IF_NEEDED`|

### Items

|Name|Description|Type|Key and additional info|
|----|-----------|----|-----------------------|
|Uptime (network)|<p>MIB: SNMPv2-MIB</p><p>Time (in hundredths of a second) since the network management portion of the system was last re-initialized.</p>|SNMP agent|system.net.uptime[sysUpTime.0]<p>**Preprocessing**</p><ul><li><p>Custom multiplier: `0.01`</p></li></ul>|
|Uptime (hardware)|<p>MIB: HOST-RESOURCES-MIB</p><p>The amount of time since this host was last initialized. Note that this is different from sysUpTime in the SNMPv2-MIB [RFC1907] because sysUpTime is the uptime of the network management portion of the system.</p>|SNMP agent|system.hw.uptime[hrSystemUptime.0]<p>**Preprocessing**</p><ul><li><p>Check for not supported value: `any error`</p><p>⛔️Custom on fail: Set value to: `0`</p></li><li><p>Custom multiplier: `0.01`</p></li></ul>|
|SNMP traps (fallback)|<p>The item is used to collect all SNMP traps unmatched by other snmptrap items</p>|SNMP trap|snmptrap.fallback|
|System location|<p>MIB: SNMPv2-MIB</p><p>Physical location of the node (e.g., `equipment room`, `3rd floor`). If not provided, the value is a zero-length string.</p>|SNMP agent|system.location[sysLocation.0]<p>**Preprocessing**</p><ul><li><p>Discard unchanged with heartbeat: `12h`</p></li></ul>|
|System contact details|<p>MIB: SNMPv2-MIB</p><p>The textual identification of the contact person for this managed node, together with information on how to contact this person.  If no contact information is known, the value is the zero-length string.</p>|SNMP agent|system.contact[sysContact.0]<p>**Preprocessing**</p><ul><li><p>Discard unchanged with heartbeat: `12h`</p></li></ul>|
|System object ID|<p>MIB: SNMPv2-MIB</p><p>The vendor's authoritative identification of the network management subsystem contained in the entity.  This value is allocated within the SMI enterprises subtree (1.3.6.1.4.1) and provides an easy and unambiguous means for determining`what kind of box' is being managed.  For example, if vendor`Flintstones, Inc.' was assigned the subtree1.3.6.1.4.1.4242, it could assign the identifier 1.3.6.1.4.1.4242.1.1 to its `Fred Router'.</p>|SNMP agent|system.objectid[sysObjectID.0]<p>**Preprocessing**</p><ul><li><p>Discard unchanged with heartbeat: `12h`</p></li></ul>|
|System name|<p>MIB: SNMPv2-MIB</p><p>An administratively-assigned name for this managed node.By convention, this is the node's fully-qualified domain name.  If the name is unknown, the value is the zero-length string.</p>|SNMP agent|system.name<p>**Preprocessing**</p><ul><li><p>Discard unchanged with heartbeat: `12h`</p></li></ul>|
|System description|<p>MIB: SNMPv2-MIB</p><p>A textual description of the entity. This value should</p><p>include the full name and version identification of the system's hardware type, software operating-system, and</p><p>networking software.</p>|SNMP agent|system.descr[sysDescr.0]<p>**Preprocessing**</p><ul><li><p>Discard unchanged with heartbeat: `12h`</p></li></ul>|
|SNMP agent availability|<p>Availability of SNMP checks on the host. The value of this item corresponds to availability icons in the host list.</p><p>Possible values:</p><p>0 - not available</p><p>1 - available</p><p>2 - unknown</p>|Zabbix internal|zabbix[host,snmp,available]|
|ICMP ping||Simple check|icmpping|
|ICMP loss||Simple check|icmppingloss|
|ICMP response time||Simple check|icmppingsec|

### Triggers

|Name|Description|Expression|Severity|Dependencies and additional info|
|----|-----------|----------|--------|--------------------------------|
|Dell Force S-Series: Host has been restarted|<p>Uptime is less than 10 minutes.</p>|`(last(/Dell Force S-Series by SNMP/system.hw.uptime[hrSystemUptime.0])>0 and last(/Dell Force S-Series by SNMP/system.hw.uptime[hrSystemUptime.0])<10m) or (last(/Dell Force S-Series by SNMP/system.hw.uptime[hrSystemUptime.0])=0 and last(/Dell Force S-Series by SNMP/system.net.uptime[sysUpTime.0])<10m)`|Warning|**Manual close**: Yes<br>**Depends on**:<br><ul><li>Dell Force S-Series: No SNMP data collection</li></ul>|
|Dell Force S-Series: System name has changed|<p>The name of the system has changed. Acknowledge to close the problem manually.</p>|`last(/Dell Force S-Series by SNMP/system.name,#1)<>last(/Dell Force S-Series by SNMP/system.name,#2) and length(last(/Dell Force S-Series by SNMP/system.name))>0`|Info|**Manual close**: Yes|
|Dell Force S-Series: No SNMP data collection|<p>SNMP is not available for polling. Please check device connectivity and SNMP settings.</p>|`max(/Dell Force S-Series by SNMP/zabbix[host,snmp,available],{$SNMP.TIMEOUT})=0`|Warning|**Depends on**:<br><ul><li>Dell Force S-Series: Unavailable by ICMP ping</li></ul>|
|Dell Force S-Series: Unavailable by ICMP ping|<p>Last three attempts returned timeout.  Please check device connectivity.</p>|`max(/Dell Force S-Series by SNMP/icmpping,#3)=0`|High||
|Dell Force S-Series: High ICMP ping loss||`min(/Dell Force S-Series by SNMP/icmppingloss,5m)>{$ICMP_LOSS_WARN} and min(/Dell Force S-Series by SNMP/icmppingloss,5m)<100`|Warning|**Depends on**:<br><ul><li>Dell Force S-Series: Unavailable by ICMP ping</li></ul>|
|Dell Force S-Series: High ICMP ping response time|<p>Average ICMP response time is too high.</p>|`avg(/Dell Force S-Series by SNMP/icmppingsec,5m)>{$ICMP_RESPONSE_TIME_WARN}`|Warning|**Depends on**:<br><ul><li>Dell Force S-Series: High ICMP ping loss</li><li>Dell Force S-Series: Unavailable by ICMP ping</li></ul>|

### LLD rule CPU and Memory and Flash Discovery

|Name|Description|Type|Key and additional info|
|----|-----------|----|-----------------------|
|CPU and Memory and Flash Discovery||SNMP agent|module.discovery|

### Item prototypes for CPU and Memory and Flash Discovery

|Name|Description|Type|Key and additional info|
|----|-----------|----|-----------------------|
|#{#SNMPINDEX}: CPU utilization|<p>MIB: F10-S-SERIES-CHASSIS-MIB</p><p>CPU utilization in percentage for last 1 minute.</p>|SNMP agent|system.cpu.util[chStackUnitCpuUtil1Min.{#SNMPINDEX}]|
|#{#SNMPINDEX}: Memory utilization|<p>MIB: F10-S-SERIES-CHASSIS-MIB</p><p>Total memory usage in percentage.</p>|SNMP agent|vm.memory.util[chStackUnitMemUsageUtil.{#SNMPINDEX}]|

### Trigger prototypes for CPU and Memory and Flash Discovery

|Name|Description|Expression|Severity|Dependencies and additional info|
|----|-----------|----------|--------|--------------------------------|
|Dell Force S-Series: #{#SNMPINDEX}: High CPU utilization|<p>The CPU utilization is too high. The system might be slow to respond.</p>|`min(/Dell Force S-Series by SNMP/system.cpu.util[chStackUnitCpuUtil1Min.{#SNMPINDEX}],5m)>{$CPU.UTIL.CRIT}`|Warning||
|Dell Force S-Series: #{#SNMPINDEX}: High memory utilization|<p>The system is running out of free memory.</p>|`min(/Dell Force S-Series by SNMP/vm.memory.util[chStackUnitMemUsageUtil.{#SNMPINDEX}],5m)>{$MEMORY.UTIL.MAX}`|Average||

### LLD rule PSU Discovery

|Name|Description|Type|Key and additional info|
|----|-----------|----|-----------------------|
|PSU Discovery|<p>A list of power supply residents in the S-series chassis.</p>|SNMP agent|psu.discovery|

### Item prototypes for PSU Discovery

|Name|Description|Type|Key and additional info|
|----|-----------|----|-----------------------|
|PSU {#SNMPVALUE}: Power supply status|<p>MIB: F10-S-SERIES-CHASSIS-MIB</p><p>The status of the power supply {#SNMPVALUE}</p>|SNMP agent|sensor.psu.status[chSysPowerSupplyOperStatus.{#SNMPINDEX}]|

### Trigger prototypes for PSU Discovery

|Name|Description|Expression|Severity|Dependencies and additional info|
|----|-----------|----------|--------|--------------------------------|
|Dell Force S-Series: PSU {#SNMPVALUE}: Power supply is in critical state|<p>Please check the power supply unit for errors</p>|`count(/Dell Force S-Series by SNMP/sensor.psu.status[chSysPowerSupplyOperStatus.{#SNMPINDEX}],#1,"eq","{$PSU_CRIT_STATUS}")=1`|Average||
|Dell Force S-Series: PSU {#SNMPVALUE}: Power supply is not in normal state|<p>Please check the power supply unit for errors</p>|`count(/Dell Force S-Series by SNMP/sensor.psu.status[chSysPowerSupplyOperStatus.{#SNMPINDEX}],#1,"ne","{$PSU_OK_STATUS}")=1`|Info|**Depends on**:<br><ul><li>Dell Force S-Series: PSU {#SNMPVALUE}: Power supply is in critical state</li></ul>|

### LLD rule FAN Discovery

|Name|Description|Type|Key and additional info|
|----|-----------|----|-----------------------|
|FAN Discovery||SNMP agent|fan.discovery|

### Item prototypes for FAN Discovery

|Name|Description|Type|Key and additional info|
|----|-----------|----|-----------------------|
|Fan {#SNMPVALUE}: Fan status|<p>MIB: F10-S-SERIES-CHASSIS-MIB</p><p>The status of the fan tray {#SNMPVALUE}.</p>|SNMP agent|sensor.fan.status[chSysFanTrayOperStatus.{#SNMPINDEX}]|

### Trigger prototypes for FAN Discovery

|Name|Description|Expression|Severity|Dependencies and additional info|
|----|-----------|----------|--------|--------------------------------|
|Dell Force S-Series: Fan {#SNMPVALUE}: Fan is in critical state|<p>Please check the fan unit</p>|`count(/Dell Force S-Series by SNMP/sensor.fan.status[chSysFanTrayOperStatus.{#SNMPINDEX}],#1,"eq","{$FAN_CRIT_STATUS}")=1`|Average||
|Dell Force S-Series: Fan {#SNMPVALUE}: Fan is not in normal state|<p>Please check the fan unit</p>|`count(/Dell Force S-Series by SNMP/sensor.fan.status[chSysFanTrayOperStatus.{#SNMPINDEX}],#1,"ne","{$FAN_OK_STATUS}")=1`|Info|**Depends on**:<br><ul><li>Dell Force S-Series: Fan {#SNMPVALUE}: Fan is in critical state</li></ul>|

### LLD rule Stack Unit Discovery

|Name|Description|Type|Key and additional info|
|----|-----------|----|-----------------------|
|Stack Unit Discovery||SNMP agent|stack.discovery|

### Item prototypes for Stack Unit Discovery

|Name|Description|Type|Key and additional info|
|----|-----------|----|-----------------------|
|Device {#SNMPVALUE}: Temperature|<p>MIB: F10-S-SERIES-CHASSIS-MIB</p><p>The temperature of the unit.</p>|SNMP agent|sensor.temp.value[chStackUnitTemp.{#SNMPINDEX}]|
|#{#SNMPVALUE}: Hardware model name|<p>MIB: F10-S-SERIES-CHASSIS-MIB</p><p>The plugged-in model ID for this unit.</p>|SNMP agent|system.hw.model[chStackUnitModelID.{#SNMPINDEX}]<p>**Preprocessing**</p><ul><li><p>Discard unchanged with heartbeat: `1d`</p></li></ul>|
|#{#SNMPVALUE}: Hardware serial number|<p>MIB: F10-S-SERIES-CHASSIS-MIB</p><p>The unit's serial number.</p>|SNMP agent|system.hw.serialnumber[chStackUnitSerialNumber.{#SNMPINDEX}]<p>**Preprocessing**</p><ul><li><p>Discard unchanged with heartbeat: `1d`</p></li></ul>|
|#{#SNMPVALUE}: Hardware version(revision)|<p>MIB: F10-S-SERIES-CHASSIS-MIB</p><p>The unit manufacturer's product revision</p>|SNMP agent|system.hw.version[chStackUnitProductRev.{#SNMPINDEX}]<p>**Preprocessing**</p><ul><li><p>Discard unchanged with heartbeat: `1d`</p></li></ul>|
|#{#SNMPVALUE}: Operating system|<p>MIB: F10-S-SERIES-CHASSIS-MIB</p><p>Current code version of this unit.</p>|SNMP agent|system.sw.os[chStackUnitCodeVersion.{#SNMPINDEX}]<p>**Preprocessing**</p><ul><li><p>Discard unchanged with heartbeat: `1d`</p></li></ul>|

### Trigger prototypes for Stack Unit Discovery

|Name|Description|Expression|Severity|Dependencies and additional info|
|----|-----------|----------|--------|--------------------------------|
|Dell Force S-Series: Device {#SNMPVALUE}: Temperature is above warning threshold|<p>This trigger uses temperature sensor values as well as temperature sensor status if available</p>|`avg(/Dell Force S-Series by SNMP/sensor.temp.value[chStackUnitTemp.{#SNMPINDEX}],5m)>{$TEMP_WARN:"{#SNMPVALUE}"}`|Warning|**Depends on**:<br><ul><li>Dell Force S-Series: Device {#SNMPVALUE}: Temperature is above critical threshold</li></ul>|
|Dell Force S-Series: Device {#SNMPVALUE}: Temperature is above critical threshold|<p>This trigger uses temperature sensor values as well as temperature sensor status if available</p>|`avg(/Dell Force S-Series by SNMP/sensor.temp.value[chStackUnitTemp.{#SNMPINDEX}],5m)>{$TEMP_CRIT:"{#SNMPVALUE}"}`|High||
|Dell Force S-Series: Device {#SNMPVALUE}: Temperature is too low||`avg(/Dell Force S-Series by SNMP/sensor.temp.value[chStackUnitTemp.{#SNMPINDEX}],5m)<{$TEMP_CRIT_LOW:"{#SNMPVALUE}"}`|Average||
|Dell Force S-Series: #{#SNMPVALUE}: Device has been replaced|<p>Device serial number has changed. Acknowledge to close the problem manually.</p>|`last(/Dell Force S-Series by SNMP/system.hw.serialnumber[chStackUnitSerialNumber.{#SNMPINDEX}],#1)<>last(/Dell Force S-Series by SNMP/system.hw.serialnumber[chStackUnitSerialNumber.{#SNMPINDEX}],#2) and length(last(/Dell Force S-Series by SNMP/system.hw.serialnumber[chStackUnitSerialNumber.{#SNMPINDEX}]))>0`|Info|**Manual close**: Yes|
|Dell Force S-Series: #{#SNMPVALUE}: Operating system description has changed|<p>The description of the operating system has changed. Possible reasons are that the system has been updated or replaced. Acknowledge to close the problem manually.</p>|`last(/Dell Force S-Series by SNMP/system.sw.os[chStackUnitCodeVersion.{#SNMPINDEX}],#1)<>last(/Dell Force S-Series by SNMP/system.sw.os[chStackUnitCodeVersion.{#SNMPINDEX}],#2) and length(last(/Dell Force S-Series by SNMP/system.sw.os[chStackUnitCodeVersion.{#SNMPINDEX}]))>0`|Info|**Manual close**: Yes<br>**Depends on**:<br><ul><li>Dell Force S-Series: System name has changed</li></ul>|

### LLD rule Network interfaces discovery

|Name|Description|Type|Key and additional info|
|----|-----------|----|-----------------------|
|Network interfaces discovery|<p>Discovering interfaces from IF-MIB.</p>|SNMP agent|net.if.discovery|

### Item prototypes for Network interfaces discovery

|Name|Description|Type|Key and additional info|
|----|-----------|----|-----------------------|
|Interface {#IFNAME}({#IFALIAS}): Operational status|<p>MIB: IF-MIB</p><p>The current operational state of the interface.</p><p>- The testing(3) state indicates that no operational packet scan be passed</p><p>- If ifAdminStatus is down(2) then ifOperStatus should be down(2)</p><p>- If ifAdminStatus is changed to up(1) then ifOperStatus should change to up(1) if the interface is ready to transmit and receive network traffic</p><p>- It should change todormant(5) if the interface is waiting for external actions (such as a serial line waiting for an incoming connection)</p><p>- It should remain in the down(2) state if and only if there is a fault that prevents it from going to the up(1) state</p><p>- It should remain in the notPresent(6) state if the interface has missing(typically, hardware) components.</p>|SNMP agent|net.if.status[ifOperStatus.{#SNMPINDEX}]|
|Interface {#IFNAME}({#IFALIAS}): Bits received|<p>MIB: IF-MIB</p><p>The total number of octets received on the interface, including framing characters. This object is a 64-bit version of ifInOctets. Discontinuities in the value of this counter can occur at re-initialization of the management system, and at other times as indicated by the value of ifCounterDiscontinuityTime.</p>|SNMP agent|net.if.in[ifHCInOctets.{#SNMPINDEX}]<p>**Preprocessing**</p><ul><li>Change per second</li><li><p>Custom multiplier: `8`</p></li></ul>|
|Interface {#IFNAME}({#IFALIAS}): Bits sent|<p>MIB: IF-MIB</p><p>The total number of octets transmitted out of the interface, including framing characters. This object is a 64-bit version of ifOutOctets.Discontinuities in the value of this counter can occur at re-initialization of the management system, and at other times as indicated by the value of ifCounterDiscontinuityTime.</p>|SNMP agent|net.if.out[ifHCOutOctets.{#SNMPINDEX}]<p>**Preprocessing**</p><ul><li>Change per second</li><li><p>Custom multiplier: `8`</p></li></ul>|
|Interface {#IFNAME}({#IFALIAS}): Inbound packets with errors|<p>MIB: IF-MIB</p><p>For packet-oriented interfaces, the number of inbound packets that contained errors preventing them from being deliverable to a higher-layer protocol.  For character-oriented or fixed-length interfaces, the number of inbound transmission units that contained errors preventing them from being deliverable to a higher-layer protocol. Discontinuities in the value of this counter can occur at re-initialization of the management system, and at other times as indicated by the value of ifCounterDiscontinuityTime.</p>|SNMP agent|net.if.in.errors[ifInErrors.{#SNMPINDEX}]<p>**Preprocessing**</p><ul><li>Change per second</li></ul>|
|Interface {#IFNAME}({#IFALIAS}): Outbound packets with errors|<p>MIB: IF-MIB</p><p>For packet-oriented interfaces, the number of outbound packets that contained errors preventing them from being deliverable to a higher-layer protocol.  For character-oriented or fixed-length interfaces, the number of outbound transmission units that contained errors preventing them from being deliverable to a higher-layer protocol. Discontinuities in the value of this counter can occur at re-initialization of the management system, and at other times as indicated by the value of ifCounterDiscontinuityTime.</p>|SNMP agent|net.if.out.errors[ifOutErrors.{#SNMPINDEX}]<p>**Preprocessing**</p><ul><li>Change per second</li></ul>|
|Interface {#IFNAME}({#IFALIAS}): Outbound packets discarded|<p>MIB: IF-MIB</p><p>The number of outbound packets which were chosen to be discarded</p><p>even though no errors had been detected to prevent their being deliverable to a higher-layer protocol.</p><p>One possible reason for discarding such a packet could be to free up buffer space.</p><p>Discontinuities in the value of this counter can occur at re-initialization of the management system,</p><p>and at other times as indicated by the value of ifCounterDiscontinuityTime.</p>|SNMP agent|net.if.out.discards[ifOutDiscards.{#SNMPINDEX}]<p>**Preprocessing**</p><ul><li>Change per second</li></ul>|
|Interface {#IFNAME}({#IFALIAS}): Inbound packets discarded|<p>MIB: IF-MIB</p><p>The number of inbound packets which were chosen to be discarded</p><p>even though no errors had been detected to prevent their being deliverable to a higher-layer protocol.</p><p>One possible reason for discarding such a packet could be to free up buffer space.</p><p>Discontinuities in the value of this counter can occur at re-initialization of the management system,</p><p>and at other times as indicated by the value of ifCounterDiscontinuityTime.</p>|SNMP agent|net.if.in.discards[ifInDiscards.{#SNMPINDEX}]<p>**Preprocessing**</p><ul><li>Change per second</li></ul>|
|Interface {#IFNAME}({#IFALIAS}): Interface type|<p>MIB: IF-MIB</p><p>The type of interface.</p><p>Additional values for ifType are assigned by the Internet Assigned Numbers Authority (IANA),</p><p>through updating the syntax of the IANAifType textual convention.</p>|SNMP agent|net.if.type[ifType.{#SNMPINDEX}]<p>**Preprocessing**</p><ul><li><p>Discard unchanged with heartbeat: `1d`</p></li></ul>|
|Interface {#IFNAME}({#IFALIAS}): Speed|<p>MIB: IF-MIB</p><p>An estimate of the interface's current bandwidth in units of 1,000,000 bits per second. If this object reports a value of `n' then the speed of the interface is somewhere in the range of `n-500,000' to`n+499,999'.  For interfaces which do not vary in bandwidth or for those where no accurate estimation can be made, this object should contain the nominal bandwidth. For a sub-layer which has no concept of bandwidth, this object should be zero.</p>|SNMP agent|net.if.speed[ifHighSpeed.{#SNMPINDEX}]<p>**Preprocessing**</p><ul><li><p>Custom multiplier: `1000000`</p></li><li><p>Discard unchanged with heartbeat: `1h`</p></li></ul>|

### Trigger prototypes for Network interfaces discovery

|Name|Description|Expression|Severity|Dependencies and additional info|
|----|-----------|----------|--------|--------------------------------|
|Dell Force S-Series: Interface {#IFNAME}({#IFALIAS}): Link down|<p>This trigger expression works as follows:<br>1. It can be triggered if the operations status is down.<br>2. `{$IFCONTROL:"{#IFNAME}"}=1` - a user can redefine the context macro to "0", marking this interface as not important. No new trigger will be fired if this interface is down.<br>3. `{TEMPLATE_NAME:METRIC.diff()}=1` - the trigger fires only if the operational status was up to (1) sometime before (so, does not fire for "eternal off" interfaces.)<br><br>WARNING: if closed manually - it will not fire again on the next poll, because of .diff.</p>|`{$IFCONTROL:"{#IFNAME}"}=1 and last(/Dell Force S-Series by SNMP/net.if.status[ifOperStatus.{#SNMPINDEX}])=2 and (last(/Dell Force S-Series by SNMP/net.if.status[ifOperStatus.{#SNMPINDEX}],#1)<>last(/Dell Force S-Series by SNMP/net.if.status[ifOperStatus.{#SNMPINDEX}],#2))`|Average|**Manual close**: Yes|
|Dell Force S-Series: Interface {#IFNAME}({#IFALIAS}): High bandwidth usage|<p>The utilization of the network interface is close to its estimated maximum bandwidth.</p>|`(avg(/Dell Force S-Series by SNMP/net.if.in[ifHCInOctets.{#SNMPINDEX}],15m)>({$IF.UTIL.MAX:"{#IFNAME}"}/100)*last(/Dell Force S-Series by SNMP/net.if.speed[ifHighSpeed.{#SNMPINDEX}]) or avg(/Dell Force S-Series by SNMP/net.if.out[ifHCOutOctets.{#SNMPINDEX}],15m)>({$IF.UTIL.MAX:"{#IFNAME}"}/100)*last(/Dell Force S-Series by SNMP/net.if.speed[ifHighSpeed.{#SNMPINDEX}])) and last(/Dell Force S-Series by SNMP/net.if.speed[ifHighSpeed.{#SNMPINDEX}])>0`|Warning|**Manual close**: Yes<br>**Depends on**:<br><ul><li>Dell Force S-Series: Interface {#IFNAME}({#IFALIAS}): Link down</li></ul>|
|Dell Force S-Series: Interface {#IFNAME}({#IFALIAS}): High error rate|<p>It recovers when it is below 80% of the `{$IF.ERRORS.WARN:"{#IFNAME}"}` threshold.</p>|`min(/Dell Force S-Series by SNMP/net.if.in.errors[ifInErrors.{#SNMPINDEX}],5m)>{$IF.ERRORS.WARN:"{#IFNAME}"} or min(/Dell Force S-Series by SNMP/net.if.out.errors[ifOutErrors.{#SNMPINDEX}],5m)>{$IF.ERRORS.WARN:"{#IFNAME}"}`|Warning|**Manual close**: Yes<br>**Depends on**:<br><ul><li>Dell Force S-Series: Interface {#IFNAME}({#IFALIAS}): Link down</li></ul>|
|Dell Force S-Series: Interface {#IFNAME}({#IFALIAS}): Ethernet has changed to lower speed than it was before|<p>This Ethernet connection has transitioned down from its known maximum speed. This might be a sign of autonegotiation issues. Acknowledge to close the problem manually.</p>|`change(/Dell Force S-Series by SNMP/net.if.speed[ifHighSpeed.{#SNMPINDEX}])<0 and last(/Dell Force S-Series by SNMP/net.if.speed[ifHighSpeed.{#SNMPINDEX}])>0 and ( last(/Dell Force S-Series by SNMP/net.if.type[ifType.{#SNMPINDEX}])=6 or last(/Dell Force S-Series by SNMP/net.if.type[ifType.{#SNMPINDEX}])=7 or last(/Dell Force S-Series by SNMP/net.if.type[ifType.{#SNMPINDEX}])=11 or last(/Dell Force S-Series by SNMP/net.if.type[ifType.{#SNMPINDEX}])=62 or last(/Dell Force S-Series by SNMP/net.if.type[ifType.{#SNMPINDEX}])=69 or last(/Dell Force S-Series by SNMP/net.if.type[ifType.{#SNMPINDEX}])=117 ) and (last(/Dell Force S-Series by SNMP/net.if.status[ifOperStatus.{#SNMPINDEX}])<>2)`|Info|**Manual close**: Yes<br>**Depends on**:<br><ul><li>Dell Force S-Series: Interface {#IFNAME}({#IFALIAS}): Link down</li></ul>|

### LLD rule EtherLike-MIB Discovery

|Name|Description|Type|Key and additional info|
|----|-----------|----|-----------------------|
|EtherLike-MIB Discovery|<p>Discovering interfaces from IF-MIB and EtherLike-MIB. Interfaces with up(1) Operational Status are discovered.</p>|SNMP agent|net.if.duplex.discovery<p>**Preprocessing**</p><ul><li><p>JavaScript: `The text is too long. Please see the template.`</p></li></ul>|

### Item prototypes for EtherLike-MIB Discovery

|Name|Description|Type|Key and additional info|
|----|-----------|----|-----------------------|
|Interface {#IFNAME}({#IFALIAS}): Duplex status|<p>MIB: EtherLike-MIB</p><p>The current mode of operation of the MAC</p><p>entity.  'unknown' indicates that the current</p><p>duplex mode could not be determined.</p><p></p><p>Management control of the duplex mode is</p><p>accomplished through the MAU MIB.  When</p><p>an interface does not support autonegotiation,</p><p>or when autonegotiation is not enabled, the</p><p>duplex mode is controlled using</p><p>ifMauDefaultType.  When autonegotiation is</p><p>supported and enabled, duplex mode is controlled</p><p>using ifMauAutoNegAdvertisedBits.  In either</p><p>case, the currently operating duplex mode is</p><p>reflected both in this object and in ifMauType.</p><p></p><p>Note that this object provides redundant</p><p>information with ifMauType.  Normally, redundant</p><p>objects are discouraged.  However, in this</p><p>instance, it allows a management application to</p><p>determine the duplex status of an interface</p><p>without having to know every possible value of</p><p>ifMauType.  This was felt to be sufficiently</p><p>valuable to justify the redundancy.</p><p>Reference: [IEEE 802.3 Std.], 30.3.1.1.32,aDuplexStatus.</p>|SNMP agent|net.if.duplex[dot3StatsDuplexStatus.{#SNMPINDEX}]|

### Trigger prototypes for EtherLike-MIB Discovery

|Name|Description|Expression|Severity|Dependencies and additional info|
|----|-----------|----------|--------|--------------------------------|
|Dell Force S-Series: Interface {#IFNAME}({#IFALIAS}): In half-duplex mode|<p>Please check autonegotiation settings and cabling.</p>|`last(/Dell Force S-Series by SNMP/net.if.duplex[dot3StatsDuplexStatus.{#SNMPINDEX}])=2`|Warning|**Manual close**: Yes|

## Feedback

Please report any issues with the template at [`https://support.zabbix.com`](https://support.zabbix.com)

You can also provide feedback, discuss the template, or ask for help at [`ZABBIX forums`](https://www.zabbix.com/forum/zabbix-suggestions-and-feedback)

