com.qualcomm.robotcore.hardware

## Interface AnalogSensor

-     public interface AnalogSensor

  Instances of this interface are sensors whose input is reported as a voltage level to an analog to digital converter.

- - ### Method Summary

    All Methods Instance Methods Abstract Methods
    Modifier and Type | Method and Description
    --- | ---
    `double` | `readRawVoltage()` Returns the sensor's current value as a raw voltage level.

- - ### Method Detail

    - #### readRawVoltage

          double readRawVoltage()

      Returns the sensor's current value as a raw voltage level. Note that for Returns the light level voltage as reported by the sensor. Note that returned values INCREASE as the light energy INCREASES.
      Returns:
        unscaled / unclipped voltage level reported by the device