:orphan:

=======================================================
 ceph-volume -- Ceph OSD deployment and inspection tool
=======================================================

.. program:: ceph-volume

Synopsis
========

**ceph-volume** [-h] [--cluster CLUSTER] [--log-level LOG_LEVEL]
[--log-path LOG_PATH]

**ceph-volume** **inventory**

**ceph-volume** **lvm** [ *trigger* | *create* | *activate* | *prepare*
| *zap* | *list* | *batch* | *new-wal* | *new-db* | *migrate* ]

**ceph-volume** **simple** [ *trigger* | *scan* | *activate* ]


Description
===========

:program:`ceph-volume` is a single purpose command line tool to deploy logical
volumes as OSDs, trying to maintain a similar API to ``ceph-disk`` when
preparing, activating, and creating OSDs.

It deviates from ``ceph-disk`` by not interacting or relying on the udev rules
that come installed for Ceph. These rules allow automatic detection of
previously setup devices that are in turn fed into ``ceph-disk`` to activate
them.


Commands
========

inventory
---------

.. program:: ceph-volume inventory

This subcommand provides information about a host's physical disc inventory and
reports metadata about these discs. Among this metadata one can find disc
specific data items (like model, size, rotational or solid state) as well as
data items specific to ceph using a device, such as if it is available for
use with ceph or if logical volumes are present.

Examples::

    ceph-volume inventory
    ceph-volume inventory /dev/sda
    ceph-volume inventory --format json-pretty

Optional arguments:

.. option:: -h, --help

   show the help message and exit

.. option:: --format

   report format, valid values are ``plain`` (default),
   ``json`` and ``json-pretty``

lvm
---

.. program:: ceph-volume lvm

By making use of LVM tags, the ``lvm`` sub-command is able to store and later
re-discover and query devices associated with OSDs so that they can later
activated.

Subcommands:

batch
^^^^^

.. program:: ceph-volume lvm batch

Creates OSDs from a list of devices using a ``filestore``
or ``bluestore`` (default) setup. It will create all necessary volume groups
and logical volumes required to have a working OSD.

Example usage with three devices::

    ceph-volume lvm batch --bluestore /dev/sda /dev/sdb /dev/sdc

Optional arguments:

.. option:: -h, --help

   show the help message and exit

.. option:: --bluestore

   Use the bluestore objectstore (default)

.. option:: --filestore

   Use the filestore objectstore

.. option:: --yes

   Skip the report and prompt to continue provisioning

.. option:: --prepare

   Only prepare OSDs, do not activate

.. option:: --dmcrypt

   Enable encryption for the underlying OSD devices

.. option:: --crush-device-class

   Define a CRUSH device class to assign the OSD to

.. option:: --no-systemd

   Do not enable or create any systemd units

.. option:: --osds-per-device

   Provision more than 1 (the default) OSD per device

.. option:: --report

   Report what the potential outcome would be for the current input (requires devices
   to be passed in)

.. option:: --format

   Output format when reporting (used along with --report), can be one of 'pretty'
   (default) or 'json'

.. option:: --block-db-size

   Set (or override) the "bluestore_block_db_size" value, in bytes

.. option:: --journal-size

   Override the "osd_journal_size" value, in megabytes

Required positional arguments:

.. describe:: <DEVICE>

   Full path to a raw device, like ``/dev/sda``. Multiple
   ``<DEVICE>`` paths can be passed in.

activate
^^^^^^^^

.. program:: ceph-volume lvm activate

Enables a systemd unit that persists the OSD ID and its UUID (also called
``fsid`` in Ceph CLI tools), so that at boot time it can understand what OSD is
enabled and needs to be mounted.

Usage::

    ceph-volume lvm activate --bluestore <osd id> <osd fsid>

Optional Arguments:

.. option:: -h, --help

   show the help message and exit

.. option:: --auto-detect-objectstore

   Automatically detect the objectstore by inspecting
   the OSD

.. option:: --bluestore

   bluestore objectstore (default)

.. option:: --filestore

   filestore objectstore

.. option:: --all

   Activate all OSDs found in the system

.. option:: --no-systemd

   Skip creating and enabling systemd units and starting of OSD
   services

Multiple OSDs can be activated at once by using the (idempotent) ``--all`` flag::

    ceph-volume lvm activate --all


prepare
^^^^^^^

.. program:: ceph-volume lvm prepare

Prepares a logical volume to be used as an OSD and journal using a ``filestore``
or ``bluestore`` (default) setup. It will not create or modify the logical volumes
except for adding extra metadata.

Usage::

    ceph-volume lvm prepare --filestore --data <data lv> --journal <journal device>

Optional arguments:

.. option:: -h, --help

   show the help message and exit

.. option:: --journal JOURNAL

   logical group name, path to a logical volume, or path to a device

.. option:: --bluestore

   Use the bluestore objectstore (default)

.. option:: --block.wal

   Path to a bluestore block.wal logical volume or partition

.. option:: --block.db

   Path to a bluestore block.db logical volume or partition

.. option:: --filestore

   Use the filestore objectstore

.. option:: --dmcrypt

   Enable encryption for the underlying OSD devices

.. option:: --osd-id OSD_ID

   Reuse an existing OSD id

.. option:: --osd-fsid OSD_FSID

   Reuse an existing OSD fsid

.. option:: --crush-device-class

   Define a CRUSH device class to assign the OSD to

Required arguments:

.. option:: --data

   A logical group name or a path to a logical volume

For encrypting an OSD, the ``--dmcrypt`` flag must be added when preparing
(also supported in the ``create`` sub-command).


create
^^^^^^

Wraps the two-step process to provision a new osd (calling ``prepare`` first
and then ``activate``) into a single one. The reason to prefer ``prepare`` and
then ``activate`` is to gradually introduce new OSDs into a cluster, and
avoiding large amounts of data being rebalanced.

The single-call process unifies exactly what ``prepare`` and ``activate`` do,
with the convenience of doing it all at once. Flags and general usage are
equivalent to those of the ``prepare`` and ``activate`` subcommand.

trigger
^^^^^^^

This subcommand is not meant to be used directly, and it is used by systemd so
that it proxies input to ``ceph-volume lvm activate`` by parsing the
input from systemd, detecting the UUID and ID associated with an OSD.

Usage::

    ceph-volume lvm trigger <SYSTEMD-DATA>

The systemd "data" is expected to be in the format of::

    <OSD ID>-<OSD UUID>

The lvs associated with the OSD need to have been prepared previously,
so that all needed tags and metadata exist.

Positional arguments:

.. describe:: <SYSTEMD_DATA>

   Data from a systemd unit containing ID and UUID of the OSD.

list
^^^^

List devices or logical volumes associated with Ceph. An association is
determined if a device has information relating to an OSD. This is
verified by querying LVM's metadata and correlating it with devices.

The lvs associated with the OSD need to have been prepared previously by
ceph-volume so that all needed tags and metadata exist.

Usage::

    ceph-volume lvm list

List a particular device, reporting all metadata about it::

    ceph-volume lvm list /dev/sda1

List a logical volume, along with all its metadata (vg is a volume
group, and lv the logical volume name)::

    ceph-volume lvm list {vg/lv}

Positional arguments:

.. describe:: <DEVICE>

   Either in the form of ``vg/lv`` for logical volumes,
   ``/path/to/sda1`` or ``/path/to/sda`` for regular devices.


zap
^^^

Zaps the given logical volume or partition. If given a path to a logical
volume it must be in the format of vg/lv. Any file systems present
on the given lv or partition will be removed and all data will be purged.

However, the lv or partition will be kept intact.

Usage, for logical volumes::

      ceph-volume lvm zap {vg/lv}

Usage, for logical partitions::

      ceph-volume lvm zap /dev/sdc1

For full removal of the device use the ``--destroy`` flag (allowed for all
device types)::

      ceph-volume lvm zap --destroy /dev/sdc1

Multiple devices can be removed by specifying the OSD ID and/or the OSD FSID::

      ceph-volume lvm zap --destroy --osd-id 1
      ceph-volume lvm zap --destroy --osd-id 1 --osd-fsid C9605912-8395-4D76-AFC0-7DFDAC315D59


Positional arguments:

.. describe:: <DEVICE>

   Either in the form of ``vg/lv`` for logical volumes,
   ``/path/to/sda1`` or ``/path/to/sda`` for regular devices.


new-wal
^^^^^^^

.. program:: ceph-volume lvm new-wal

Attaches the given logical volume to OSD as a WAL. Logical volume
name format is vg/lv. Fails if OSD has already got attached WAL.

Usage::

    ceph-volume lvm new-wal --osd-id OSD_ID --osd-fsid OSD_FSID --target <target lv>

Optional arguments:

.. option:: -h, --help

   show the help message and exit

.. option:: --no-systemd

   Skip checking OSD systemd unit

Required arguments:

.. option:: --target

   logical volume name to attach as WAL

new-db
^^^^^^

.. program:: ceph-volume lvm new-db

Attaches the given logical volume to OSD as a DB. Logical volume
name format is vg/lv. Fails if OSD has already got attached DB.

Usage::

    ceph-volume lvm new-db --osd-id OSD_ID --osd-fsid OSD_FSID --target <target lv>

Optional arguments:

.. option:: -h, --help

   show the help message and exit

.. option:: --no-systemd

   Skip checking OSD systemd unit

Required arguments:

.. option:: --target

   logical volume name to attach as DB

migrate
^^^^^^^

.. program:: ceph-volume lvm migrate

Moves BlueFS data from source volume(s) to the target one, source volumes
(except the main, i.e. data or block one) are removed on success. LVM volumes
are permitted for Target only, both already attached or new one. In the latter
case it is attached to the OSD replacing one of the source devices. Following
replacement rules apply (in the order of precedence, stop on the first match):

    - if source list has DB volume - target device replaces it.
    - if source list has WAL volume - target device replace it.
    - if source list has slow volume only - operation is not permitted,
      requires explicit allocation via new-db/new-wal command.

Usage::

    ceph-volume lvm migrate --osd-id OSD_ID --osd-fsid OSD_FSID --target <target lv> --from {data|db|wal} [{data|db|wal} ...]

Optional arguments:

.. option:: -h, --help

   show the help message and exit

.. option:: --no-systemd

   Skip checking OSD systemd unit

Required arguments:

.. option:: --from

   list of source device type names

.. option:: --target

   logical volume to move data to

simple
------

Scan legacy OSD directories or data devices that may have been created by
ceph-disk, or manually.

Subcommands:

activate
^^^^^^^^

.. program:: ceph-volume simple activate

Enables a systemd unit that persists the OSD ID and its UUID (also called
``fsid`` in Ceph CLI tools), so that at boot time it can understand what OSD is
enabled and needs to be mounted, while reading information that was previously
created and persisted at ``/etc/ceph/osd/`` in JSON format.

Usage::

    ceph-volume simple activate --bluestore <osd id> <osd fsid>

Optional Arguments:

.. option:: -h, --help

   show the help message and exit

.. option:: --bluestore

   bluestore objectstore (default)

.. option:: --filestore

   filestore objectstore

.. note::

   It requires a matching JSON file with the following format::

    /etc/ceph/osd/<osd id>-<osd fsid>.json


scan
^^^^

.. program:: ceph-volume simple scan

Scan a running OSD or data device for an OSD for metadata that can later be
used to activate and manage the OSD with ceph-volume. The scan method will
create a JSON file with the required information plus anything found in the OSD
directory as well.

Optionally, the JSON blob can be sent to stdout for further inspection.

Usage on all running OSDs::

    ceph-volume simple scan

Usage on data devices::

    ceph-volume simple scan <data device>

Running OSD directories::

    ceph-volume simple scan <path to osd dir>


Optional arguments:

.. option:: -h, --help

   show the help message and exit

.. option:: --stdout

   Send the JSON blob to stdout

.. option:: --force

   If the JSON file exists at destination, overwrite it

Optional Positional arguments:

.. describe:: <DATA DEVICE or OSD DIR>

   Actual data partition or a path to the running OSD

trigger
^^^^^^^

This subcommand is not meant to be used directly, and it is used by systemd so
that it proxies input to ``ceph-volume simple activate`` by parsing the
input from systemd, detecting the UUID and ID associated with an OSD.

Usage::

    ceph-volume simple trigger <SYSTEMD-DATA>

The systemd "data" is expected to be in the format of::

    <OSD ID>-<OSD UUID>

The JSON file associated with the OSD need to have been persisted previously by
a scan (or manually), so that all needed metadata can be used.

Positional arguments:

.. describe:: <SYSTEMD_DATA>

   Data from a systemd unit containing ID and UUID of the OSD.


Availability
============

:program:`ceph-volume` is part of Ceph, a massively scalable, open-source, distributed storage system. Please refer to
the documentation at http://docs.ceph.com/ for more information.


See also
========

:doc:`ceph-osd <ceph-osd>`\(8),
