..  SPDX-License-Identifier: BSD-3-Clause
    Copyright 2017 The DPDK contributors

DPDK Release 17.02
==================

.. **Read this first.**

   The text below explains how to update the release notes.

   Use proper spelling, capitalization and punctuation in all sections.

   Variable and config names should be quoted as fixed width text: ``LIKE_THIS``.

   Build the docs and view the output file to ensure the changes are correct::

      make doc-guides-html

      firefox build/doc/html/guides/rel_notes/release_17_02.html


New Features
------------

.. This section should contain new features added in this release. Sample format:

   * **Add a title in the past tense with a full stop.**

     Add a short 1-2 sentence description in the past tense. The description
     should be enough to allow someone scanning the release notes to understand
     the new feature.

     If the feature adds a lot of sub-features you can use a bullet list like this.

     * Added feature foo to do something.
     * Enhanced feature bar to do something else.

     Refer to the previous release notes for examples.

     This section is a comment. do not overwrite or remove it.
     Also, make sure to start the actual text at the margin.
     =========================================================

* **Added support for representing buses in EAL**

  The ``rte_bus`` structure was introduced into the EAL. This allows for
  devices to be represented by buses they are connected to. A new bus can be
  added to DPDK by extending the ``rte_bus`` structure and implementing the
  scan and probe functions. Once a new bus is registered using the provided
  APIs, new devices can be detected and initialized using bus scan and probe
  callbacks.

  With this change, devices other than PCI or VDEV type can be represented
  in the DPDK framework.

* **Added generic EAL API for I/O device memory read/write operations.**

  This API introduces 8 bit, 16 bit, 32 bit and 64 bit I/O device
  memory read/write operations along with "relaxed" versions.

  Weakly-ordered architectures like ARM need an additional I/O barrier for
  device memory read/write access over PCI bus. By introducing the EAL
  abstraction for I/O device memory read/write access, the drivers can access
  I/O device memory in an architecture-agnostic manner. The relaxed version
  does not have an additional I/O memory barrier, which is useful in accessing
  the device registers of integrated controllers which is implicitly strongly
  ordered with respect to memory access.

* **Added generic flow API (rte_flow).**

  This API provides a generic means to configure hardware to match specific
  ingress or egress traffic, alter its behavior and query related counters
  according to any number of user-defined rules.

  In order to expose a single interface with an unambiguous behavior that is
  common to all poll-mode drivers (PMDs) the ``rte_flow`` API is slightly
  higher-level than the legacy filtering framework, which it encompasses and
  supersedes (including all functions and filter types) .

  See the :doc:`../prog_guide/rte_flow` documentation for more information.

* **Added firmware version get API.**

  Added a new function ``rte_eth_dev_fw_version_get()`` to fetch the firmware
  version for a given device.

* **Added APIs for MACsec offload support to the ixgbe PMD.**

  Six new APIs have been added to the ixgbe PMD for MACsec offload support.
  The declarations for the APIs can be found in ``rte_pmd_ixgbe.h``.

* **Added I219 NICs support.**

  Added support for I219 Intel 1GbE NICs.

* **Added VF Daemon (VFD) for i40e. - EXPERIMENTAL**

  This is an EXPERIMENTAL feature to enhance the capability of the DPDK PF as
  many VF management features are not currently supported by the kernel PF
  driver. Some new private APIs are implemented directly in the PMD without an
  abstraction layer. They can be used directly by some users who have the
  need.

  The new APIs to control VFs directly from PF include:

  * Set VF MAC anti-spoofing.
  * Set VF VLAN anti-spoofing.
  * Set TX loopback.
  * Set VF unicast promiscuous mode.
  * Set VF multicast promiscuous mode.
  * Set VF MTU.
  * Get/reset VF stats.
  * Set VF MAC address.
  * Set VF VLAN stripping.
  * Vf VLAN insertion.
  * Set VF broadcast mode.
  * Set VF VLAN tag.
  * Set VF VLAN filter.

  VFD also includes VF to PF mailbox message management from an application.
  When the PF receives mailbox messages from the VF the PF should call the
  callback provided by the application to know if they're permitted to be
  processed.

  As an EXPERIMENTAL feature, please be aware it can be changed or even
  removed without prior notice.

* **Updated the i40e base driver.**

  Updated the i40e base driver, including the following changes:

  * Replace existing legacy ``memcpy()`` calls with ``i40e_memcpy()`` calls.
  * Use ``BIT()`` macro instead of bit fields.
  * Add clear all WoL filters implementation.
  * Add broadcast promiscuous control per VLAN.
  * Remove unused ``X722_SUPPORT`` and ``I40E_NDIS_SUPPORT`` macros.

* **Updated the enic driver.**

  * Set new Rx checksum flags in mbufs to indicate unknown, good or bad checksums.
  * Fix set/remove of MAC addresses. Allow up to 64 addresses per device.
  * Enable TSO on outer headers.

* **Added Solarflare libefx-based network PMD.**

  Added a new network PMD which supports Solarflare SFN7xxx and SFN8xxx family
  of 10/40 Gbps adapters.

* **Updated the mlx4 driver.**

  * Addressed a few bugs.

* **Added support for Mellanox ConnectX-5 adapters (mlx5).**

  Added support for Mellanox ConnectX-5 family of 10/25/40/50/100 Gbps
  adapters to the existing mlx5 PMD.

* **Updated the mlx5 driver.**

  * Improve Tx performance by using vector logic.
  * Improve RSS balancing when number of queues is not a power of two.
  * Generic flow API support for Ethernet, IPv4, IPv4, UDP, TCP, VLAN and
    VXLAN pattern items with DROP and QUEUE actions.
  * Support for extended statistics.
  * Addressed several data path bugs.
  * As of MLNX_OFED 4.0-1.0.1.0, the Toeplitz RSS hash function is not
    symmetric anymore for consistency with other PMDs.

* **virtio-user with vhost-kernel as another exceptional path.**

  Previously, we upstreamed a virtual device, virtio-user with vhost-user as
  the backend as a way of enabling IPC (Inter-Process Communication) and user
  space container networking.

  Virtio-user with vhost-kernel as the backend is a solution for the exception
  path, such as KNI, which exchanges packets with the kernel networking stack.
  This solution is very promising in:

  * Maintenance: vhost and vhost-net (kernel) is an upstreamed and extensively
    used kernel module.
  * Features: vhost-net is designed to be a networking solution, which has
    lots of networking related features, like multi-queue, TSO, multi-seg
    mbuf, etc.
  * Performance: similar to KNI, this solution would use one or more
    kthreads to send/receive packets from user space DPDK applications,
    which has little impact on user space polling thread (except that
    it might enter into kernel space to wake up those kthreads if
    necessary).

* **Added virtio Rx interrupt support.**

  Added a feature to enable Rx interrupt mode for virtio pci net devices as
  bound to VFIO (noiommu mode) and driven by virtio PMD.

  With this feature, the virtio PMD can switch between polling mode and
  interrupt mode, to achieve best performance, and at the same time save
  power. It can work on both legacy and modern virtio devices. In this mode,
  each ``rxq`` is mapped with an excluded MSIx interrupt.

  See the :ref:`Virtio Interrupt Mode <virtio_interrupt_mode>` documentation
  for more information.

* **Added ARMv8 crypto PMD.**

  A new crypto PMD has been added, which provides combined mode cryptographic
  operations optimized for ARMv8 processors. The driver can be used to enhance
  performance in processing chained operations such as cipher + HMAC.

* **Updated the QAT PMD.**

  The QAT PMD has been updated with additional support for:

  * DES algorithm.
  * Scatter-gather list (SGL) support.

* **Updated the AESNI MB PMD.**

  * The Intel(R) Multi Buffer Crypto for IPsec library used in
    AESNI MB PMD has been moved to a new repository, in GitHub.
  * Support has been added for single operations (cipher only and
    authentication only).

* **Updated the AES-NI GCM PMD.**

  The AES-NI GCM PMD was migrated from the Multi Buffer library to the ISA-L
  library. The migration entailed adding additional support for:

  * GMAC algorithm.
  * 256-bit cipher key.
  * Session-less mode.
  * Out-of place processing
  * Scatter-gather support for chained mbufs (only out-of place and destination
    mbuf must be contiguous)

* **Added crypto performance test application.**

  Added a new performance test application for measuring performance
  parameters of PMDs available in the crypto tree.

* **Added Elastic Flow Distributor library (rte_efd).**

  Added a new library which uses perfect hashing to determine a target/value
  for a given incoming flow key.

  The library does not store the key itself for lookup operations, and
  therefore, lookup performance is not dependent on the key size. Also, the
  target/value can be any arbitrary value (8 bits by default). Finally, the
  storage requirement is much smaller than a hash-based flow table and
  therefore, it can better fit in CPU cache and scale to millions of flow
  keys.

  See the :ref:`Elastic Flow Distributor Library <Efd_Library>` documentation in
  the Programmers Guide document, for more information.


Resolved Issues
---------------

.. This section should contain bug fixes added to the relevant sections. Sample format:

   * **code/section Fixed issue in the past tense with a full stop.**

     Add a short 1-2 sentence description of the resolved issue in the past tense.
     The title should contain the code/lib section like a commit message.
     Add the entries in alphabetic order in the relevant sections below.

   This section is a comment. do not overwrite or remove it.
   Also, make sure to start the actual text at the margin.
   =========================================================

Drivers
~~~~~~~

* **net/virtio: Fixed multiple process support.**

  Fixed a few regressions introduced in recent releases that break the virtio
  multiple process support.


Examples
~~~~~~~~

* **examples/ethtool: Fixed crash with non-PCI devices.**

  Fixed issue where querying a non-PCI device was dereferencing non-existent
  PCI data resulting in a segmentation fault.



API Changes
-----------

.. This section should contain API changes. Sample format:

   * Add a short 1-2 sentence description of the API change. Use fixed width
     quotes for ``rte_function_names`` or ``rte_struct_names``. Use the past tense.

   This section is a comment. do not overwrite or remove it.
   Also, make sure to start the actual text at the margin.
   =========================================================

* **Moved five APIs for VF management from the ethdev to the ixgbe PMD.**

  The following five APIs for VF management from the PF have been removed from
  the ethdev, renamed, and added to the ixgbe PMD::

     rte_eth_dev_set_vf_rate_limit()
     rte_eth_dev_set_vf_rx()
     rte_eth_dev_set_vf_rxmode()
     rte_eth_dev_set_vf_tx()
     rte_eth_dev_set_vf_vlan_filter()

  The API's have been renamed to the following::

     rte_pmd_ixgbe_set_vf_rate_limit()
     rte_pmd_ixgbe_set_vf_rx()
     rte_pmd_ixgbe_set_vf_rxmode()
     rte_pmd_ixgbe_set_vf_tx()
     rte_pmd_ixgbe_set_vf_vlan_filter()

  The declarations for the API’s can be found in ``rte_pmd_ixgbe.h``.


ABI Changes
-----------

.. This section should contain ABI changes. Sample format:

   * Add a short 1-2 sentence description of the ABI change that was announced in
     the previous releases and made in this release. Use fixed width quotes for
     ``rte_function_names`` or ``rte_struct_names``. Use the past tense.

   This section is a comment. do not overwrite or remove it.
   Also, make sure to start the actual text at the margin.
   =========================================================



Shared Library Versions
-----------------------

.. Update any library version updated in this release and prepend with a ``+``
   sign, like this:

     librte_acl.so.2
   + librte_cfgfile.so.2
     librte_cmdline.so.2

   This section is a comment. do not overwrite or remove it.
   =========================================================


The libraries prepended with a plus sign were incremented in this version.

.. code-block:: diff

     librte_acl.so.2
     librte_cfgfile.so.2
     librte_cmdline.so.2
     librte_cryptodev.so.2
     librte_distributor.so.1
     librte_eal.so.3
   + librte_ethdev.so.6
     librte_hash.so.2
     librte_ip_frag.so.1
     librte_jobstats.so.1
     librte_kni.so.2
     librte_kvargs.so.1
     librte_lpm.so.2
     librte_mbuf.so.2
     librte_mempool.so.2
     librte_meter.so.1
     librte_net.so.1
     librte_pdump.so.1
     librte_pipeline.so.3
     librte_pmd_bond.so.1
     librte_pmd_ring.so.2
     librte_port.so.3
     librte_power.so.1
     librte_reorder.so.1
     librte_ring.so.1
     librte_sched.so.1
     librte_table.so.2
     librte_timer.so.1
     librte_vhost.so.3


Tested Platforms
----------------

.. This section should contain a list of platforms that were tested with this release.

   The format is:

   * <vendor> platform with <vendor> <type of devices> combinations

     * List of CPU
     * List of OS
     * List of devices
     * Other relevant details...

   This section is a comment. do not overwrite or remove it.
   Also, make sure to start the actual text at the margin.
   =========================================================

This release has been tested with the below list of CPU/device/firmware/OS.
Each section describes a different set of combinations.

* Intel(R) platforms with Mellanox(R) NICs combinations

   * Platform details

     * Intel(R) Xeon(R) CPU E5-2697 v2 @ 2.70GHz
     * Intel(R) Xeon(R) CPU E5-2680 v2 @ 2.80GHz
     * Intel(R) Xeon(R) CPU E5-2697 v3 @ 2.60GHz

   * OS:

     * CentOS 7.0
     * Fedora 23
     * Fedora 24
     * FreeBSD 10.3
     * Red Hat Enterprise Linux 7.2
     * SUSE Enterprise Linux 12
     * Ubuntu 14.04 LTS
     * Ubuntu 15.10
     * Ubuntu 16.04 LTS
     * Wind River Linux 8

   * MLNX_OFED: 4.0-1.0.1.0

   * NICs:

     * Mellanox(R) ConnectX(R)-3 Pro 40G MCX354A-FCC_Ax (2x40G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1007
       * Firmware version: 2.40.5030

     * Mellanox(R) ConnectX(R)-4 10G MCX4111A-XCAT (1x10G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 10G MCX4121A-XCAT (2x10G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 25G MCX4111A-ACAT (1x25G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 25G MCX4121A-ACAT (2x25G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 40G MCX4131A-BCAT/MCX413A-BCAT (1x40G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 40G MCX415A-BCAT (1x40G)

       * Host interface: PCI Express 3.0 x16
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 50G MCX4131A-GCAT/MCX413A-GCAT (1x50G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 50G MCX414A-BCAT (2x50G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 50G MCX415A-GCAT/MCX416A-BCAT/MCX416A-GCAT (2x50G)

       * Host interface: PCI Express 3.0 x16
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 50G MCX415A-CCAT (1x100G)

       * Host interface: PCI Express 3.0 x16
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 100G MCX416A-CCAT (2x100G)

       * Host interface: PCI Express 3.0 x16
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 Lx 10G MCX4121A-XCAT (2x10G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1015
       * Firmware version: 14.18.1000

     * Mellanox(R) ConnectX(R)-4 Lx 25G MCX4121A-ACAT (2x25G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1015
       * Firmware version: 14.18.1000

     * Mellanox(R) ConnectX(R)-5 100G MCX556A-ECAT (2x100G)

       * Host interface: PCI Express 3.0 x16
       * Device ID: 15b3:1017
       * Firmware version: 16.18.1000

     * Mellanox(R) ConnectX-5 Ex EN 100G MCX516A-CDAT (2x100G)

       * Host interface: PCI Express 4.0 x16
       * Device ID: 15b3:1019
       * Firmware version: 16.18.1000

* IBM(R) Power8(R) with Mellanox(R) NICs combinations

   * Machine:

     * Processor: POWER8E (raw), AltiVec supported

       * type-model: 8247-22L
       * Firmware FW810.21 (SV810_108)

   * OS: Ubuntu 16.04 LTS PPC le

   * MLNX_OFED: 4.0-1.0.1.0

   * NICs:

     * Mellanox(R) ConnectX(R)-4 10G MCX4111A-XCAT (1x10G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 10G MCX4121A-XCAT (2x10G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 25G MCX4111A-ACAT (1x25G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 25G MCX4121A-ACAT (2x25G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 40G MCX4131A-BCAT/MCX413A-BCAT (1x40G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 40G MCX415A-BCAT (1x40G)

       * Host interface: PCI Express 3.0 x16
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 50G MCX4131A-GCAT/MCX413A-GCAT (1x50G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 50G MCX414A-BCAT (2x50G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 50G MCX415A-GCAT/MCX416A-BCAT/MCX416A-GCAT (2x50G)

       * Host interface: PCI Express 3.0 x16
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 50G MCX415A-CCAT (1x100G)

       * Host interface: PCI Express 3.0 x16
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 100G MCX416A-CCAT (2x100G)

       * Host interface: PCI Express 3.0 x16
       * Device ID: 15b3:1013
       * Firmware version: 12.18.1000

     * Mellanox(R) ConnectX(R)-4 Lx 10G MCX4121A-XCAT (2x10G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1015
       * Firmware version: 14.18.1000

     * Mellanox(R) ConnectX(R)-4 Lx 25G MCX4121A-ACAT (2x25G)

       * Host interface: PCI Express 3.0 x8
       * Device ID: 15b3:1015
       * Firmware version: 14.18.1000

     * Mellanox(R) ConnectX(R)-5 100G MCX556A-ECAT (2x100G)

       * Host interface: PCI Express 3.0 x16
       * Device ID: 15b3:1017
       * Firmware version: 16.18.1000

* Intel(R) platforms with Intel(R) NICs combinations

   * Platform details

     * Intel(R) Atom(TM) CPU C2758 @ 2.40GHz
     * Intel(R) Xeon(R) CPU D-1540 @ 2.00GHz
     * Intel(R) Xeon(R) CPU E5-4667 v3 @ 2.00GHz
     * Intel(R) Xeon(R) CPU E5-2680 v2 @ 2.80GHz
     * Intel(R) Xeon(R) CPU E5-2699 v3 @ 2.30GHz
     * Intel(R) Xeon(R) CPU E5-2695 v4 @ 2.10GHz
     * Intel(R) Xeon(R) CPU E5-2658 v2 @ 2.40GHz

   * OS:

     * CentOS 7.2
     * Fedora 25
     * FreeBSD 11
     * Red Hat Enterprise Linux Server release 7.3
     * SUSE Enterprise Linux 12
     * Wind River Linux 8
     * Ubuntu 16.04
     * Ubuntu 16.10

   * NICs:

     * Intel(R) 82599ES 10 Gigabit Ethernet Controller

       * Firmware version: 0x61bf0001
       * Device id (pf/vf): 8086:10fb / 8086:10ed
       * Driver version: 4.0.1-k (ixgbe)

     * Intel(R) Corporation Ethernet Connection X552/X557-AT 10GBASE-T

       * Firmware version: 0x800001cf
       * Device id (pf/vf): 8086:15ad / 8086:15a8
       * Driver version: 4.2.5 (ixgbe)

     * Intel(R) Ethernet Converged Network Adapter X710-DA4 (4x10G)

       * Firmware version: 5.05
       * Device id (pf/vf): 8086:1572 / 8086:154c
       * Driver version: 1.5.23 (i40e)

     * Intel(R) Ethernet Converged Network Adapter X710-DA2 (2x10G)

       * Firmware version: 5.05
       * Device id (pf/vf): 8086:1572 / 8086:154c
       * Driver version: 1.5.23 (i40e)

     * Intel(R) Ethernet Converged Network Adapter XL710-QDA1 (1x40G)

       * Firmware version: 5.05
       * Device id (pf/vf): 8086:1584 / 8086:154c
       * Driver version: 1.5.23 (i40e)

     * Intel(R) Ethernet Converged Network Adapter XL710-QDA2 (2X40G)

       * Firmware version: 5.05
       * Device id (pf/vf): 8086:1583 / 8086:154c
       * Driver version: 1.5.23 (i40e)

     * Intel(R) Corporation I350 Gigabit Network Connection

       * Firmware version: 1.48, 0x800006e7
       * Device id (pf/vf): 8086:1521 / 8086:1520
       * Driver version: 5.2.13-k (igb)
