* Renesas SCI serial interface

Required properties:
- compatible: must be "renesas,scif", "renesas,scifa" or "renesas,sci"
- reg: exactly one register range with length
- clock: input clock frequency for the SCI unit
