#
# Xilinx ZYNQ U-Boot
#
# (C) Copyright 2013 Xilinx, Inc.
#
# SPDX-License-Identifier:	GPL-2.0+
#

1. About this

This document describes the information about Xilinx Zynq U-Boot -
like supported boards, ML status and TODO list.

2. Zynq boards

Xilinx Zynq-7000 All Programmable SoCs enable extensive system level
differentiation, integration, and flexibility through hardware, software,
and I/O programmability.

* zc702 (single qspi, gem0, mmc) [1]
* zc706 (dual parallel qspi, gem0, mmc) [2]
* zed (single qspi, gem0, mmc) [3]
* microzed (single qspi, gem0, mmc) [4]
* zc770
  - zc770-xm010 (single qspi, gem0, mmc)
  - zc770-xm011 (8 or 16 bit nand)
  - zc770-xm012 (nor)
  - zc770-xm013 (dual parallel qspi, gem1)

3. Building

 ex. configure and build for zc702 board
   $ make zynq_zc702_config
   $ make

4. Bootmode

Zynq has a facility to read the bootmode from the slcr bootmode register
once user is setting through jumpers on the board - see page no:1546 on [5]

All possible bootmode values are defined in Table 6-2:Boot_Mode MIO Pins
on [5].

board_late_init() will read the bootmode values using slcr bootmode register
at runtime and assign the modeboot variable to specific bootmode string which
is intern used in autoboot.

SLCR bootmode register Bit[3:0] values
#define ZYNQ_BM_NOR		0x02
#define ZYNQ_BM_SD		0x05
#define ZYNQ_BM_JTAG		0x0

"modeboot" variable can assign any of "norboot", "sdboot" or "jtagboot"
bootmode strings at runtime.

5. Mainline status

- Added basic board configurations support.
- Added zynq u-boot bsp code - arch/arm/cpu/armv7/zynq
- Added zynq boards named - zc70x, zed, microzed, zc770_xm010/xm011/xm012/xm013
- Added zynq drivers:
  serial - drivers/serial/serial_zynq.c
  net - drivers/net/zynq_gem.c
  mmc - drivers/mmc/zynq_sdhci.c
  spi - drivers/spi/zynq_spi.c
  qspi - drivers/spi/zynq_qspi.c
  i2c - drivers/i2c/zynq_i2c.c
  nand - drivers/mtd/nand/zynq_nand.c
- Done proper cleanups on board configurations
- Added basic FDT support for zynq boards
- d-cache support for zynq_gem.c

6. TODO

- Add FDT support on individual drivers

[1] http://www.xilinx.com/products/boards-and-kits/EK-Z7-ZC702-G.htm
[2] http://www.xilinx.com/products/boards-and-kits/EK-Z7-ZC706-G.htm
[3] http://zedboard.org/product/zedboard
[4] http://zedboard.org/product/microzed
[5] http://www.xilinx.com/support/documentation/user_guides/ug585-Zynq-7000-TRM.pdf

--
Jagannadha Sutradharudu Teki <jaganna@xilinx.com>
Sun Dec 15 14:52:41 IST 2013
