Overview
--------
The LS1046A Development System (QDS) is a high-performance computing,
evaluation, and development platform that supports the QorIQ LS1046A
LayerScape Architecture processor. The LS1046AQDS provides SW development
platform for the Freescale LS1046A processor series, with a complete
debugging environment.

LS1046A SoC Overview
--------------------
Please refer arch/arm/cpu/armv8/fsl-layerscape/doc/README.soc for LS1046A
SoC overview.

 LS1046AQDS board Overview
 -----------------------
 - SERDES Connections, 8 lanes supporting:
      - PCI Express - 3.0
      - SGMII, SGMII 2.5
      - QSGMII
      - SATA 3.0
      - XFI
 - DDR Controller
     - 8GB 64bits DDR4 SDRAM. Support rates of up to 2133MT/s
 -IFC/Local Bus
    - One in-socket 128 MB NOR flash 16-bit data bus
    - One 512 MB NAND flash with ECC support
    - PromJet Port
    - FPGA connection
 - USB 3.0
    - Three high speed USB 3.0 ports
    - First USB 3.0 port configured as Host with Type-A connector
    - The other two USB 3.0 ports configured as OTG with micro-AB connector
 - SDHC port connects directly to an adapter card slot, featuring:
    - Optional clock feedback paths, and optional high-speed voltage translation assistance
    - SD slots for SD, SDHC (1x, 4x, 8x), and/or MMC
    - eMMC memory devices
 - DSPI: Onboard support for three SPI flash memory devices
 - 4 I2C controllers
 - One SATA onboard connectors
 - UART
   - Two 4-pin serial ports at up to 115.2 Kbit/s
   - Two DB9 D-Type connectors supporting one Serial port each
 - ARM JTAG support

Memory map from core's view
----------------------------
Start Address    End Address     Description		Size
0x00_0000_0000 - 0x00_000F_FFFF  Secure Boot ROM	1MB
0x00_0100_0000 - 0x00_0FFF_FFFF  CCSRBAR		240MB
0x00_1000_0000 - 0x00_1000_FFFF  OCRAM0 		64KB
0x00_1001_0000 - 0x00_1001_FFFF  OCRAM1 		64KB
0x00_2000_0000 - 0x00_20FF_FFFF  DCSR			16MB
0x00_6000_0000 - 0x00_67FF_FFFF  IFC - NOR Flash	128MB
0x00_7E80_0000 - 0x00_7E80_FFFF  IFC - NAND Flash	64KB
0x00_7FB0_0000 - 0x00_7FB0_0FFF  IFC - FPGA		4KB
0x00_8000_0000 - 0x00_FFFF_FFFF  DRAM1			2GB
0x05_0000_0000 - 0x05_07FF_FFFF  QMAN S/W Portal	128M
0x05_0800_0000 - 0x05_0FFF_FFFF  BMAN S/W Portal	128M
0x08_8000_0000 - 0x09_FFFF_FFFF  DRAM2			6GB
0x40_0000_0000 - 0x47_FFFF_FFFF  PCI Express1		32G
0x48_0000_0000 - 0x4F_FFFF_FFFF  PCI Express2		32G
0x50_0000_0000 - 0x57_FFFF_FFFF  PCI Express3		32G

Booting Options
---------------
a) Promjet Boot
b) NOR boot
c) NAND boot
d) SD boot
e) QSPI boot
