TPS65090 Frontend PMU with Switchmode Charger

Required Properties:
-compatible: "ti,tps65090-charger"

Optional Properties:
-ti,enable-low-current-chrg: Enables charging when a low current is detected
 while the default logic is to stop charging.

This node is a subnode of the tps65090 PMIC.

Example:

	tps65090-charger {
		compatible = "ti,tps65090-charger";
		ti,enable-low-current-chrg;
	};
