U-Boot for Freescale i.MX25

This file contains information for the port of U-Boot to the Freescale i.MX25
SoC.

1. CONVENTIONS FOR FUSE ASSIGNMENTS
-----------------------------------

1.1 MAC Address: It is stored in the words 26 to 31 of fuse bank 0, using the
    natural MAC byte order (i.e. MSB first).
