Qualcomm pm8916 PMIC

This PMIC is connected using SPMI bus so should be child of SPMI bus controller.

Required properties:
- compatible: "qcom,spmi-pmic";
- reg: SPMI Slave ID, size (ignored)
- #address-cells: 0x1 (peripheral ID)
- #size-cells: 0x1 (size of peripheral register space)

Example:

pm8916@0 {
	compatible = "qcom,spmi-pmic";
	reg = <0x0 0x1>;
	#address-cells = <0x1>;
	#size-cells = <0x1>;
};
