JFFS2 NAND support:

To enable, use the following #define in the board configuration file:

#define CONFIG_JFFS2_NAND

Configuration of partitions is similar to how this is done in  U-Boot
for  JFFS2  on top NOR flash.
