/*
 * (C) Copyright 2008-2009
 * BuS Elektronik GmbH & Co. KG <www.bus-elektronik.de>
 * Jens Scharsig <esw@bus-elektronik.de>
 *
 * SPDX-License-Identifier:	GPL-2.0+
 */

U-Boot vcxk video controller driver
======================================

By defining CONFIG_VIDEO_VCXK this driver can be used with VC2K, VC4K and
VC8K devices on following boards:

board           | ARCH          | Vendor
-----------------------------------------------------------------------
EB+CPU5282-T1   | MCF5282       | BuS Elektronik GmbH & Co. KG
EB+MCF-EVB123   | MCF5282       | BuS Elektronik GmbH & Co. KG
EB+CPUx9K2      | AT91RM9200    | BuS Elektronik GmbH & Co. KG
ZLSA            | AT91RM9200    | Ruf Telematik AG

Driver configuration
--------------------

The driver needs some defines to describe the target hardware:

CONFIG_SYS_VCXK_BASE

	base address of VCxK hardware memory

CONFIG_SYS_VCXK_DEFAULT_LINEALIGN

	defines the physical alignment of a pixel row

CONFIG_SYS_VCXK_DOUBLEBUFFERED

	some boards that use vcxk prevent read from framebuffer memory.
	define this option to enable double buffering (needs 16KiB RAM)

CONFIG_SYS_VCXK_<xxxx>_PIN

	defines the number of the I/O line PIN in the port
	valid values for <xxxx> are:

		ACKNOWLEDGE
			describes the acknowledge line from vcxk hardware

		ENABLE
			describes the enable line to vcxk hardware

		INVERT
			describes the invert line to vcxk hardware

		RESET
			describes the reset line to vcxk hardware

		REQUEST
			describes the request line to vcxk hardware

CONFIG_SYS_VCXK_<xxxx>_PORT

	defines the I/O port which is connected with the line
	for valid values for <xxxx> see CONFIG_SYS_VCXK_<xxxx>_PIN

CONFIG_SYS_VCXK_<xxxx>_DDR

	defines the register which configures the direction
	for valid values for <xxxx> see CONFIG_SYS_VCXK_<xxxx>_PIN
