How to use U-Boot on Engicam i.CoreM6 RQS Solo/DualLite and Quad/Dual Starter Kit:
----------------------------------------------------------------------------------

$ make mrproper

- Configure U-Boot for Engicam i.CoreM6 RQS Quad/Dual:
$ make imx6q_icore_rqs_mmc_defconfig

- Configure U-Boot for Engicam i.CoreM6 RQS Solo/DualLite:
$ make imx6dl_icore_rqs_mmc_defconfig

- Build U-Boot
$ make

This will generate the SPL image called SPL and the u-boot-dtb.img.

- Flash the SPL image into the micro SD card:

sudo dd if=SPL of=/dev/mmcblk0 bs=1k seek=1; sync

- Flash the u-boot-dtb.img image into the micro SD card:

sudo dd if=u-boot-dtb.img of=/dev/mmcblk0 bs=1k seek=69; sync

- Jumper settings:

MMC Boot: JM3 Closed

- Connect the Serial cable between the Starter Kit and the PC for the console.
(J28 is the Linux Serial console connector)

- Insert the micro SD card in the board, power it up and U-Boot messages should
come up.
