How to use U-Boot on Solid-run mx6 Hummingboard and Cubox-i
-----------------------------------------------------------

- Build U-Boot for Hummingboard/Cubox-i:

$ make mrproper
$ make mx6cuboxi_defconfig
$ make

This will generate the SPL image called SPL and the u-boot.img.

- Flash the SPL image into the SD card:

sudo dd if=SPL of=/dev/mmcblk0 bs=1k seek=1; sync

- Flash the u-boot.img image into the SD card:

sudo dd if=u-boot.img of=/dev/mmcblk0 bs=1k seek=69; sync

- Insert the SD card in the board, power it up and U-Boot messages should
come up.
