(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "IR908-7C-F" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (at 1.778 3.048 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "IR908-7C-F" (at -1.016 -2.794 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "lalboard:IR908-7C-F" (at 0 4.445 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.everlight.com/file/ProductFile/201407052136280483.pdf" (at -1.27 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IR LED" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "940nm Sidelooker IR LED" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "LED*SideEmitter*Rectangular*W4.5mm*H1.6mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "IR908-7C-F_0_1"
      (polyline
        (pts
          (xy -2.54 0)
          (xy 0 0)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 1.27)
          (xy -2.54 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.381 3.175)
          (xy -0.127 3.175)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.143 1.651)
          (xy 0.381 3.175)
          (xy 0.381 2.667)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -1.27)
          (xy 0 1.27)
          (xy -2.54 0)
          (xy 0 -1.27)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.413 1.651)
          (xy -0.889 3.175)
          (xy -0.889 2.667)
          (xy -0.889 3.175)
          (xy -1.397 3.175)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
    )
    (symbol "IR908-7C-F_1_1"
      (pin passive line (at -5.08 0 0) (length 2.54)
        (name "K" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 0 180) (length 2.54)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "PT908-7B-F" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "Q" (at 5.08 1.27 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "PT908-7B-F" (at 5.08 -1.27 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "lalboard:PT908-7C-F" (at 2.54 12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.everlight.com/file/ProductFile/PT908-7B-F.pdf" (at 6.35 16.51 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "npn phototransistor" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "940nm Sidelooker Phototransistor" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "PT908-7B-F_0_1"
      (polyline
        (pts
          (xy -1.905 1.27)
          (xy -2.54 1.27)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 2.54)
          (xy -1.905 2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.635 0.635)
          (xy 2.54 2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -3.81 3.175)
          (xy -1.905 1.27)
          (xy -1.905 1.905)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -3.175 4.445)
          (xy -1.27 2.54)
          (xy -1.27 3.175)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.635 -0.635)
          (xy 2.54 -2.54)
          (xy 2.54 -2.54)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.635 1.905)
          (xy 0.635 -1.905)
          (xy 0.635 -1.905)
        )
        (stroke (width 0.508) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 -1.778)
          (xy 1.778 -1.27)
          (xy 2.286 -2.286)
          (xy 1.27 -1.778)
          (xy 1.27 -1.778)
        )
        (stroke (width 0) (type default))
        (fill (type outline))
      )
      (circle (center 1.27 0) (radius 2.8194)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
    )
    (symbol "PT908-7B-F_1_1"
      (pin passive line (at 2.54 -5.08 90) (length 2.54)
        (name "E" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.54 5.08 270) (length 2.54)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "RP2040" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -29.21 49.53 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "RP2040" (at 24.13 -49.53 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "RP2040_minimal:RP2040-QFN-56" (at -19.05 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -19.05 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "RP2040_0_0"
      (text "Raspberry Pi" (at 0 5.08 0)
        (effects (font (size 2.54 2.54)))
      )
      (text "RP2040" (at 0 0 0)
        (effects (font (size 2.54 2.54)))
      )
    )
    (symbol "RP2040_0_1"
      (rectangle (start 29.21 48.26) (end -29.21 -48.26)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "RP2040_1_1"
      (pin power_in line (at 8.89 50.8 270) (length 2.54)
        (name "IOVDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 6.35 50.8 270) (length 2.54)
        (name "IOVDD" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 12.7 180) (length 2.54)
        (name "GPIO8" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 10.16 180) (length 2.54)
        (name "GPIO9" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 7.62 180) (length 2.54)
        (name "GPIO10" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 5.08 180) (length 2.54)
        (name "GPIO11" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 2.54 180) (length 2.54)
        (name "GPIO12" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 0 180) (length 2.54)
        (name "GPIO13" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -2.54 180) (length 2.54)
        (name "GPIO14" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -5.08 180) (length 2.54)
        (name "GPIO15" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 -50.8 90) (length 2.54)
        (name "TESTEN" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 33.02 180) (length 2.54)
        (name "GPIO0" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -31.75 -2.54 0) (length 2.54)
        (name "XIN" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -31.75 -7.62 0) (length 2.54)
        (name "XOUT" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 3.81 50.8 270) (length 2.54)
        (name "IOVDD" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -17.78 50.8 270) (length 2.54)
        (name "DVDD" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -31.75 -31.75 0) (length 2.54)
        (name "SWCLK" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 -34.29 0) (length 2.54)
        (name "SWD" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -31.75 -20.32 0) (length 2.54)
        (name "RUN" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -7.62 180) (length 2.54)
        (name "GPIO16" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -10.16 180) (length 2.54)
        (name "GPIO17" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -12.7 180) (length 2.54)
        (name "GPIO18" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 30.48 180) (length 2.54)
        (name "GPIO1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -15.24 180) (length 2.54)
        (name "GPIO19" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -17.78 180) (length 2.54)
        (name "GPIO20" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -20.32 180) (length 2.54)
        (name "GPIO21" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 1.27 50.8 270) (length 2.54)
        (name "IOVDD" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -22.86 180) (length 2.54)
        (name "GPIO22" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -25.4 180) (length 2.54)
        (name "GPIO23" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -27.94 180) (length 2.54)
        (name "GPIO24" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -30.48 180) (length 2.54)
        (name "GPIO25" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -35.56 180) (length 2.54)
        (name "GPIO26_ADC0" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -38.1 180) (length 2.54)
        (name "GPIO27_ADC1" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 27.94 180) (length 2.54)
        (name "GPIO2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -40.64 180) (length 2.54)
        (name "GPIO28_ADC2" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 -43.18 180) (length 2.54)
        (name "GPIO29_ADC3" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -1.27 50.8 270) (length 2.54)
        (name "IOVDD" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.51 50.8 270) (length 2.54)
        (name "ADC_AVDD" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 50.8 270) (length 2.54)
        (name "VREG_IN" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 50.8 270) (length 2.54)
        (name "VREG_VOUT" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 40.64 180) (length 2.54)
        (name "USB_DM" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 43.18 180) (length 2.54)
        (name "USB_DP" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.7 50.8 270) (length 2.54)
        (name "USB_VDD" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -3.81 50.8 270) (length 2.54)
        (name "IOVDD" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 25.4 180) (length 2.54)
        (name "GPIO3" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -20.32 50.8 270) (length 2.54)
        (name "DVDD" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 20.32 0) (length 2.54)
        (name "QSPI_SD3" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -31.75 16.51 0) (length 2.54)
        (name "QSPI_SCLK" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 27.94 0) (length 2.54)
        (name "QSPI_SD0" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 22.86 0) (length 2.54)
        (name "QSPI_SD2" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 25.4 0) (length 2.54)
        (name "QSPI_SD1" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -31.75 31.75 0) (length 2.54)
        (name "QSPI_SS" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -50.8 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 22.86 180) (length 2.54)
        (name "GPIO4" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 20.32 180) (length 2.54)
        (name "GPIO5" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 17.78 180) (length 2.54)
        (name "GPIO6" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 31.75 15.24 180) (length 2.54)
        (name "GPIO7" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TS-1187A-B-A-B" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "S" (at -2.54 2.54 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "TS-1187A-B-A-B" (at -2.54 -2.54 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "TS-1187A-B-A-B:SW_TS-1187A-B-A-B" (at 0 7.62 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "MF" "XKB Industrial Precision" (at 1.27 20.32 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.5mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "Package" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "None" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/TS-1187A-B-A-B/XKB+Industrial+Precision/view-part/?ref=eda" (at 1.27 2.54 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (at 0 22.86 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "A0" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/TS-1187A-B-A-B/XKB+Industrial+Precision/view-part/?ref=snap" (at 1.27 5.08 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "TS-1187A-B-A-B" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\nTS-1187A-B-A-B XKB Connectivity\n" (at -1.27 12.7 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "Not in stock" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "XKB Industrial Precision" (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "TS-1187A-B-A-B_0_0"
      (polyline
        (pts
          (xy -2.54 0)
          (xy -5.08 0)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 0)
          (xy 2.794 2.1336)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 0)
          (xy 2.921 0)
        )
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (circle (center 2.54 0) (radius 0.3302)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
      (pin passive line (at -7.62 0 0) (length 2.54)
        (name "~" (effects (font (size 1.016 1.016))))
        (number "A" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -7.62 0 0) (length 2.54)
        (name "~" (effects (font (size 1.016 1.016))))
        (number "B" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.016 1.016))))
        (number "C" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.016 1.016))))
        (number "D" (effects (font (size 1.016 1.016))))
      )
    )
  )
)
