com.qualcomm.robotcore.eventloop.opmode

## Annotation Type Autonomous

-     @Documented
       @Target(value=TYPE)
       @Retention(value=RUNTIME)
      public @interface Autonomous

  Provides an easy and non-centralized way of determining the OpMode list shown on an FTC Driver Station. Put an `Autonomous` annotation on your autonomous OpModes that you want to show up in the driver station display. If you want to temporarily disable an opmode, then set then also add a `Disabled` annotation to it.
  See Also:
    `TeleOp`, `Disabled`, `OpModeRegistrar`

- - ### Optional Element Summary

    Optional Elements
    Modifier and Type | Optional Element and Description
    --- | ---
    `java.lang.String` | `group` Optionally indicates a group of other OpModes with which the annotated OpMode should be sorted on the driver station OpMode list.
    `java.lang.String` | `name` The name to be used on the driver station display.

- - ### Element Detail

    - #### name

          public abstract java.lang.String name

      The name to be used on the driver station display. If empty, the name of the OpMode class will be used.
      Returns:
        the name to use for the OpMode in the driver station.
      Default:
        ""

  - - #### group

          public abstract java.lang.String group

      Optionally indicates a group of other OpModes with which the annotated OpMode should be sorted on the driver station OpMode list.
      Returns:
        the group into which the annotated OpMode is to be categorized
      Default:
        ""