Chipidea EHCI controller (part of OTG controller) used on Qualcomm devices.

Required properties:
- compatible: must be "qcom,ehci-host"
- reg: start address and size of the registers

ehci@78d9000 {
	compatible = "qcom,ehci-host";
	reg = <0x78d9000 0x400>;
};
